A B C D E F G H I K L M N O P Q R S T V W _

## S

SelectMask6cParam - Class in com.unitech.lib.uhf.params
  The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
SelectMask6cParam() - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, String, int) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, <any>) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
Session - Enum in com.unitech.lib.uhf.types
  The Session enumeration represents the session of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAction(ActionState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operational state of the device associated with the instance.
setAction(Mask6cAction) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
setAddress(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the address of the device to which the instance of BaseReader is connected.
setAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the address of the device to which the BaseTransport instance is connected.
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
setAutoOffTime(int) - Method in class com.unitech.lib.htx.HT730Reader
setAutoOffTime(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time which the equipment automatically turns off.
setAutoOffTime(int) - Method in class com.unitech.lib.rpx.RP902Reader
setBank(BankType) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Bank value in "Selection Mask".
setBeeper(BeeperState) - Method in class com.unitech.lib.htx.HT730Reader
setBeeper(BeeperState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the beeper operation status of the equipment.
setBeeper(BeeperState) - Method in class com.unitech.lib.rpx.RP902Reader
setBLF(BLFType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
setCheckInterval(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time period for checking the battery status of the device associated with the BaseReader class instance.
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets whether or not the RFID UHF module of the device will run the Inventory continuously.
setDeviceName(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the name of the device to which the instance of BaseReader is connected.
setDeviceName(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the name of the device to which the BaseTransport instance is connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.reader.BaseReader
  Sets the type of device to which instance of BaseReader will be connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the type of device to which the instance will be connected.
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
setFindDevice(FindDevice) - Method in class com.unitech.lib.htx.HT730Reader
setFindDevice(FindDevice) - Method in class com.unitech.lib.reader.BaseReader
  Sets the find device status of the equipment.
setFindDevice(FindDevice) - Method in class com.unitech.lib.rpx.RP902Reader
setGlobalBand(GlobalBandType) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the national orientation of the RFID UHF module of the instrument.
setIdleTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument sets the time for which the radio waves are not output in the Inventory operation and the rest of the time.
setInventoryTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the time at which radio waves are actually output in Inventory operation of the RFID UHF module of the instrument.
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setLastError(ResultCode) - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
setLength(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Length of the EPCMaskParam instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the pattern length of the Mask6cPattern instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Length value of "Selection Mask".
setMacAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the MAC address of the device to which the BaseTransport instance is connected.
setMax(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the maximum Power Gian Level value for a PowerRange instance.
setMaxQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the maximum Q value.
setMin(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the Power Gian Level minimum value for a PowerRange instance.
setMinQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the minimum Q value.
setMode(FindDeviceMode) - Method in class com.unitech.lib.reader.params.FindDevice
  Set FindDeviceMode.
setModuleProfile(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
setOffset(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the offset of the EPCMaskParam instance.
setOffset(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Offset value of "Selection Mask".
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.htx.HT730Reader
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operating mode status of the equipment.
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.rpx.RP902Reader
setPattern(String) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Pattern for the EPCMaskParam instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the Mask pattern for the instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Pattern value of "Selection Mask".
setPower(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the antenna output of the RFID UHF module of the instrument.
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the power mode the RFID UHF module of the appliance uses to perform the inventory.
setReadMode(ReadMode) - Method in class com.unitech.lib.htx.HT730Reader
setReadMode(ReadMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the read mode status of the equipment.
setReadMode(ReadMode) - Method in class com.unitech.lib.rpx.RP902Reader
setSelectMask6c(int, SelectMask6cParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison behavior of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the memory bank to be compared.
setSelectMask6cEnabled(int, boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set whether or not to use the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the start address of the memory to start the comparison.
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison value and length of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Flag of the tag to save the comparison result of Selection Mask item of the RFID UHF module of the device.
setSession(Session) - Method in class com.unitech.lib.uhf.BaseUHF
  Device's RFID UHF module sets the Session to check the status of the Session of the tag to be read by Inventory operation.
setStartQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, set the starting Q value.
setState(ConnectState, Object) - Method in class com.unitech.lib.transport.BaseTransport
setStateListener(IConnectStateEventListener) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the listener to receive the connection status of an instance of the BaseTransport class.
setTarget(Target) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the state of target of tag to read by Inventory operation.
setTarget(Mask6cTarget) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Target Flag of "Selection Mask".
setTARI(TARIType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'TID memory'.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'TID memory'.
setTime(Date) - Method in class com.unitech.lib.htx.HT730Reader
setTime(Date) - Method in class com.unitech.lib.reader.BaseReader
  Sets the system time of the instrument.
setTime(Date) - Method in class com.unitech.lib.rpx.RP902Reader
setTimeout(int) - Method in class com.unitech.lib.reader.params.FindDevice
  Set timeout.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
setUsed(boolean) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set whether or not to use "Selection Mask".
setUser(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setUser(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setVibrator(VibratorState) - Method in class com.unitech.lib.htx.HT730Reader
setVibrator(VibratorState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the vibrator operation status of the equipment.
setVibrator(VibratorState) - Method in class com.unitech.lib.rpx.RP902Reader
SKUType - Enum in com.unitech.lib.types
  The SKUType enumeration represents the type of device associated with the SDK.
StateChangedEventArgs(BaseReader, ConnectState, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.StateChangedEventArgs
stop() - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to stop the operation being performed.

A B C D E F G H I K L M N O P Q R S T V W _