A B C D E F G H I K L M N O P Q R S T V W _

## L

listen() - Method in class com.unitech.lib.reader.BaseReader
  Allows the BaseReader class to wait for connection until the connection is made from the device.
listen() - Method in class com.unitech.lib.transport.BaseTransport
  An instance of the BaseTransport class waits for the device to connect.
listen() - Method in class com.unitech.lib.transport.TransportBluetooth
lock6c(Lock6cParam, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to lock or unlock the RFID UHF tags of the ISO18000-6c Gen2 standard.
Lock6cParam - Class in com.unitech.lib.uhf.params
  The Lock6cParam class is used to pass information that the RFID UHF's Lock command performs.
Lock6cParam() - Constructor for class com.unitech.lib.uhf.params.Lock6cParam
  Creates an instance of the Lock6cParam class.
Lock6cParam(LockState, LockState, LockState, LockState, LockState) - Constructor for class com.unitech.lib.uhf.params.Lock6cParam
  Creates an instance of the Lock6cParam class.
LockState - Enum in com.unitech.lib.uhf.types
  The LockState enumeration represents the lock state.

A B C D E F G H I K L M N O P Q R S T V W _