A B C D E F G H I K L M N O P Q R S T V W _

## I

idleTime - Variable in class com.unitech.lib.reader.params.DutyCycle
IEnumType - Interface in com.unitech.lib.types
  The IEnumType interface provides the common functionality of all enumerations that the SDK uses.
IModuleRfidUhfEventListener - Interface in com.unitech.lib.uhf.event
INFO - Static variable in class com.unitech.lib.transport.BaseTransport
initModule() - Method in class com.unitech.lib.uhf.BaseUHF
  After the Device is connected, it calls to instantiate the BaseUHF instance.
initReader() - Method in class com.unitech.lib.htx.HT730Reader
initReader() - Method in class com.unitech.lib.reader.BaseReader
  Initializes an BaseReader instance after the BaseReader instance is associated with the device.
initReader() - Method in class com.unitech.lib.rpx.RP902Reader
inventory6c() - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to inventory the RFID UHF tag of ISO18000-6c Gen2 standard.
inventoryTime - Variable in class com.unitech.lib.reader.params.DutyCycle
IO - Static variable in class com.unitech.lib.transport.BaseTransport
IReaderEventListener - Interface in com.unitech.lib.reader.event
IRfidUhfEventListener - Interface in com.unitech.lib.uhf.event
  The IRfidUhfEventListener interface is an interface that defines event handling methods for handling events raised by the BaseUHF instance.
isUsed() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns whether or not "Selection Mask" is enabled.

A B C D E F G H I K L M N O P Q R S T V W _