A B C D E F G H I K L M N O P Q R S T U V W X _

## T

T4Min - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
T4Min - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_Timings.Fields
TAG - Variable in class com.unitech.lib.reader.BaseReader
TAG - Variable in class com.unitech.lib.reader.device.BaseDevice
TAG - Variable in class com.unitech.lib.reader.protocol.Protocol
TAG - Variable in class com.unitech.lib.transport.BaseTransport
TAG - Variable in class com.unitech.lib.uhf.BaseUHF
TAG - Variable in class com.unitech.lib.uhf.module.BaseModuleUHF
TagAccessResult - Class in com.unitech.lib.uhf.params
  The TagAccessResult class is used to pass the tag access result information.
TagAccessResult(byte[], byte[], ResultCode, ActionType, BankType) - Constructor for class com.unitech.lib.uhf.params.TagAccessResult
tagCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: ADC value.
TagExtParam - Class in com.unitech.lib.uhf.params
  The TagExtParam class is used to pass the tag information.
TagExtParam(int) - Constructor for class com.unitech.lib.uhf.params.TagExtParam
TagExtParam(int, int) - Constructor for class com.unitech.lib.uhf.params.TagExtParam
TagExtParam(byte[], byte[], byte[], short, long, int, short) - Constructor for class com.unitech.lib.uhf.params.TagExtParam
tagList - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
tagList - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
tagListSizeMax - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
tagListSizeMax - Variable in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
tagReply - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
  < I Param: RFU.
tagReply - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
  < I Param: Data to be written.
tagReply - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
  < I Param: Data to be written.
tagReply - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
  < I Param: RFU.
tagReply - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
  < I Param: Password.
tagReply - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Write
  < I Param: Data to be written.
tagReply - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Kill.Fields
tagReply - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Write.Fields
tagReply - Variable in class com.unitech.stuhflBridge.BR_Gen2_BlockWrite.Fields
tagReply - Variable in class com.unitech.stuhflBridge.BR_Gen2_Kill.Fields
tagReply - Variable in class com.unitech.stuhflBridge.BR_Gen2_Lock.Fields
tagReply - Variable in class com.unitech.stuhflBridge.BR_Gen2_Write.Fields
target - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Target setting
Target - Enum in com.unitech.lib.uhf.types
  The Target enumeration type indicates the status of the Target of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
target - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: Select mode to be applied (CLEAR_LIST, ADD2LIST, CLEAR_AND_ADD).
target - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Select mode to be applied (CLEAR_LIST, ADD2LIST, CLEAR_AND_ADD).
target - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams
  < I/O Param: STUHFL_D_GB29768_SESSION_S0, ...
target - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams
  < I/O Param: STUHFL_D_GEN2_SESSION_S0, ...
target - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
target - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
targetDepletionMode - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams
  < I/O Param: Target A/B toggle
targetDepletionMode - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams
  < I/O Param: Toggle between Target A and B
tari - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
tari - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_ProtocolCfg.Fields
tariType - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The TARI setting, only for RP902
TARIType - Enum in com.unitech.lib.uhf.types
  The TARIType enumeration represents the TARI by which the RFID UHF module inventories the TAG.
tc - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
  < I/O Param: Coding: STUHFL_D_GB29768_CODING_FM0, STUHFL_D_GB29768_CODING_MILLER2, ...
tc - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_ProtocolCfg.Fields
temperature - Variable in class com.unitech.stuhfl.STUHFL_T_Temperature
TemperatureStateEventArgs(BaseReader, double, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.TemperatureStateEventArgs
tid() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's TID value.
tid - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Tag EPC.
time - Variable in class com.unitech.stuhfl.STUHFL_T_Time
  < O Param: human readable time information
timeout - Variable in class com.unitech.stuhfl.STUHFL_T_FindDevice
timeout - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
  < I Param: Antenna Power mode
timeout - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_AntennaPower.Fields
timestamp - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
timestamp - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
toAscii(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toBoolean(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toByte(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toByte(String, int) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toBytes(String) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toBytes(int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toBytes(long) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toBytes(boolean) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toBytes(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toBytes(String, int) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toggleTarget - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The toggle target setting
toggleTarget - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams
  < I/O Param: For QUERY Target field
toggleTarget - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams
  < I/O Param: For QUERY Target field
toHex(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.ANTENNA_POWER_MODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.CONTINUOUS_MODULATION_MODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.FREQUENCY_HOP_MODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_ACTION_ATTRIBUTE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_ACTION_SECMODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_AREA
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_BLF
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_CODING
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_CONDITION
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_CONFIGURATION
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_RULE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_SESSION
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_SORT_MODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_SORT_TARGET
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_TARGET
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GB29768_TC
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_BLF
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_CODING
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_GENERIC_CMD
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_MEMORY_BANK
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_SELECT_MODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_SELECT_TARGET
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_SESSION
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_TARGET
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.GEN2_TARI
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.HW_ID
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.POWER
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.PROFILE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.REPORT_OPTION
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.RET_CODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.RSSI_MODE
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.RWD_CFG_ID
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.TREXT_LEAD
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.TUNER_CAP
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.TUNING_ALGO
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.TUNING_STATUS
toInt() - Method in enum com.unitech.stuhfl.STUHFL_E.USED_ANTENNA
toInteger(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toInteger(byte[], int, int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toInteger(byte[], int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toInteger(byte[], int, int, int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toInteger(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toInteger(String, int) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toLong(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toLong(byte[], int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toMask() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns an array for mask
toMask() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns an array for mask
toRawString(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toRawString(byte[], int, int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toShort(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toShort(byte[], int, int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toShort(byte[], int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toShort(byte[], int, int, int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toShort(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toShort(String, int) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
toString() - Method in class com.unitech.lib.protocol.Response
toString() - Method in class com.unitech.lib.reader.BaseReader
toString() - Method in class com.unitech.lib.reader.event.ReaderEventManager.ActionChangedEventArgs
toString() - Method in class com.unitech.lib.reader.event.ReaderEventManager.BatteryStateEventArgs
toString() - Method in class com.unitech.lib.reader.event.ReaderEventManager.StateChangedEventArgs
toString() - Method in class com.unitech.lib.reader.event.ReaderEventManager.TemperatureStateEventArgs
toString() - Method in class com.unitech.lib.reader.params.DataRange
toString() - Method in class com.unitech.lib.reader.params.DutyCycle
toString() - Method in class com.unitech.lib.reader.params.FindDevice
toString() - Method in class com.unitech.lib.reader.params.KeyEventItem
toString() - Method in enum com.unitech.lib.reader.types.BeeperState
toString() - Method in enum com.unitech.lib.reader.types.KeyState
toString() - Method in enum com.unitech.lib.reader.types.KeyType
toString() - Method in enum com.unitech.lib.reader.types.NotificationState
toString() - Method in enum com.unitech.lib.reader.types.VibratorState
toString() - Method in enum com.unitech.lib.rpx.types.CommandType
toString() - Method in enum com.unitech.lib.rpx.types.DeviceOptionType
toString() - Method in enum com.unitech.lib.rpx.types.SubCommandType
toString() - Method in class com.unitech.lib.transport.BaseTransport
toString() - Method in enum com.unitech.lib.transport.types.ConnectState
toString() - Method in enum com.unitech.lib.transport.types.ConnectType
toString() - Method in enum com.unitech.lib.types.ActionState
toString() - Method in enum com.unitech.lib.types.ActionType
toString() - Method in enum com.unitech.lib.types.DataFormat
toString() - Method in enum com.unitech.lib.types.DataInfo
toString() - Method in enum com.unitech.lib.types.DataTerminator
toString() - Method in enum com.unitech.lib.types.DeviceType
toString() - Method in enum com.unitech.lib.types.FindDeviceMode
toString() - Method in interface com.unitech.lib.types.IEnumType
  Return the name of the enum
toString() - Method in enum com.unitech.lib.types.ModuleUHFType
toString() - Method in enum com.unitech.lib.types.OperatingMode
toString() - Method in enum com.unitech.lib.types.ReadMode
toString() - Method in enum com.unitech.lib.types.ResultCode
toString() - Method in enum com.unitech.lib.types.SKUType
toString() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Return the EPCMaskParam information with format: [Kill Password], [Access Password], [EPC], [Bank], [TID], [User]
toString() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Return the Lock6cParam information with format: [Kill Password], [Access Password], [EPC], [Bank], [TID], [User]
toString() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Return the Mask6cPattern information with format: [Pattern], [Length]
toString() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Return the PermaLock6cParam information with format: [Kill Password], [Access Password], [EPC], [Bank], [TID], [User]
toString() - Method in class com.unitech.lib.uhf.params.PowerRange
  Return the PowerRange information with format: [Min], [Max]
toString() - Method in class com.unitech.lib.uhf.params.RFIDConfig
toString() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Return the SelectMask6cParam information with format: [Used], [Target], [Action], [Bank], [Offset], [Pattern], [Length]
toString() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Return the TagAccessResult information with format: [Result Code], [Action Type], [EPC], [Data], [Bank]
toString() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's RSSI and frequency
toString() - Method in enum com.unitech.lib.uhf.types.AlgorithmType
toString() - Method in enum com.unitech.lib.uhf.types.BankType
toString() - Method in enum com.unitech.lib.uhf.types.BLFType
toString() - Method in enum com.unitech.lib.uhf.types.Encoding
toString() - Method in enum com.unitech.lib.uhf.types.GlobalBandType
toString() - Method in enum com.unitech.lib.uhf.types.LockState
toString() - Method in enum com.unitech.lib.uhf.types.Mask6cAction
toString(Mask6cTarget) - Method in enum com.unitech.lib.uhf.types.Mask6cAction
toString() - Method in enum com.unitech.lib.uhf.types.Mask6cTarget
toString() - Method in enum com.unitech.lib.uhf.types.PowerMode
toString() - Method in enum com.unitech.lib.uhf.types.Session
toString() - Method in enum com.unitech.lib.uhf.types.Target
toString() - Method in enum com.unitech.lib.uhf.types.TARIType
toString(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toString(byte[], int, int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
toString() - Method in class com.unitech.stuhfl.STUHFL_T_AutoOffTime
toString() - Method in class com.unitech.stuhfl.STUHFL_T_BatteryInfo
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Beeper
toString() - Method in class com.unitech.stuhfl.STUHFL_T_BTMAC
toString() - Method in class com.unitech.stuhfl.STUHFL_T_DataFormat
toString() - Method in class com.unitech.stuhfl.STUHFL_T_DataInfo
toString() - Method in class com.unitech.stuhfl.STUHFL_T_DataRange
toString() - Method in class com.unitech.stuhfl.STUHFL_T_DataTerminator
toString() - Method in class com.unitech.stuhfl.STUHFL_T_FindDevice
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Erase
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Read
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Read
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Write
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Model
toString() - Method in class com.unitech.stuhfl.STUHFL_T_OperatingMode
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ReadMode
toString() - Method in class com.unitech.stuhfl.STUHFL_T_SerialNumber
toString() - Method in class com.unitech.stuhfl.STUHFL_T_SKU
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqProfile
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AdaptiveSensitivity
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Option
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AdaptiveSensitivity
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Option
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
toString() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Temperature
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Time
toString() - Method in class com.unitech.stuhfl.STUHFL_T_VersionBoard
toString() - Method in class com.unitech.stuhfl.STUHFL_T_VersionBoardInfo
toString() - Method in class com.unitech.stuhfl.STUHFL_T_VersionLib
toString() - Method in class com.unitech.stuhfl.STUHFL_T_Vibrator
toString() - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_Caps
  < I/O Param: OUT capacitance of tuning table
toString() - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem
  < rfu
toString() - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
  < I/O Param: OUT capacitance of tuning table
toString() - Method in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Number of RX count errors.
toString() - Method in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Tag TID.
TransportBluetooth - Class in com.unitech.lib.transport
  The Transport class is a class for abstracting connections with Reader devices.
TransportBluetooth() - Constructor for class com.unitech.lib.transport.TransportBluetooth
  Create an instance of the TransportBluetooth class
TransportBluetooth(DeviceType, String, String) - Constructor for class com.unitech.lib.transport.TransportBluetooth
  Create an instance of the TransportBluetooth class
TransportUART - Class in com.unitech.lib.transport
TransportUART(DeviceType, String, int) - Constructor for class com.unitech.lib.transport.TransportUART
trext - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
trext - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
  < I/O Param: Coding: STUHFL_D_GEN2_CODING_FM0, ...
trext - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_ProtocolCfg.Fields
trext - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_ProtocolCfg.Fields
triggerEvent(int, int, Object) - Method in class com.unitech.lib.htx.protocol.ProtocolHT730
triggerEvent(int, int, Object) - Method in interface com.unitech.lib.protocol.IProtocol
triggerEvent(int, int, Object) - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
truncation - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Mask length.
truncation - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
tune(boolean, boolean, STUHFL_E.TUNING_ALGO) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Perform tuning for actual selected channel list
tune(boolean, boolean, STUHFL_E.TUNING_ALGO, short) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Perform tuning for actual selected channel list
tuningStatus - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Inventory rounds already done.
txOutputLevel - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
txOutputLevel - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields

A B C D E F G H I K L M N O P Q R S T U V W X _