A B C D E F G H I K L M N O P Q R S T U V W X _

## G

GBT29768_SORT_MASK_SIZE - Static variable in class com.unitech.stuhflBridge.NativeDefines
GEN2_LOCK_MASK_SIZE - Static variable in class com.unitech.stuhflBridge.NativeDefines
GEN2_SELECT_MASK_SIZE - Static variable in class com.unitech.stuhflBridge.NativeDefines
generateReaderActionChanged(BaseReader, ResultCode, ActionState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderBatteryState(BaseReader, int, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderKeyChanged(BaseReader, KeyType, KeyState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderNotificationState(BaseReader, NotificationState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderStateChanged(BaseReader, ConnectState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderTemperatureState(BaseReader, double, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateUHFAccessResult(BaseUHF, ResultCode, ActionState, String, String, Object) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
generateUHFReadTag(BaseUHF, String, Object) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
getAccessPassword() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAccessPassword() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAction() - Method in interface com.unitech.lib.device.IReader
  Returns the current behavior of the device associated with an instance of the BaseReader class.
getAction() - Method in class com.unitech.lib.reader.BaseReader
  Returns the current behavior of the device associated with an instance of the BaseReader class.
getAction() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Action value of "Selection Mask".
getAction(ActionType) - Static method in class com.unitech.lib.util.ActionUtil
getAddress() - Method in interface com.unitech.lib.device.IReader
  Returns the address of the device associated with an instance of the BaseReader class.
getAddress() - Method in class com.unitech.lib.reader.BaseReader
  Returns the address of the device associated with an instance of the BaseReader class.
getAddress() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the address of the device to which the BaseTransport instance is connected.
getAlgorithmType() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
getAlgorithmType() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getAlgorithmType() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getAlgorithmType() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getAlgorithmType() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getAppName(Context) - Static method in class com.unitech.lib.util.SysUtil
getAutoOffTime() - Method in class com.unitech.lib.htx.HT730Reader
getAutoOffTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time which the instrument automatically turns off.
getAutoOffTime() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getAutoOffTime() - Method in class com.unitech.lib.rpx.RP902Reader
getAutoOffTimeList() - Method in class com.unitech.lib.htx.HT730Reader
getAutoOffTimeList() - Method in class com.unitech.lib.reader.BaseReader
  Returns the equipment supports auto off time list, the unit is minutes
getAutoOffTimeList() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getAutoOffTimeList() - Method in class com.unitech.lib.rpx.RP902Reader
getBank() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
getBatteryRemains() - Method in class com.unitech.lib.rpx.device.DeviceRP902
  Get the device's battery status
getBatteryState() - Method in class com.unitech.lib.htx.HT730Reader
getBatteryState() - Method in class com.unitech.lib.reader.BaseReader
  Returns the battery state of the equipment.
getBatteryState() - Method in class com.unitech.lib.rpx.RP902Reader
getBaudRate() - Method in class com.unitech.lib.transport.TransportUART
getBeeper() - Method in class com.unitech.lib.htx.HT730Reader
getBeeper() - Method in class com.unitech.lib.reader.BaseReader
  Returns the beeper operation status of the equipment.
getBeeper() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getBeeper() - Method in class com.unitech.lib.rpx.RP902Reader
getBLF() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
getBLF() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getBLF() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getBLF() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getBLF() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getCaps(int) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Get tuning cap values from channel item.
getCheckInterval() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time period for checking the battery status of the device associated with an instance of the BaseReader class.
getCode() - Method in exception com.unitech.lib.diagnositics.ReaderException
  Get fault and motion results.
getCode() - Method in class com.unitech.lib.protocol.Response
getCode() - Method in enum com.unitech.lib.reader.types.BeeperState
getCode() - Method in enum com.unitech.lib.reader.types.KeyState
getCode() - Method in enum com.unitech.lib.reader.types.KeyType
getCode() - Method in enum com.unitech.lib.reader.types.NotificationState
getCode() - Method in enum com.unitech.lib.reader.types.VibratorState
getCode() - Method in enum com.unitech.lib.rpx.types.CommandType
getCode() - Method in enum com.unitech.lib.rpx.types.DeviceOptionType
getCode() - Method in enum com.unitech.lib.rpx.types.SubCommandType
getCode() - Method in enum com.unitech.lib.transport.types.ConnectState
getCode() - Method in enum com.unitech.lib.transport.types.ConnectType
getCode() - Method in enum com.unitech.lib.types.ActionState
getCode() - Method in enum com.unitech.lib.types.ActionType
getCode() - Method in enum com.unitech.lib.types.DataFormat
getCode() - Method in enum com.unitech.lib.types.DataInfo
getCode() - Method in enum com.unitech.lib.types.DataTerminator
getCode() - Method in enum com.unitech.lib.types.DeviceType
getCode() - Method in enum com.unitech.lib.types.FindDeviceMode
getCode() - Method in interface com.unitech.lib.types.IEnumType
  Get the enum code value
getCode() - Method in enum com.unitech.lib.types.ModuleUHFType
getCode() - Method in enum com.unitech.lib.types.OperatingMode
getCode() - Method in enum com.unitech.lib.types.ReadMode
getCode() - Method in enum com.unitech.lib.types.ResultCode
getCode() - Method in enum com.unitech.lib.types.SKUType
getCode() - Method in enum com.unitech.lib.uhf.types.AlgorithmType
getCode() - Method in enum com.unitech.lib.uhf.types.BankType
getCode() - Method in enum com.unitech.lib.uhf.types.BLFType
getCode() - Method in enum com.unitech.lib.uhf.types.Encoding
getCode() - Method in enum com.unitech.lib.uhf.types.GlobalBandType
getCode() - Method in enum com.unitech.lib.uhf.types.LockState
getCode() - Method in enum com.unitech.lib.uhf.types.Mask6cAction
getCode() - Method in enum com.unitech.lib.uhf.types.Mask6cTarget
getCode() - Method in enum com.unitech.lib.uhf.types.PowerMode
getCode() - Method in enum com.unitech.lib.uhf.types.Session
getCode() - Method in enum com.unitech.lib.uhf.types.Target
getCode() - Method in enum com.unitech.lib.uhf.types.TARIType
getConfig() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the config of RFID module
getConfig() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getConfig() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getConfig() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getConfig() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getConnectType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the instance of BaseReader associated with device.
getConnectType() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the instance of Transport associated with device.
getContext() - Static method in class com.unitech.lib.util.SysUtil
getContinuousMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns whether the RFID UHF module on the device will cause the Inventory to run continuously.
getContinuousMode() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getContinuousMode() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getContinuousMode() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getContinuousMode() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getData() - Method in class com.unitech.lib.protocol.Response
getData() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access result data value with HEX format.
getDataFormat() - Method in class com.unitech.lib.htx.HT730Reader
getDataFormat() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data format setting of the equipment.
getDataFormat() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getDataFormat() - Method in class com.unitech.lib.rpx.RP902Reader
getDataInfo() - Method in class com.unitech.lib.htx.HT730Reader
getDataInfo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data info setting of the equipment.
getDataInfo() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getDataInfo() - Method in class com.unitech.lib.rpx.RP902Reader
getDataRange() - Method in class com.unitech.lib.htx.HT730Reader
getDataRange() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data range setting of the equipment.
getDataRange() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getDataRange() - Method in class com.unitech.lib.rpx.RP902Reader
getDataTerminator() - Method in class com.unitech.lib.htx.HT730Reader
getDataTerminator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data terminator setting of the equipment.
getDataTerminator() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getDataTerminator() - Method in class com.unitech.lib.rpx.RP902Reader
getDeviceName() - Method in interface com.unitech.lib.device.IReader
  Returns the name of the Device associated with an instance of the BaseReader class.
getDeviceName() - Method in class com.unitech.lib.reader.BaseReader
  Returns the name of the Device associated with an instance of the BaseReader class.
getDeviceName() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the name of the Device to which the BaseTransport instance is connected.
getDeviceType() - Method in interface com.unitech.lib.device.IReader
  Returns the type of Device to which the instance is connected.
getDeviceType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the type of Device to which the instance is connected.
getDeviceType() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the type of device to which the instance will be connected.
getEncoding() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
getEncoding() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getEncoding() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getEncoding() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getEncoding() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getEpc() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access tag's EPC value with HEX format.
getEpc() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's EPC value with HEX format.
getEpc() - Method in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
getFastMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
getFastMode() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getFastMode() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
  Returns the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
getFastMode() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
  Returns the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
getFastMode() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getFindDevice() - Method in class com.unitech.lib.htx.HT730Reader
getFindDevice() - Method in class com.unitech.lib.reader.BaseReader
  Returns the find device status of the equipment.
getFindDevice() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getFindDevice() - Method in class com.unitech.lib.rpx.RP902Reader
getFrequency() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's frequency value.
getFront() - Method in class com.unitech.lib.util.collections.ByteQueue
  Get the front position of the data
getGlobalBand() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the national orientation of the RFID UHF module of the instrument.
getGlobalBand() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getGlobalBand() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getIdleTime() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument returns the time that the radio waves are not output in the Inventory operation and is resting.
getIdleTime() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getIdleTime() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getIdleTime() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getIdleTime() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getImmortalTicket() - Method in class com.unitech.lib.util.ServiceHandler
  Get a ticket for a work continued longer than 30 sec.
getInstance(Context) - Static method in class com.unitech.lib.pogo.PogoCtrl
  Instantiates a new Pogo ctrl object.
getInstance() - Static method in class com.unitech.stuhfl.STUHFL
getInventoryCfg() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getInventoryTime() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the time at which radio waves are actually output from the Inventory operation of the RFID UHF module in the instrument.
getInventoryTime() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getInventoryTime() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getInventoryTime() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getInventoryTime() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getKeyState() - Method in class com.unitech.lib.reader.params.KeyEventItem
getKeyType() - Method in class com.unitech.lib.reader.params.KeyEventItem
getKillPassword() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getKillPassword() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getLastError() - Method in interface com.unitech.lib.device.IReader
  Returns the result code for the last action.
getLastError() - Method in class com.unitech.lib.reader.BaseReader
  Returns the result code for the last action.
getLength() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns the Length of the EPCMaskParam instance.
getLength() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Returns the pattern length of the Mask6cPattern instance.
getLength() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Length value of "Selection Mask".
getLogLevel() - Static method in class com.unitech.lib.util.diagnotics.UniLog
getMacAddress() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the MAC address of the device to which the BaseTransport instance is connected.
getMask6cAction(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cAction(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMask6cBank(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cBank(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMask6cMaxSize() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cMaxSize() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMask6cOffset(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cOffset(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMask6cPattern(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cPattern(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMask6cTarget(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cTarget(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMask6cUsed(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMask6cUsed(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMax() - Method in class com.unitech.lib.uhf.params.PowerRange
  Returns the maximum Power Gian Level value for a PowerRange instance.
getMaxQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the maximum Q value.
getMaxQ() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getMaxQ() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMaxQ() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMaxQ() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getMessage() - Method in enum com.unitech.lib.types.ResultCode
  Returns the result code's description.
getMin() - Method in class com.unitech.lib.uhf.params.PowerRange
  Returns the Power Gian Level minimum value for a PowerRange instance.
getMinQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the minimum Q value.
getMinQ() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getMinQ() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getMinQ() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getMinQ() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getMode() - Method in class com.unitech.lib.reader.params.FindDevice
  Returns FindDeviceMode.
getModuleInfo(DeviceOptionType) - Method in class com.unitech.lib.htx.device.DeviceHT730
  Get the specific module's model number in the device
getModuleInfo(DeviceOptionType) - Method in class com.unitech.lib.rpx.device.DeviceRP902
  Get the specific module's model number in the device
getModuleProfile() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
getModuleProfile() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getModuleProfile() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getModuleProfile() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getNull(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
getOffset() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns the offset of the EPCMaskParam instance.
getOffset() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Offset value of "Selection Mask".
getOperatingMode() - Method in class com.unitech.lib.htx.HT730Reader
getOperatingMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the operating mode status of the equipment.
getOperatingMode() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getOperatingMode() - Method in class com.unitech.lib.rpx.RP902Reader
getPath() - Method in class com.unitech.lib.transport.TransportUART
getPattern() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns Pattern of the EPCMaskParam instance.
getPattern() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Returns the Mask pattern of the Mask6cPattern instance.
getPattern() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Pattern value of "Selection Mask".
getPC() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's PC value with HEX format.
getPos(int) - Method in class com.unitech.lib.util.collections.ByteQueue
getPower() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna output of the RFID UHF module of the instrument.
getPower() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getPower() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getPower() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getPower() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getPowerGainRange() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getPowerGainRange() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getPowerMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the power mode that the RFID UHF module of the appliance uses to perform the inventory.
getPowerMode() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getPowerMode() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getPowerMode() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getPowerRange() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna output range of the RFID UHF module of the instrument.
getPowerRange() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getPowerRange() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getProtocol() - Method in interface com.unitech.lib.device.IReader
  Use only within the SDK.
getProtocol() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
getProtocol() - Method in class com.unitech.lib.reader.device.BaseDevice
getProtocol() - Method in class com.unitech.lib.uhf.module.BaseModuleUHF
  Use only within the SDK.
getProtocolCfg() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getQueueSize() - Method in class com.unitech.lib.util.collections.ByteQueue
getReadMode() - Method in class com.unitech.lib.htx.HT730Reader
getReadMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the read mode status of the equipment.
getReadMode() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getReadMode() - Method in class com.unitech.lib.rpx.RP902Reader
getRegion() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getRegion() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getResultCode(byte[]) - Static method in class com.unitech.lib.protocol.Response
getRfidUhf() - Method in class com.unitech.lib.reader.BaseReader
  If the BaseReader instance supports the RFID UHF module, it returns an interface object that can control the RFID UHF module.
getRssi() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's RSSI value.
getSelectMask6c(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6c(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6c(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cAction(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the comparison behavior of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cAction(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cAction(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cBank(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the Device's RFID UHF module returns the memory bank to compare.
getSelectMask6cBank(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cBank(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cEnabled(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns whether to use the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cEnabled(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cEnabled(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cMaxSize() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the max size of select mask list status of the RFID UHF module.
getSelectMask6cMaxSize() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cMaxSize() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cOffset(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the Device returns the starting address of the memory to start the comparison.
getSelectMask6cOffset(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cOffset(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cPattern(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the comparison value and length of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cPattern(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cPattern(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSelectMask6cTarget(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Flag of the tag to store the comparison result of Selection Mask item of RFID UHF module of Device.
getSelectMask6cTarget(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSelectMask6cTarget(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSerialNo() - Method in interface com.unitech.lib.device.IReader
  Returns the serial number of the device.
getSerialNo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the serial number of the device.
getSerialNo() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getSession() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the device returns the Session to check the state of the Session of the tag to be read by the Inventory operation.
getSession() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSession() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getSession() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getSession() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getSize() - Method in class com.unitech.lib.util.collections.ByteQueue
  Get the byte size in the queue
getSize(int) - Method in class com.unitech.lib.util.collections.ByteQueue
getSize(int, int) - Method in class com.unitech.lib.util.collections.ByteQueue
getSKU() - Method in class com.unitech.lib.htx.HT730Reader
getSKU() - Method in class com.unitech.lib.reader.BaseReader
  Returns the SKU type of the equipment.
getSKU() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getSKU() - Method in class com.unitech.lib.rpx.RP902Reader
getSKU() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getSKU() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getSKU() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getSKU() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getStartQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, it returns the starting Q value.
getStartQ() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getStartQ() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getStartQ() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getStartQ() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getState() - Method in class com.unitech.lib.reader.BaseReader
  Returns the connection status of the device with the instance of the BaseReader class.
getState() - Method in class com.unitech.lib.transport.BaseTransport
  The instance of BaseTransport returns the connection status with device.
getTail() - Method in class com.unitech.lib.util.collections.ByteQueue
getTarget() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the device returns the status of the Target of the tag to be read by the Inventory operation.
getTarget() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getTarget() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getTarget() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getTarget() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Target Flag of "Selection Mask".
getTarget() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getTARI() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
getTARI() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getTARI() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getTARI() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getTARI() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getTemperature() - Method in class com.unitech.lib.htx.HT730Reader
getTemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the temperature of the equipment.
getTemperature() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getTemperature() - Method in class com.unitech.lib.rpx.RP902Reader
getTemperature() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getTemperature() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getTicket() - Method in class com.unitech.lib.util.ServiceHandler
  Get a ticket for a work
getTid() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'TID memory'.
getTid() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'TID memory'.
getTID() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's TID value with HEX format.
getTime() - Method in class com.unitech.lib.htx.HT730Reader
getTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the system time of the device.
getTime() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getTime() - Method in class com.unitech.lib.rpx.RP902Reader
getTimeout() - Method in class com.unitech.lib.reader.params.FindDevice
  Returns timeout value.
getTimeout() - Method in class com.unitech.lib.uhf.module.BaseModuleUHF
  Returns the timeout value of the communication with RFID UHF module.
getToggleTarget() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
getToggleTarget() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getToggleTarget() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
  Returns the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
getToggleTarget() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
  Returns the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
getToggleTarget() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getTransport() - Method in class com.unitech.lib.reader.BaseReader
  Returns an instance of the BaseTransport class that connects an instance of the BaseReader class to the Device.
getTransport() - Method in class com.unitech.lib.reader.device.BaseDevice
getTransport() - Method in class com.unitech.lib.reader.protocol.Protocol
getType() - Method in enum com.unitech.lib.rpx.types.DeviceOptionType
getType() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the RFID UHF module type of the connected Device.
getType() - Method in class com.unitech.lib.uhf.module.BaseModuleUHF
  Returns the RFID UHF module type of the connected Device.
getUartPath() - Method in class com.unitech.lib.pogo.PogoCtrl
getUser() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getUser() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getVersion() - Method in interface com.unitech.lib.device.IReader
  Returns the firmware version of the device associated with the instance of the BaseReader class.
getVersion() - Method in class com.unitech.lib.htx.device.DeviceHT730
getVersion() - Method in class com.unitech.lib.reader.BaseReader
  Returns the firmware version of the device associated with the instance of the BaseReader class.
getVersion() - Method in class com.unitech.lib.reader.device.BaseDevice
getVersion() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getVersion() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the version of the RFID UHF module.
getVersion() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
getVersion() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
getVersion() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
getVersion() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
getVersion(Context) - Static method in class com.unitech.lib.util.SysUtil
getVibrator() - Method in class com.unitech.lib.htx.HT730Reader
getVibrator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the vibrator operation status of the equipment.
getVibrator() - Method in class com.unitech.lib.rpx.device.DeviceRP902
getVibrator() - Method in class com.unitech.lib.rpx.RP902Reader
GlobalBandType - Enum in com.unitech.lib.uhf.types
  The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.

A B C D E F G H I K L M N O P Q R S T U V W X _