com.unitech.stuhfl

## Class STUHFL_T_ST25RU3993_FreqHop

- java.lang.Object
- - com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop
  - - com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop

-     public class STUHFL_T_ST25RU3993_FreqHop
      extends BR_ST25RU3993_FreqHop

- - ### Nested Class Summary

    - ### Nested classes/interfaces inherited from class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop

      `BR_ST25RU3993_FreqHop.Fields`

  - ### Field Summary

    Fields
    Modifier and Type | Field and Description
    --- | ---
    `int` | `maxSendingTime`
    `int` | `minSendingTime` < I/O Param: Maximum sending time before frequency hopping is performed.
    `STUHFL_E.FREQUENCY_HOP_MODE` | `mode` < I/O Param: Minimum sending time before frequency hopping is performed

  - ### Constructor Summary

    Constructors
    Constructor and Description
    `STUHFL_T_ST25RU3993_FreqHop()`
    `STUHFL_T_ST25RU3993_FreqHop(int maxSendingTime, int minSendingTime, STUHFL_E.FREQUENCY_HOP_MODE mode)`
    `STUHFL_T_ST25RU3993_FreqHop(STUHFL_T_ST25RU3993_FreqHop other)` < I/O Param: Hopping mode

  - ### Method Summary

    All Methods Instance Methods Concrete Methods
    Modifier and Type | Method and Description
    --- | ---
    `STUHFL_E.RET_CODE` | `commit()` Set new frequency hopping time configuration
    `STUHFL_E.RET_CODE` | `fetch()` Get frequency hopping time configuration
    `java.lang.String` | `toString()`

    - ### Methods inherited from class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop

      `_Get_FreqHop, _Set_FreqHop`

    - ### Methods inherited from class java.lang.Object

      `clone, equals, finalize, getClass, hashCode, notify, notifyAll, wait, wait, wait`

- - ### Field Detail

    - #### maxSendingTime

          public int maxSendingTime

    - #### minSendingTime

          public int minSendingTime

      < I/O Param: Maximum sending time before frequency hopping is performed. Minimum allowed value: 40ms

    - #### mode

          public STUHFL_E.FREQUENCY_HOP_MODE mode

      < I/O Param: Minimum sending time before frequency hopping is performed

  - ### Constructor Detail

    - #### STUHFL_T_ST25RU3993_FreqHop

          public STUHFL_T_ST25RU3993_FreqHop(STUHFL_T_ST25RU3993_FreqHop other)

      < I/O Param: Hopping mode

    - #### STUHFL_T_ST25RU3993_FreqHop

          public STUHFL_T_ST25RU3993_FreqHop(int maxSendingTime,
                                             int minSendingTime,
                                             STUHFL_E.FREQUENCY_HOP_MODE mode)

    - #### STUHFL_T_ST25RU3993_FreqHop

          public STUHFL_T_ST25RU3993_FreqHop()

  - ### Method Detail

    - #### commit

          public STUHFL_E.RET_CODE commit()

      Set new frequency hopping time configuration
      Returns:
        error code

    - #### fetch

          public STUHFL_E.RET_CODE fetch()

      Get frequency hopping time configuration
      Returns:
        error code

    - #### toString

          public java.lang.String toString()

      Overrides:
        `toString` in class `java.lang.Object`