A B C D E F G H I K L M N O P Q R S T U V W X _

## M

MacToHost16(short) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
MacToHost32(int) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
major - Variable in class com.unitech.stuhfl.STUHFL_T_VersionLib
major - Variable in class com.unitech.stuhflBridge.BR_Version.Fields
majorHW - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoard
  < O Param: Build version board SW
majorSW - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoard
mask - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: Bank (TagInfo, Coding, Security, User) on which apply the sort.
mask - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
mask - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Bank (File, EPC, TID, USER) on which apply the select.
mask - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
mask - Variable in class com.unitech.stuhflBridge.BR_Gen2_Lock.Fields
mask - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
Mask6cAction - Enum in com.unitech.lib.uhf.types
  The Mask6cAction enumeration type indicates the status of the Flag when the RFID UHF module performs the Inventory operation and the pattern of the given Selection Mask is set as the Target value of the Selection Mask according to the condition.
Mask6cPattern - Class in com.unitech.lib.uhf.params
  The Mask6cPattern class is a class that represents the Mask Pattern of a Selection Mask in terms of pattern and length.
Mask6cPattern() - Constructor for class com.unitech.lib.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cPattern(<any>) - Constructor for class com.unitech.lib.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cPattern(String, int) - Constructor for class com.unitech.lib.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cTarget - Enum in com.unitech.lib.uhf.types
  The Mask6cTarget enumeration represents the Flag where the result status of the Selection Mask will be saved when the RFID UHF module is inventoried.
maskBitLength - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: Bit starting address to which mask is applied (bit address).
maskBitLength - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Starting address to which mask is applied.
maskBitLength - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
maskBitLength - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
maskBitPointer - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: Selection mask.
maskBitPointer - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Selection mask.
maskBitPointer - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
maskBitPointer - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
maxFrequency - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqProfile
maxFrequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqProfile.Fields
maxPercent() - Method in enum com.unitech.lib.uhf.module.impinj.types.PowerModeLevel
  Get the max percent value.
maxQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The maximum Q value
maxQ - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
  < I/O Param: Minimum value that Q could reach
maxSendingTime - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
  < I Param: Flag to enable or disable modulation
maxSendingTime - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
maxSendingTime - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
maxSendingTime - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop.Fields
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Erase
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Read
  < I Param: Word address to which read data.
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: Elicit the tag behavior according to Gb29768 Sort specification.
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
  < I Param: Word address to which write data.
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
  < I Param: Password.
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Read
  < I Param: Word address to which read data.
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Elicit the tag behavior according to Gen2 Select specification.
memoryBank - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Write
  < I Param: Word address to which write data.
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Erase.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Lock.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Read.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Write.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gen2_BlockWrite.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gen2_Read.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
memoryBank - Variable in class com.unitech.stuhflBridge.BR_Gen2_Write.Fields
micro - Variable in class com.unitech.stuhfl.STUHFL_T_VersionLib
  < O Param: Minor version
micro - Variable in class com.unitech.stuhflBridge.BR_Version.Fields
  < O Param: Minor version
microHW - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoard
  < O Param: Minor version board HW
microSW - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoard
  < O Param: Minor version board SW
minFrequency - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqProfile
minFrequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqProfile.Fields
minor - Variable in class com.unitech.stuhfl.STUHFL_T_VersionLib
  < O Param: Major version
minor - Variable in class com.unitech.stuhflBridge.BR_Version.Fields
  < O Param: Major version
minorHW - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoard
  < O Param: Major version board HW
minorSW - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoard
  < O Param: Major version board SW
minQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The minimum Q value
minQ - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
  < I/O Param: Q starting value
minSendingTime - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
  < I/O Param: Maximum sending time before frequency hopping is performed.
minSendingTime - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop.Fields
mLastTime - Variable in class com.unitech.lib.reader.BaseReader
mode - Variable in class com.unitech.stuhfl.STUHFL_T_FindDevice
mode - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
mode - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
mode - Variable in class com.unitech.stuhfl.STUHFL_T_OperatingMode
mode - Variable in class com.unitech.stuhfl.STUHFL_T_ReadMode
mode - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
mode - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
  < I/O Param: Minimum sending time before frequency hopping is performed
mode - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
mode - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
mode - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_AntennaPower.Fields
mode - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop.Fields
modelName - Variable in class com.unitech.stuhfl.STUHFL_T_Model
modulationMode - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
  < I Param: Maximum modulation time in ms.
modulationMode - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
moduleProfile - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The module's profile setting, only for HT730
ModuleUHFRM100 - Class in com.unitech.lib.uhf.module.impinj
ModuleUHFRM100(IReader, IProtocol, IModuleRfidUhfEventListener, int) - Constructor for class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
  Create an instance of the BaseModuleUHF class.
ModuleUHFST25RU3993 - Class in com.unitech.lib.uhf.module.stseries
ModuleUHFST25RU3993(IReader, IProtocol, IModuleRfidUhfEventListener) - Constructor for class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
  Create an instance of the ModuleRfidUhf class.
ModuleUHFType - Enum in com.unitech.lib.types
  The ModuleUHFType enumeration indicates the type of RFID UHF Module installed in the instrument.

A B C D E F G H I K L M N O P Q R S T U V W X _