A B C D E F G H I K L M N O P Q R S T U V W X _

## S

sel - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams
SelectMask6cParam - Class in com.unitech.lib.uhf.params
  The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
SelectMask6cParam() - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, String, int) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, <any>) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
send(byte[], int) - Method in class com.unitech.lib.htx.protocol.ProtocolHT730
send(byte[], int) - Method in interface com.unitech.lib.protocol.IProtocol
  Send the data to module and receive the response
send(byte[], int) - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
sensitivity - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: RSSI log mean value.
ServiceConnection() - Constructor for class com.unitech.lib.util.ServiceHandler.ServiceConnection
ServiceHandler - Class in com.unitech.lib.util
  Created by USER
ServiceHandler(Context, String, String, ServiceHandler.ServiceConnectionCallback) - Constructor for class com.unitech.lib.util.ServiceHandler
ServiceHandler.ServiceConnection - Class in com.unitech.lib.util
ServiceHandler.ServiceConnectionCallback - Interface in com.unitech.lib.util
session - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Session setting
Session - Enum in com.unitech.lib.uhf.types
  The Session enumeration represents the session of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
session - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams
  < I/O Param: Condition setting
session - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams
  < I/O Param: For QUERY Sel field
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAction(ActionState) - Method in interface com.unitech.lib.device.IReader
  Use only within the SDK.
setAction(ActionState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operational state of the device associated with the instance.
setAction(Mask6cAction) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
setAddress(String) - Method in interface com.unitech.lib.device.IReader
  Sets the address of the device to which the instance of BaseReader is connected.
setAddress(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the address of the device to which the instance of BaseReader is connected.
setAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the address of the device to which the BaseTransport instance is connected.
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setAutoOffTime(int) - Method in class com.unitech.lib.htx.HT730Reader
setAutoOffTime(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time which the equipment automatically turns off.
setAutoOffTime(int) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setAutoOffTime(int) - Method in class com.unitech.lib.rpx.RP902Reader
setBank(BankType) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Bank value in "Selection Mask".
setBeeper(BeeperState) - Method in class com.unitech.lib.htx.HT730Reader
setBeeper(BeeperState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the beeper operation status of the equipment.
setBeeper(BeeperState) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setBeeper(BeeperState) - Method in class com.unitech.lib.rpx.RP902Reader
setBLF(BLFType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
setBLF(BLFType) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setBLF(BLFType) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setBLF(BLFType) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setBLF(BLFType) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setCaps(int, short, short, short) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Set tuning cap values for selected channel item.
setCheckInterval(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time period for checking the battery status of the device associated with the BaseReader class instance.
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.BaseUHF
  Setup the config of the RFID module
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setConnected(boolean) - Method in class com.unitech.stuhflBridge.LibBridge
setContext(Context) - Static method in class com.unitech.lib.util.SysUtil
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets whether or not the RFID UHF module of the device will run the Inventory continuously.
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setDataFormat(DataFormat) - Method in class com.unitech.lib.htx.HT730Reader
setDataFormat(DataFormat) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data format setting of the equipment.
setDataFormat(DataFormat) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setDataFormat(DataFormat) - Method in class com.unitech.lib.rpx.RP902Reader
setDataInfo(DataInfo) - Method in class com.unitech.lib.htx.HT730Reader
setDataInfo(DataInfo) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data info setting of the equipment.
setDataInfo(DataInfo) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setDataInfo(DataInfo) - Method in class com.unitech.lib.rpx.RP902Reader
setDataRange(DataRange) - Method in class com.unitech.lib.htx.HT730Reader
setDataRange(DataRange) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data range setting of the equipment.
setDataRange(DataRange) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setDataRange(DataRange) - Method in class com.unitech.lib.rpx.RP902Reader
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.htx.HT730Reader
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data terminator setting of the equipment.
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.rpx.RP902Reader
setDeviceName(String) - Method in interface com.unitech.lib.device.IReader
  Sets the name of the device to which the instance of BaseReader is connected.
setDeviceName(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the name of the device to which the instance of BaseReader is connected.
setDeviceName(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the name of the device to which the BaseTransport instance is connected.
setDeviceType(DeviceType) - Method in interface com.unitech.lib.device.IReader
  Sets the type of device to which instance of BaseReader will be connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.reader.BaseReader
  Sets the type of device to which instance of BaseReader will be connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the type of device to which the instance will be connected.
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setException(ReaderException) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setException(ReaderException) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setFastMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setFastMode(boolean) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
  Sets the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
  Sets the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setFindDevice(FindDevice) - Method in class com.unitech.lib.htx.HT730Reader
setFindDevice(FindDevice) - Method in class com.unitech.lib.reader.BaseReader
  Sets the find device status of the equipment.
setFindDevice(FindDevice) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setFindDevice(FindDevice) - Method in class com.unitech.lib.rpx.RP902Reader
setFront(int) - Method in class com.unitech.lib.util.collections.ByteQueue
setGlobalBand(GlobalBandType) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the national orientation of the RFID UHF module of the instrument.
setGlobalBand(GlobalBandType) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setGlobalBand(GlobalBandType) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setIdleTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument sets the time for which the radio waves are not output in the Inventory operation and the rest of the time.
setIdleTime(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setIdleTime(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setIdleTime(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setIdleTime(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setIdleTimeEx(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setInventoryTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the time at which radio waves are actually output in Inventory operation of the RFID UHF module of the instrument.
setInventoryTime(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setInventoryTime(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setInventoryTime(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setInventoryTime(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setLastError(ResultCode) - Method in interface com.unitech.lib.device.IReader
  Use only within the SDK.
setLastError(ResultCode) - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
setLength(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Length of the EPCMaskParam instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the pattern length of the Mask6cPattern instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Length value of "Selection Mask".
setLogLevel(int) - Static method in class com.unitech.lib.util.diagnotics.UniLog
setMacAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the MAC address of the device to which the BaseTransport instance is connected.
setMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMask6cPattern(int, String, int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMask6cPattern(int, String, int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMask6cUsed(int, boolean) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMask6cUsed(int, boolean) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMax(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the maximum Power Gian Level value for a PowerRange instance.
setMaxQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the maximum Q value.
setMaxQ(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setMaxQ(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMaxQ(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMaxQ(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setMin(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the Power Gian Level minimum value for a PowerRange instance.
setMinQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the minimum Q value.
setMinQ(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setMinQ(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setMinQ(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setMinQ(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setMode(FindDeviceMode) - Method in class com.unitech.lib.reader.params.FindDevice
  Set FindDeviceMode.
setModuleProfile(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
setModuleProfile(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setModuleProfile(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setModuleProfile(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setOffset(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the offset of the EPCMaskParam instance.
setOffset(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Offset value of "Selection Mask".
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.htx.HT730Reader
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operating mode status of the equipment.
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.rpx.RP902Reader
setPattern(String) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Pattern for the EPCMaskParam instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the Mask pattern for the instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Pattern value of "Selection Mask".
setPower(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the antenna output of the RFID UHF module of the instrument.
setPower(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setPower(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setPower(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setPower(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the power mode the RFID UHF module of the appliance uses to perform the inventory.
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setReadMode(ReadMode) - Method in class com.unitech.lib.htx.HT730Reader
setReadMode(ReadMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the read mode status of the equipment.
setReadMode(ReadMode) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setReadMode(ReadMode) - Method in class com.unitech.lib.rpx.RP902Reader
setRegion(GlobalBandType) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setRegion(GlobalBandType) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setSelectMask() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setSelectMask() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setSelectMask6c(int, SelectMask6cParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6c(int, SelectMask6cParam) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6c(int, SelectMask6cParam) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSelectMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison behavior of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSelectMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the memory bank to be compared.
setSelectMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSelectMask6cEnabled(int, boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set whether or not to use the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cEnabled(int, boolean) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6cEnabled(int, boolean) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSelectMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the start address of the memory to start the comparison.
setSelectMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison value and length of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Flag of the tag to save the comparison result of Selection Mask item of the RFID UHF module of the device.
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setSession(Session) - Method in class com.unitech.lib.uhf.BaseUHF
  Device's RFID UHF module sets the Session to check the status of the Session of the tag to be read by Inventory operation.
setSession(Session) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setSession(Session) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setSession(Session) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setSession(Session) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setStartQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, set the starting Q value.
setStartQ(int) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setStartQ(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setStartQ(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setStartQ(int) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setState(ConnectState, Object) - Method in class com.unitech.lib.transport.BaseTransport
setStateListener(IConnectStateEventListener) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the listener to receive the connection status of an instance of the BaseTransport class.
setTail(int) - Method in class com.unitech.lib.util.collections.ByteQueue
setTarget(Target) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the state of target of tag to read by Inventory operation.
setTarget(Target) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setTarget(Target) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setTarget(Target) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setTarget(Mask6cTarget) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Target Flag of "Selection Mask".
setTarget(Target) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setTARI(TARIType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
setTARI(TARIType) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setTARI(TARIType) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
setTARI(TARIType) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
setTARI(TARIType) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setTid(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'TID memory'.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'TID memory'.
setTime(Date) - Method in class com.unitech.lib.htx.HT730Reader
setTime(Date) - Method in class com.unitech.lib.reader.BaseReader
  Sets the system time of the instrument.
setTime(String) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setTime(Date) - Method in class com.unitech.lib.rpx.RP902Reader
setTimeout(int) - Method in class com.unitech.lib.reader.params.FindDevice
  Set timeout.
setTimeout(int) - Method in class com.unitech.lib.uhf.module.BaseModuleUHF
  Set the timeout value of the communication with RFID UHF module.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
  Sets the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
  Sets the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
setUsed(boolean) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set whether or not to use "Selection Mask".
setUser(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setUser(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setVibrator(VibratorState) - Method in class com.unitech.lib.htx.HT730Reader
setVibrator(VibratorState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the vibrator operation status of the equipment.
setVibrator(VibratorState) - Method in class com.unitech.lib.rpx.device.DeviceRP902
setVibrator(VibratorState) - Method in class com.unitech.lib.rpx.RP902Reader
shutdown() - Static method in class com.unitech.lib.util.diagnotics.UniLog
skipCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Number of collisions.
skipLBTcheck - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
  < I/O Param: RSSI threshold value
skipLBTcheck - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
skipStopResponse(boolean) - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
sku - Variable in class com.unitech.stuhfl.STUHFL_T_SKU
SKUType - Enum in com.unitech.lib.types
  The SKUType enumeration represents the type of device associated with the SDK.
sleep(int) - Static method in class com.unitech.lib.util.SysUtil
sn - Variable in class com.unitech.stuhfl.STUHFL_T_SerialNumber
  < O Param: human readable board hardware information
sndData - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < I Param: Append tag handle to generic command.
sndData - Variable in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
sndDataBitLength - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < I Param: Size in bits of expected received data.
sndDataBitLength - Variable in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
start() - Method in class com.unitech.lib.htx.protocol.ProtocolHT730
start() - Method in class com.unitech.lib.reader.device.BaseDevice
start() - Method in class com.unitech.lib.reader.protocol.Protocol
start() - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
start(IRunnerListener) - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  Start Gb29768 Inventory process depending on the current inventory and Gb29768 configuration
start(IRunnerListener) - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  Start Gen2 Inventory process depending on the current inventory and Gb29768 configuration
startQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The start Q value
startQ - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
  < I/O Param: Flag to enable automatic Q adaption
startUp(String, String) - Static method in class com.unitech.lib.util.diagnotics.UniLog
startUp(String, String, UniLog.ILoggingCheckPermissionListener) - Static method in class com.unitech.lib.util.diagnotics.UniLog
startUp(int, String, String) - Static method in class com.unitech.lib.util.diagnotics.UniLog
startUp(int, String, String, UniLog.ILoggingCheckPermissionListener) - Static method in class com.unitech.lib.util.diagnotics.UniLog
StateChangedEventArgs(BaseReader, ConnectState, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.StateChangedEventArgs
statistics - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  < I Param: Defines Inventory data report scheme.
statistics - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  < I Param: Defines Inventory data report scheme (Round/Slot, HeartBeat).
stop() - Method in class com.unitech.lib.htx.protocol.ProtocolHT730
stop() - Method in class com.unitech.lib.reader.device.BaseDevice
stop() - Method in class com.unitech.lib.reader.protocol.Protocol
stop() - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
stop() - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to stop the operation being performed.
stop() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
stop() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
stop() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  Stop actual runnning Gb29768 Inventory process
stop() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  Stop actual running Gen2 Inventory process
stopAction() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
stopAction() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
StringUtil - Class in com.unitech.lib.util.diagnotics
StringUtil() - Constructor for class com.unitech.lib.util.diagnotics.StringUtil
STUHFL - Class in com.unitech.stuhfl
STUHFL_D_DEFAULT_FREQUENCY - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_FREQUENCY_MAX_VALUE - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_GEN2_GENERIC_CMD_MAX_RCV_DATA_BYTES - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_GEN2_GENERIC_CMD_MAX_SND_DATA_BYTES - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_GEN2_MAXQ - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_GEN2_TIMING_USE_DEFAULT_T4MIN - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_INVENTORYREPORT_HEART_BEAT_DURATION_MS - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_LOG_LEVEL_COUNT - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_ANTENNA - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_BLOCKWRITE_DATA_LEN - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_EPC_LENGTH - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_FREQUENCY - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_PC_LENGTH - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_READ_DATA_LEN - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_REGISTERS - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_TAG_LIST_SIZE - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_TID_LENGTH - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_TIME_LENGTH - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_VERSION_INFO_LENGTH - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_WRITE_DATA_LEN - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_MAX_XPC_LENGTH - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_NB_C_VALUES - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_PASSWORD_LEN - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_RESET_DEFAULT_ALL_FREQS - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_D_TUNING_ALGO_ENABLE_FPD - Static variable in class com.unitech.stuhflBridge.NativeDefines
STUHFL_E - Class in com.unitech.stuhfl
STUHFL_E() - Constructor for class com.unitech.stuhfl.STUHFL_E
STUHFL_E.ANTENNA_POWER_MODE - Enum in com.unitech.stuhfl
STUHFL_E.CONTINUOUS_MODULATION_MODE - Enum in com.unitech.stuhfl
STUHFL_E.FREQUENCY_HOP_MODE - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_ACTION_ATTRIBUTE - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_ACTION_SECMODE - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_AREA - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_BLF - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_CODING - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_CONDITION - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_CONFIGURATION - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_RULE - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_SESSION - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_SORT_MODE - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_SORT_TARGET - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_TARGET - Enum in com.unitech.stuhfl
STUHFL_E.GB29768_TC - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_BLF - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_CODING - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_GENERIC_CMD - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_MEMORY_BANK - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_SELECT_MODE - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_SELECT_TARGET - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_SESSION - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_TARGET - Enum in com.unitech.stuhfl
STUHFL_E.GEN2_TARI - Enum in com.unitech.stuhfl
STUHFL_E.HW_ID - Enum in com.unitech.stuhfl
STUHFL_E.POWER - Enum in com.unitech.stuhfl
STUHFL_E.PROFILE - Enum in com.unitech.stuhfl
STUHFL_E.REPORT_OPTION - Enum in com.unitech.stuhfl
STUHFL_E.RET_CODE - Enum in com.unitech.stuhfl
STUHFL_E.RSSI_MODE - Enum in com.unitech.stuhfl
STUHFL_E.RWD_CFG_ID - Enum in com.unitech.stuhfl
STUHFL_E.TREXT_LEAD - Enum in com.unitech.stuhfl
STUHFL_E.TUNER_CAP - Enum in com.unitech.stuhfl
STUHFL_E.TUNING_ALGO - Enum in com.unitech.stuhfl
STUHFL_E.TUNING_STATUS - Enum in com.unitech.stuhfl
STUHFL_E.USED_ANTENNA - Enum in com.unitech.stuhfl
STUHFL_T_AutoOffTime - Class in com.unitech.stuhfl
STUHFL_T_AutoOffTime() - Constructor for class com.unitech.stuhfl.STUHFL_T_AutoOffTime
STUHFL_T_BatteryInfo - Class in com.unitech.stuhfl
STUHFL_T_BatteryInfo() - Constructor for class com.unitech.stuhfl.STUHFL_T_BatteryInfo
STUHFL_T_Beeper - Class in com.unitech.stuhfl
STUHFL_T_Beeper() - Constructor for class com.unitech.stuhfl.STUHFL_T_Beeper
STUHFL_T_BTMAC - Class in com.unitech.stuhfl
STUHFL_T_BTMAC() - Constructor for class com.unitech.stuhfl.STUHFL_T_BTMAC
STUHFL_T_DataFormat - Class in com.unitech.stuhfl
STUHFL_T_DataFormat() - Constructor for class com.unitech.stuhfl.STUHFL_T_DataFormat
STUHFL_T_DataInfo - Class in com.unitech.stuhfl
STUHFL_T_DataInfo() - Constructor for class com.unitech.stuhfl.STUHFL_T_DataInfo
STUHFL_T_DataRange - Class in com.unitech.stuhfl
STUHFL_T_DataRange() - Constructor for class com.unitech.stuhfl.STUHFL_T_DataRange
STUHFL_T_DataTerminator - Class in com.unitech.stuhfl
STUHFL_T_DataTerminator() - Constructor for class com.unitech.stuhfl.STUHFL_T_DataTerminator
STUHFL_T_FactoryReset - Class in com.unitech.stuhfl
STUHFL_T_FactoryReset() - Constructor for class com.unitech.stuhfl.STUHFL_T_FactoryReset
STUHFL_T_FindDevice - Class in com.unitech.stuhfl
STUHFL_T_FindDevice() - Constructor for class com.unitech.stuhfl.STUHFL_T_FindDevice
STUHFL_T_Gb29768_Erase - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Erase(STUHFL_T_Gb29768_Erase) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Erase
  < I Param: Password.
STUHFL_T_Gb29768_Erase(STUHFL_E.GB29768_AREA, byte, long, byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Erase
STUHFL_T_Gb29768_Erase() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Erase
STUHFL_T_Gb29768_Inventory - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Inventory(STUHFL_T_Gb29768_Inventory) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
STUHFL_T_Gb29768_Inventory() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
STUHFL_T_Gb29768_Inventory(long) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
STUHFL_T_Gb29768_Inventory(STUHFL_E.RSSI_MODE, long, int, STUHFL_E.REPORT_OPTION) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
STUHFL_T_Gb29768_Kill - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Kill(STUHFL_T_Gb29768_Kill) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
  < O Param: Tag reply.
STUHFL_T_Gb29768_Kill(byte[], short, short, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
STUHFL_T_Gb29768_Kill() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
STUHFL_T_Gb29768_Lock - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Lock(STUHFL_T_Gb29768_Lock) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
  < I Param: Password.
STUHFL_T_Gb29768_Lock(STUHFL_E.GB29768_AREA, STUHFL_E.GB29768_CONFIGURATION, STUHFL_E.GB29768_ACTION_ATTRIBUTE, byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
STUHFL_T_Gb29768_Lock() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
STUHFL_T_Gb29768_Read - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Read(STUHFL_T_Gb29768_Read) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Read
  < O Param: Read data.
STUHFL_T_Gb29768_Read(long, short, short, byte[], byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Read
STUHFL_T_Gb29768_Read() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Read
STUHFL_T_Gb29768_Sort - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Sort(STUHFL_T_Gb29768_Sort) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: Mask length (in bits).
STUHFL_T_Gb29768_Sort(STUHFL_E.GB29768_SORT_MODE, STUHFL_E.GB29768_SORT_TARGET, STUHFL_E.GB29768_RULE, STUHFL_E.GB29768_AREA, byte[], long, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
STUHFL_T_Gb29768_Sort() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
STUHFL_T_Gb29768_Write - Class in com.unitech.stuhfl
STUHFL_T_Gb29768_Write(STUHFL_T_Gb29768_Write) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
  < O Param: Tag reply.
STUHFL_T_Gb29768_Write(long, short, byte[], byte[], short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
STUHFL_T_Gb29768_Write() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
STUHFL_T_Gen2_BlockWrite - Class in com.unitech.stuhfl
STUHFL_T_Gen2_BlockWrite(STUHFL_T_Gen2_BlockWrite) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
  < O Param: Tag reply.
STUHFL_T_Gen2_BlockWrite(long, byte[], STUHFL_E.GEN2_MEMORY_BANK, byte[], short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
STUHFL_T_Gen2_BlockWrite() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
STUHFL_T_Gen2_GenericCmd - Class in com.unitech.stuhfl
STUHFL_T_Gen2_GenericCmd(STUHFL_T_Gen2_GenericCmd) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < O Param: Data received from Tag.
STUHFL_T_Gen2_GenericCmd(byte[], STUHFL_E.GEN2_GENERIC_CMD, short, int, int, boolean, byte[], byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
STUHFL_T_Gen2_GenericCmd() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
STUHFL_T_Gen2_Inventory - Class in com.unitech.stuhfl
STUHFL_T_Gen2_Inventory(STUHFL_T_Gen2_Inventory) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
STUHFL_T_Gen2_Inventory(STUHFL_E.RSSI_MODE, long, int, STUHFL_E.REPORT_OPTION) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
STUHFL_T_Gen2_Inventory() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
STUHFL_T_Gen2_Inventory(long) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
STUHFL_T_Gen2_Kill - Class in com.unitech.stuhfl
STUHFL_T_Gen2_Kill(STUHFL_T_Gen2_Kill) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
  < O Param: Tag reply.
STUHFL_T_Gen2_Kill(byte[], short, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
STUHFL_T_Gen2_Kill() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
STUHFL_T_Gen2_Lock - Class in com.unitech.stuhfl
STUHFL_T_Gen2_Lock(STUHFL_T_Gen2_Lock) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
  < O Param: Tag reply.
STUHFL_T_Gen2_Lock(byte[], byte[], short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
STUHFL_T_Gen2_Lock() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
STUHFL_T_Gen2_Read - Class in com.unitech.stuhfl
STUHFL_T_Gen2_Read(STUHFL_T_Gen2_Read) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Read
  < O Param: Read data.
STUHFL_T_Gen2_Read(long, STUHFL_E.GEN2_MEMORY_BANK, short, byte[], byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Read
STUHFL_T_Gen2_Read() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Read
STUHFL_T_Gen2_Select - Class in com.unitech.stuhfl
STUHFL_T_Gen2_Select(STUHFL_T_Gen2_Select) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: Truncate enabling.
STUHFL_T_Gen2_Select(STUHFL_E.GEN2_SELECT_MODE, STUHFL_E.GEN2_SELECT_TARGET, short, STUHFL_E.GEN2_MEMORY_BANK, byte[], long, short, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Select
STUHFL_T_Gen2_Select() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Select
STUHFL_T_Gen2_Write - Class in com.unitech.stuhfl
STUHFL_T_Gen2_Write(STUHFL_T_Gen2_Write) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Write
  < O Param: Tag reply.
STUHFL_T_Gen2_Write(long, STUHFL_E.GEN2_MEMORY_BANK, byte[], byte[], short) - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Write
STUHFL_T_Gen2_Write() - Constructor for class com.unitech.stuhfl.STUHFL_T_Gen2_Write
STUHFL_T_InventoryStatistics() - Constructor for class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
STUHFL_T_InventoryStatistics(IRunnerListener.STUHFL_T_InventoryStatistics) - Constructor for class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
STUHFL_T_InventoryStatistics(long, long, short, short, byte, short, long, int, long, long, long, long, long, long, long, long) - Constructor for class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
STUHFL_T_InventoryTag() - Constructor for class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
STUHFL_T_InventoryTag(IRunnerListener.STUHFL_T_InventoryTag) - Constructor for class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
STUHFL_T_InventoryTag(long, short, short, short, short, byte, byte, byte[], byte[], byte[], byte[]) - Constructor for class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
STUHFL_T_Model - Class in com.unitech.stuhfl
STUHFL_T_Model() - Constructor for class com.unitech.stuhfl.STUHFL_T_Model
STUHFL_T_OperatingMode - Class in com.unitech.stuhfl
STUHFL_T_OperatingMode() - Constructor for class com.unitech.stuhfl.STUHFL_T_OperatingMode
STUHFL_T_ReadMode - Class in com.unitech.stuhfl
STUHFL_T_ReadMode() - Constructor for class com.unitech.stuhfl.STUHFL_T_ReadMode
STUHFL_T_SerialNumber - Class in com.unitech.stuhfl
STUHFL_T_SerialNumber(STUHFL_T_SerialNumber) - Constructor for class com.unitech.stuhfl.STUHFL_T_SerialNumber
STUHFL_T_SerialNumber() - Constructor for class com.unitech.stuhfl.STUHFL_T_SerialNumber
STUHFL_T_SKU - Class in com.unitech.stuhfl
STUHFL_T_SKU() - Constructor for class com.unitech.stuhfl.STUHFL_T_SKU
STUHFL_T_ST25RU3993_AntennaPower - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_AntennaPower(STUHFL_T_ST25RU3993_AntennaPower) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
  < I Param: Frequency to be used
STUHFL_T_ST25RU3993_AntennaPower(STUHFL_E.ANTENNA_POWER_MODE, int, long) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
STUHFL_T_ST25RU3993_AntennaPower() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
STUHFL_T_ST25RU3993_Caps(short, short, short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_Caps
STUHFL_T_ST25RU3993_Caps() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_Caps
STUHFL_T_ST25RU3993_Caps(short, short, short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
STUHFL_T_ST25RU3993_Caps() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
STUHFL_T_ST25RU3993_ChannelItem(long, short, short, short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem
STUHFL_T_ST25RU3993_ChannelList - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_ChannelList(STUHFL_T_ST25RU3993_ChannelList) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  < I/O Param: Tuning capacitors for each frequency
STUHFL_T_ST25RU3993_ChannelList(STUHFL_E.USED_ANTENNA, boolean, short, List<BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem>) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
STUHFL_T_ST25RU3993_ChannelList() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
STUHFL_T_ST25RU3993_ChannelList(STUHFL_E.PROFILE) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
STUHFL_T_ST25RU3993_FreqContinuousModulation - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_FreqContinuousModulation(STUHFL_T_ST25RU3993_FreqContinuousModulation) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
  < I Param: Modulation mode
STUHFL_T_ST25RU3993_FreqContinuousModulation(long, boolean, int, STUHFL_E.CONTINUOUS_MODULATION_MODE) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
STUHFL_T_ST25RU3993_FreqContinuousModulation() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
STUHFL_T_ST25RU3993_FreqHop - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_FreqHop(STUHFL_T_ST25RU3993_FreqHop) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
  < I/O Param: Hopping mode
STUHFL_T_ST25RU3993_FreqHop(int, int, STUHFL_E.FREQUENCY_HOP_MODE) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
STUHFL_T_ST25RU3993_FreqHop() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
STUHFL_T_ST25RU3993_FreqLBT - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_FreqLBT(STUHFL_T_ST25RU3993_FreqLBT) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
  < I/O Param: Flag to wheter LBT check shall be skipped at all
STUHFL_T_ST25RU3993_FreqLBT(int, int, short, boolean) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
STUHFL_T_ST25RU3993_FreqLBT() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
STUHFL_T_ST25RU3993_FreqProfile - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_FreqProfile() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqProfile
STUHFL_T_ST25RU3993_FreqReflectedPowerInfo - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_FreqReflectedPowerInfo(STUHFL_T_ST25RU3993_FreqReflectedPowerInfo) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
  < O Param: Reflected Q
STUHFL_T_ST25RU3993_FreqReflectedPowerInfo(long, boolean, short, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
STUHFL_T_ST25RU3993_FreqReflectedPowerInfo() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
STUHFL_T_ST25RU3993_FreqRssi - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_FreqRssi(STUHFL_T_ST25RU3993_FreqRssi) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
  < O Param: Q parameter of logarithmic scaled RSSI
STUHFL_T_ST25RU3993_FreqRssi(long, short, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
STUHFL_T_ST25RU3993_FreqRssi() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
STUHFL_T_ST25RU3993_Gb29768_FilterCalibration - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_FilterCalibration(STUHFL_T_ST25RU3993_Gb29768_FilterCalibration) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
  < I/O Param: Low pass filter value.
STUHFL_T_ST25RU3993_Gb29768_FilterCalibration(STUHFL_E.GB29768_BLF, STUHFL_E.GB29768_CODING, byte, byte) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
STUHFL_T_ST25RU3993_Gb29768_FilterCalibration() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg(STUHFL_T_ST25RU3993_Gb29768_InventoryCfg) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg(STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning, STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AdaptiveSensitivity, STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams, STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision, STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Option) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AdaptiveSensitivity - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Option - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg(STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
  < I/O Param: Refernce time of forward link: STUHFL_D_GB29768_TC_12_5, STUHFL_D_GB29768_TC_6_25
STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg(STUHFL_E.TREXT_LEAD, STUHFL_E.GB29768_BLF, STUHFL_E.GB29768_CODING, STUHFL_E.GB29768_TC) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
STUHFL_T_ST25RU3993_Gb29768_RxFilter - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gb29768_RxFilter(STUHFL_T_ST25RU3993_Gb29768_RxFilter) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
  < I/O Param: RX filter value
STUHFL_T_ST25RU3993_Gb29768_RxFilter(STUHFL_E.GB29768_BLF, STUHFL_E.GB29768_CODING, byte) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
STUHFL_T_ST25RU3993_Gb29768_RxFilter() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
STUHFL_T_ST25RU3993_Gen2_FilterCalibration - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_FilterCalibration(STUHFL_T_ST25RU3993_Gen2_FilterCalibration) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
  < I/O Param: Low pass filter value.
STUHFL_T_ST25RU3993_Gen2_FilterCalibration(STUHFL_E.GEN2_BLF, STUHFL_E.GEN2_CODING, byte, byte) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
STUHFL_T_ST25RU3993_Gen2_FilterCalibration() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
STUHFL_T_ST25RU3993_Gen2_InventoryCfg - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_InventoryCfg(STUHFL_T_ST25RU3993_Gen2_InventoryCfg) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
STUHFL_T_ST25RU3993_Gen2_InventoryCfg(STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Option, STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision, STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning, STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams, STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AdaptiveSensitivity) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
STUHFL_T_ST25RU3993_Gen2_InventoryCfg() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AdaptiveSensitivity - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Option - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_InventoryCfg.QueryParams - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_ProtocolCfg - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_ProtocolCfg(STUHFL_T_ST25RU3993_Gen2_ProtocolCfg) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
  < I/O Param: Usage of short or long preamble: true if the preamble is long, i.e. with pilot tone
STUHFL_T_ST25RU3993_Gen2_ProtocolCfg(STUHFL_E.GEN2_TARI, STUHFL_E.GEN2_BLF, STUHFL_E.GEN2_CODING, STUHFL_E.TREXT_LEAD) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
STUHFL_T_ST25RU3993_Gen2_ProtocolCfg() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
STUHFL_T_ST25RU3993_Gen2_RxFilter - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_RxFilter(STUHFL_T_ST25RU3993_Gen2_RxFilter) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
  < I/O Param: RX filter value
STUHFL_T_ST25RU3993_Gen2_RxFilter(STUHFL_E.GEN2_BLF, STUHFL_E.GEN2_CODING, byte) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
STUHFL_T_ST25RU3993_Gen2_RxFilter() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
STUHFL_T_ST25RU3993_Gen2_Timings - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Gen2_Timings(STUHFL_T_ST25RU3993_Gen2_Timings) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
  < I/O Param: T4 minimum value in us.
STUHFL_T_ST25RU3993_Gen2_Timings(int) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
STUHFL_T_ST25RU3993_Gen2_Timings() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
STUHFL_T_ST25RU3993_PowerAmplifierCfg - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_PowerAmplifierCfg(STUHFL_T_ST25RU3993_PowerAmplifierCfg) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
  < I/O Param: Use external Power Amplifier
STUHFL_T_ST25RU3993_PowerAmplifierCfg(boolean) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
STUHFL_T_ST25RU3993_PowerAmplifierCfg() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
STUHFL_T_ST25RU3993_Register - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_Register(STUHFL_T_ST25RU3993_Register) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
  < I/O Param: Register data
STUHFL_T_ST25RU3993_Register(short, byte) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
STUHFL_T_ST25RU3993_Register(short) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
STUHFL_T_ST25RU3993_Register() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
STUHFL_T_ST25RU3993_RegisterMultiple - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_RegisterMultiple(STUHFL_T_ST25RU3993_RegisterMultiple) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
  < I/O Param: Multiple Register data
STUHFL_T_ST25RU3993_RegisterMultiple(short[], byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
STUHFL_T_ST25RU3993_RegisterMultiple(short[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
STUHFL_T_ST25RU3993_RegisterMultiple() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
STUHFL_T_ST25RU3993_RwdConfig - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_RwdConfig(STUHFL_T_ST25RU3993_RwdConfig) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
  < I/O Param: Corresponding configuration value
STUHFL_T_ST25RU3993_RwdConfig(STUHFL_E.RWD_CFG_ID, int) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
STUHFL_T_ST25RU3993_RwdConfig() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
STUHFL_T_ST25RU3993_TuningCaps - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_TuningCaps(STUHFL_T_ST25RU3993_TuningCaps) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
  < I/O Param: Tuning caps at antenna
STUHFL_T_ST25RU3993_TuningCaps(STUHFL_E.USED_ANTENNA, byte, BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
STUHFL_T_ST25RU3993_TuningCaps() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
STUHFL_T_ST25RU3993_TxRxCfg - Class in com.unitech.stuhfl
STUHFL_T_ST25RU3993_TxRxCfg(STUHFL_T_ST25RU3993_TxRxCfg) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
  < rfu
STUHFL_T_ST25RU3993_TxRxCfg(byte, byte, STUHFL_E.USED_ANTENNA, int, short) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
STUHFL_T_ST25RU3993_TxRxCfg() - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
STUHFL_T_Temperature - Class in com.unitech.stuhfl
STUHFL_T_Temperature() - Constructor for class com.unitech.stuhfl.STUHFL_T_Temperature
STUHFL_T_Time - Class in com.unitech.stuhfl
STUHFL_T_Time(STUHFL_T_Time) - Constructor for class com.unitech.stuhfl.STUHFL_T_Time
STUHFL_T_Time() - Constructor for class com.unitech.stuhfl.STUHFL_T_Time
STUHFL_T_VersionBoard - Class in com.unitech.stuhfl
STUHFL_T_VersionBoard(STUHFL_T_VersionBoard) - Constructor for class com.unitech.stuhfl.STUHFL_T_VersionBoard
  < O Param: Build version board HW
STUHFL_T_VersionBoard() - Constructor for class com.unitech.stuhfl.STUHFL_T_VersionBoard
STUHFL_T_VersionBoardInfo - Class in com.unitech.stuhfl
STUHFL_T_VersionBoardInfo(STUHFL_T_VersionBoardInfo) - Constructor for class com.unitech.stuhfl.STUHFL_T_VersionBoardInfo
  < O Param: human readable board hardware information
STUHFL_T_VersionBoardInfo() - Constructor for class com.unitech.stuhfl.STUHFL_T_VersionBoardInfo
STUHFL_T_VersionLib - Class in com.unitech.stuhfl
STUHFL_T_VersionLib(STUHFL_T_VersionLib) - Constructor for class com.unitech.stuhfl.STUHFL_T_VersionLib
  < O Param: Nano version
STUHFL_T_VersionLib() - Constructor for class com.unitech.stuhfl.STUHFL_T_VersionLib
STUHFL_T_Vibrator - Class in com.unitech.stuhfl
STUHFL_T_Vibrator() - Constructor for class com.unitech.stuhfl.STUHFL_T_Vibrator
SubCommandType - Enum in com.unitech.lib.rpx.types
  The SubCommandType enumeration represents the sub command type of device associated with the SDK.
sw - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoardInfo
SysUtil - Class in com.unitech.lib.util
SysUtil() - Constructor for class com.unitech.lib.util.SysUtil

A B C D E F G H I K L M N O P Q R S T U V W X _