A B C D E F G H I K L M N O P Q R S T U V W X _

## E

e(String, String, Object...) - Static method in class com.unitech.lib.util.diagnotics.UniLog
e(String, Throwable, String, Object...) - Static method in class com.unitech.lib.util.diagnotics.UniLog
e(String, String) - Static method in class com.unitech.lib.util.diagnotics.UniLog
emptySlotCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Number of detected tags.
enable - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AdaptiveSensitivity
  < I/O Param: Adaptive sensitivity interval (in inventory rounds)
enable - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AdaptiveSensitivity
enableContMod - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
  < I Param: Frequency to be used for continuouse modulation
enableContMod - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
encoding - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Encoding setting, only for RP902
Encoding - Enum in com.unitech.lib.uhf.types
  The Encoding enumeration represents the miller encoding by which the RFID UHF module inventories the TAG.
endThreshold - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision
enqueue(byte[]) - Method in class com.unitech.lib.util.collections.ByteQueue
enqueue(byte[], int) - Method in class com.unitech.lib.util.collections.ByteQueue
enqueue(byte[], int, int) - Method in class com.unitech.lib.util.collections.ByteQueue
enterBootloader() - Method in class com.unitech.stuhfl.STUHFL
  Shutdown FW and enter STM32 ROM bootloader of EVAL board.
epc() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access tag's EPC value.
epc() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's EPC value.
epc - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Tag XPC.
EPCMaskParam - Class in com.unitech.lib.uhf.params
  The EPCMaskParam class stores information about the EPC Mask when the RFID UHF module sets or returns an EPC Mask.
EPCMaskParam() - Constructor for class com.unitech.lib.uhf.params.EPCMaskParam
  Creates an instance of the EPCMaskParam class.
EPCMaskParam(int, int, String) - Constructor for class com.unitech.lib.uhf.params.EPCMaskParam
  Creates an instance of the EPCMaskParam class.
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Erase.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Kill.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Lock.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Read.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gb29768_Write.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_BlockWrite.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_Kill.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_Lock.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_Read.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Gen2_Write.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_AntennaPower.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqProfile.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqRssi.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_FilterCalibration.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_ProtocolCfg.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_RxFilter.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_FilterCalibration.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_ProtocolCfg.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_RxFilter.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_Timings.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_PowerAmplifierCfg.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_RwdConfig.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
equals(Object) - Method in class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields
equals(Object) - Method in class com.unitech.stuhflBridge.BR_Version.Fields
ERROR - Static variable in class com.unitech.lib.util.diagnotics.UniLog
execute() - Method in class com.unitech.stuhfl.STUHFL_T_FactoryReset
  Execute the factory reset command.
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Erase
  Perform Gb29768 erase command to erase data in transponders.
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  Perform Gb29768 Inventory depending on the current inventory and Gb29768 configuration All public data fields must be prepared upfront.
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
  Perform Gb29768 Kill command to kill transponders.
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
  Perform Gb29768 Lock command to lock transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Read
  Perform Gb29768 Read command to read from the Gb29768 transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  Perform Gb29768 Sort command to select or filter transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gb29768_Write
  Perform Gb29768 Write command to write data to Gb29768 transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_BlockWrite
  Perform Gen2 Block Write command to write block data to Gen2 transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  Perform generic Gen2 bit exchange
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  Perform Gen2 Inventory depending on the current inventory and Gen2 configuration All public data fields must be prepared upfront.
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
  Perform Gen2 Kill command to kill transponders.
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Lock
  Perform Gen2 Lock command to lock transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Read
  Perform Gen2 Read command to read from the Gen2 transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  Perform Gen2 Select command to select or filter transponders
execute() - Method in class com.unitech.stuhfl.STUHFL_T_Gen2_Write
  Perform Gen2 Write command to write data to Gen2 transponders
expectedRcvDataBitLength - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < I Param: Tag response timeout.
expectedRcvDataBitLength - Variable in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
external - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
external - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_PowerAmplifierCfg.Fields

A B C D E F G H I K L M N O P Q R S T U V W X _