A B C D E F G H I K L M N O P Q R S T U V W X _

## A

action - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
  < I Param: Configure attribute and security mode of storage area.
action - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Select
  < I Param: indicates whether the select modifies a tag's SL flag or its inventoried flag.
action - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Lock.Fields
action - Variable in class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
ActionChangedEventArgs(BaseReader, ResultCode, ActionState, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.ActionChangedEventArgs
ActionState - Enum in com.unitech.lib.types
  ActionState indicates the current operation status of the device.
ActionType - Enum in com.unitech.lib.types
  ActionType indicates the operation type of the device.
actionType() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access action type.
ActionUtil - Class in com.unitech.lib.util
ActionUtil() - Constructor for class com.unitech.lib.util.ActionUtil
activeChannelListIdx - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  < I Param: Set/Get channel list to/from persistent flash memory
activeChannelListIdx - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.Fields
adaptiveQ - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
adaptiveSensitivity - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
AdaptiveSensitivity(int, boolean) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AdaptiveSensitivity
  < I/O Param: Flag to enable automatic sensitivity adjustment
adaptiveSensitivity - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
AdaptiveSensitivity(boolean, int) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AdaptiveSensitivity
  < I/O Param: Adaptive sensitivity interval (in inventory rounds)
adaptiveSensitivity_enable - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
adaptiveSensitivity_enable - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
adaptiveSensitivity_interval - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
adaptiveSensitivity_interval - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
adc - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Current Frequency.
add(long) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Add item to local channelList.
add(long, short, short, short) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Add item to local channelList.
addListener(IReaderEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Adds a Listener to receive events on an instance of the BaseReader class.
addListener(IReaderEventListener) - Method in class com.unitech.lib.reader.event.ReaderEventManager
addListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.BaseUHF
  Adds an event handler to receive events that occur in the instance.
addListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
addr - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
addr - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
addr - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
addrMultiple - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
agc - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Antenna at which Tag was detected.
algorithm - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Q algorithm setting
algorithm - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning
  < I/O Param: Deviation level for retuning in percentage
algorithm - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning
  < I/O Param: Deviation of (I^2+Q^2) to trigger retuning
AlgorithmType - Enum in com.unitech.lib.uhf.types
  The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
alternateAntennaInterval - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
  < I/O Param: Antenna to be used
alternateAntennaInterval - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields
antenna() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the antenna at which tag was detected.
antenna - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
antenna - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
antenna - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.Fields
antenna - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.Fields
antenna - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Tag detection time stamp.
antiCollision - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
Anticollision(int, int, int) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision
  < I Param: GBT anticollision CIN threshold parameter.
antiCollision - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
Anticollision(boolean, byte, byte, byte, byte, byte[], byte[]) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
  < I/O Param: Q algorithm C1 values for each Q
antiCollision_adaptiveQ - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
antiCollision_C1 - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
antiCollision_C2 - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
antiCollision_ccnThreshold - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
antiCollision_cinThreshold - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
antiCollision_endThreshold - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
antiCollision_maxQ - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
antiCollision_minQ - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
antiCollision_options - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
antiCollision_startQ - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
appendRN16 - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < I Param: Size in bits of data sent to Tag.
appendRN16 - Variable in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
applyTunerSetting - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
  < I Param: Frequency to be used for the measurement
applyTunerSetting - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
assertAction() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
assertAction() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
assertModule() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
assertModule() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
assertPassword(String) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
assertPassword(String) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
assertPassword(String) - Static method in class com.unitech.lib.util.LibUtil
assertSelectMask(int) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
assertSelectMask(int) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
autoAck - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Option
  < I Param: Fast Inventory enabling.
autoOffTime - Variable in class com.unitech.stuhfl.STUHFL_T_AutoOffTime
autoTuning - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
AutoTuning(int, short, STUHFL_E.TUNING_ALGO, boolean) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning
  < I/O Param: Algorithm used for automatic (re)tuning.
autoTuning - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
AutoTuning(int, int, STUHFL_E.TUNING_ALGO, boolean) - Constructor for class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning
  < I/O Param: Perfom false positive check during tuning
autoTuning_algorithm - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
autoTuning_algorithm - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
autoTuning_falsePositiveDetection - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
autoTuning_falsePositiveDetection - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
autoTuning_interval - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
autoTuning_interval - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
autoTuning_level - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
autoTuning_level - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
available() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the length of data that can be read with the read method.
available() - Method in class com.unitech.lib.transport.TransportBluetooth
available() - Method in class com.unitech.lib.transport.TransportUART

A B C D E F G H I K L M N O P Q R S T U V W X _