A B C D E F G H I K L M N O P Q R S T U V W X _

## L

L1 - Static variable in class com.unitech.lib.util.diagnotics.UniLog
L2 - Static variable in class com.unitech.lib.util.diagnotics.UniLog
L3 - Static variable in class com.unitech.lib.util.diagnotics.UniLog
L4 - Static variable in class com.unitech.lib.util.diagnotics.UniLog
length - Variable in class com.unitech.lib.reader.params.DataRange
level - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning
  < I/O Param: Auto tuning check interval (in inventory rounds)
level - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning
  < I/O Param: Auto tuning check interval (in inventory rounds)
LibBridge - Class in com.unitech.stuhflBridge
LibBridge() - Constructor for class com.unitech.stuhflBridge.LibBridge
LibUtil - Class in com.unitech.lib.util
LibUtil() - Constructor for class com.unitech.lib.util.LibUtil
listen() - Method in class com.unitech.lib.reader.BaseReader
  Allows the BaseReader class to wait for connection until the connection is made from the device.
listen() - Method in class com.unitech.lib.transport.BaseTransport
  An instance of the BaseTransport class waits for the device to connect.
listen() - Method in class com.unitech.lib.transport.TransportBluetooth
listen() - Method in class com.unitech.lib.transport.TransportUART
listener - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
listener - Variable in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
listeningTime - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
listeningTime - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
lock(Lock6cParam, String) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
lock(Lock6cParam, String) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
lock6c(Lock6cParam, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to lock or unlock the RFID UHF tags of the ISO18000-6c Gen2 standard.
lock6c(Lock6cParam, String) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
lock6c(Lock6cParam, String) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
Lock6cParam - Class in com.unitech.lib.uhf.params
  The Lock6cParam class is used to pass information that the RFID UHF's Lock command performs.
Lock6cParam() - Constructor for class com.unitech.lib.uhf.params.Lock6cParam
  Creates an instance of the Lock6cParam class.
Lock6cParam(LockState, LockState, LockState, LockState, LockState) - Constructor for class com.unitech.lib.uhf.params.Lock6cParam
  Creates an instance of the Lock6cParam class.
LockState - Enum in com.unitech.lib.uhf.types
  The LockState enumeration represents the lock state.
lowPass - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
  < I/O Param: High pass filter value.
lowPass - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
  < I/O Param: High pass filter value.
lowPass - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_FilterCalibration.Fields
lowPass - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_FilterCalibration.Fields

A B C D E F G H I K L M N O P Q R S T U V W X _