A B C D E F G H I K L M N O P Q R S T U V W X _

## R

rcvData - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < I Param: Data being sent to Tag.
rcvData - Variable in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
read(byte[], int) - Method in class com.unitech.lib.htx.protocol.ProtocolHT730
read(byte[], int) - Method in interface com.unitech.lib.protocol.IProtocol
read(byte[], int) - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
read(byte[], int, int) - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
read(byte[], int) - Method in class com.unitech.lib.rpx.RP902Reader
read(byte[], int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[]) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportUART
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportUART
read(byte[], int) - Method in interface com.unitech.stuhflBridge.ISerialStream
ReaderEventManager - Class in com.unitech.lib.reader.event
ReaderEventManager() - Constructor for class com.unitech.lib.reader.event.ReaderEventManager
ReaderEventManager.ActionChangedEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.BatteryStateEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.KeyChangedEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.NotificationStateEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.StateChangedEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.TemperatureStateEventArgs - Class in com.unitech.lib.reader.event
ReaderException - Exception in com.unitech.lib.diagnositics
  The exception class and contain result code
ReaderException(ResultCode) - Constructor for exception com.unitech.lib.diagnositics.ReaderException
readMemory(BankType, int, int, String) - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
readMemory(BankType, int, int, String) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
readMemory6c(BankType, int, int, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to read specific memory of RFID UHF tag of ISO18000-6c Gen2 standard.
readMemory6c(BankType, int, int, String) - Method in class com.unitech.lib.uhf.impinj.UHFRM100
readMemory6c(BankType, int, int, String) - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
ReadMode - Enum in com.unitech.lib.types
  The ReadMode enumeration represents the type of device associated with the SDK.
readTID - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Option
readTID - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Option
  < I Param: Automatic Ack enabling.
reboot() - Method in class com.unitech.stuhfl.STUHFL
  Reboot FW NOTE: This function will never return, as the reboot is triggered immediately
recom - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
  < I Param: RFU.
recom - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Kill
  < I Param: Password.
recom - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Kill.Fields
recommission - Variable in class com.unitech.stuhflBridge.BR_Gen2_Kill.Fields
reflectedI - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
  < I/O Param: flag to apply tuner settings for frequency
reflectedI - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
reflectedQ - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
  < O Param: Reflected I
reflectedQ - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
releaseTicket(long) - Method in class com.unitech.lib.util.ServiceHandler
  Release your working ticket
remove() - Method in class com.unitech.lib.util.collections.ByteQueue
remove(long) - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Remove item from local channelList.
removeListener(IReaderEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Removes the Listener that is listening for events on an instance of the BaseReader class.
removeListener(IReaderEventListener) - Method in class com.unitech.lib.reader.event.ReaderEventManager
removeListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.BaseUHF
  Removes an event handler when it no longer needs to receive events raised by the instance.
removeListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
reportOptions - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  < I Param: additional delay that can be added for the each inventory round.
reportOptions - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  < I Param: additional delay that can be added for the each inventory round.
reportOptions - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
reportOptions - Variable in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
resetError() - Method in interface com.unitech.lib.device.IReader
  Use only within the SDK.
resetError() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
Response - Class in com.unitech.lib.protocol
Response(int) - Constructor for class com.unitech.lib.protocol.Response
Response(ResultCode) - Constructor for class com.unitech.lib.protocol.Response
Response(byte[]) - Constructor for class com.unitech.lib.protocol.Response
RESULT_CODE_ERROR - Static variable in class com.unitech.lib.pogo.PogoCtrl
RESULT_CODE_SUCCESS - Static variable in class com.unitech.lib.pogo.PogoCtrl
ResultCode - Enum in com.unitech.lib.types
  The ResultCode enumeration represents failure and behavior results.
resultCode() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access result code.
ResultCodeConvert - Class in com.unitech.lib.util.diagnotics
ResultCodeConvert() - Constructor for class com.unitech.lib.util.diagnotics.ResultCodeConvert
RETRY_COUNT - Static variable in class com.unitech.lib.reader.BaseReader
RFIDConfig - Class in com.unitech.lib.uhf.params
  The RFIDConfig class stores the config of the RFID module.
RFIDConfig() - Constructor for class com.unitech.lib.uhf.params.RFIDConfig
RfidUhfEventManager - Class in com.unitech.lib.uhf.event
RfidUhfEventManager() - Constructor for class com.unitech.lib.uhf.event.RfidUhfEventManager
rfu - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Kill
  < I Param: Password.
rfu - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
  < I/O Param: Time in ms for alternating the antennas when alternating mode is used
rfu - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Kill.Fields
rfu - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields
rfu1 - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem
  < I/O Param: Tuning capacitors for each frequencies
rfu2 - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem
  < rfu
roundCnt - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  < I Param: RSSI mode.
roundCnt - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  < I Param: RSSI mode.
roundCnt - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
roundCnt - Variable in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
roundCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: timestamp of last statistics update.
RP902Reader - Class in com.unitech.lib.rpx
  The RP902Reader class is a class that controls RP902 in connection with unitech's equipment, receives data from RP902, and delivers it to the application program.
RP902Reader(BaseTransport) - Constructor for class com.unitech.lib.rpx.RP902Reader
rssiLinI - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Q part of Tag RSSI log.
rssiLinQ - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Tag RSSI I level.
rssiLogI - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
  < I Param: Frequency for RSSI
rssiLogI - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqRssi.Fields
rssiLogI - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: Tag AGC.
rssiLogMean - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Reader status.
rssiLogQ - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
  < O Param: I parameter of logarithmic scaled RSSI
rssiLogQ - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqRssi.Fields
rssiLogQ - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryTag
  < O Param: I part of Tag RSSI log.
rssiLogThreshold - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
  < I/O Param: Idle time for LBT
rssiLogThreshold - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
rssiMode - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
rssiMode - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
rssiMode - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
rssiMode - Variable in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
rule - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Sort
  < I Param: indicates whether the select modifies a tag's match flag or its inventoried flag.
rule - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
rxCountErrCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Number of Header errors.
rxSensitivity - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
  < I/O Param: Tx output level.
rxSensitivity - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields

A B C D E F G H I K L M N O P Q R S T U V W X _