A B C D E F G H I K L M N O P Q R S T U V W X _

## F

factoryReset() - Method in class com.unitech.lib.htx.HT730Reader
factoryReset() - Method in class com.unitech.lib.reader.BaseReader
  Reset the device to factory default.
factoryReset() - Method in class com.unitech.lib.rpx.device.DeviceRP902
factoryReset() - Method in class com.unitech.lib.rpx.RP902Reader
falsePositiveDetection - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning
  < I/O Param: Algorithm to be used for re-tuning
falsePositiveDetection - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning
  < I/O Param: Algorithm used for automatic (re)tuning
fast - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Option
fastMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The fast mode setting, only for RP902
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_AutoOffTime
  Read the human readable auto off time information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_BatteryInfo
  Read the human readable board software and hardware information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_Beeper
  Read the human readable beeper information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_BTMAC
  Read the human readable device's BT MAC address information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_DataFormat
  Read the human readable data format information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_DataInfo
  Read the human readable data info information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_DataRange
  Read the human readable data info information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_DataTerminator
  Read the human readable data terminator information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_FindDevice
  Read the human readable find device information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_Model
  Read the human readable device's model information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_OperatingMode
  Read the human readable operating mode information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ReadMode
  Read the human readable read mode information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_SerialNumber
  Read the human readable board software and hardware information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_SKU
  Read the human readable SKU information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
  Get current antenna power mode
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Get frequency channel list
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
  Get frequency hopping time configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
  Get actual listen before talk configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqProfile
  Get frequency profile
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
  Measure and get reflected power I/Q values for selected frequency
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
  Get frequency RSSI information from board for selected frequency
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
  Get reader Rx Filter calibration for GB/T 29768 config
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
  Get general GB/T-29768 inventory configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
  Get GB/T-29768 protocol configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
  Set reader Rx Filter configuration for GB/T 29768 config
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
  Get reader Rx Filter calibration for Gen2 config
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
  Get general Gen2 inventory configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
  Get Gen2 protocol configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
  Get reader Rx Filter configuration for Gen2 config
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
  Get Gen2 protocols timings
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
  Get actual power amplifier configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
  Reads one ST25RU3993 register at address and puts the value into the reply to the host.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
  Write multiple ST25RU3993 registers from addresses addr and store content in data
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
  Get reader configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
  Get Cin, Clen and Cout of tuning caps at given antenna
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
  Get TxRx configuration
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_Temperature
  Read the human readable temperature information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_Time
  Read the human readable time information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_VersionBoard
  Read the software and hardware numbers from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_VersionBoardInfo
  Read the human readable board software and hardware information from board.
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_VersionLib
  Retrieve the native library version
fetch() - Method in class com.unitech.stuhfl.STUHFL_T_Vibrator
  Read the human readable vibrator information from board.
Fields(int, short, long, byte[]) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Erase.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Erase.Fields
Fields(int, long, int, int, IRunnerListener, int) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
Fields(byte[], short, short, short) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Kill.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Kill.Fields
Fields(int, int, int, byte[]) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Lock.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Lock.Fields
Fields(long, short, short, byte[], byte[]) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Read.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Read.Fields
Fields(int, int, int, int, byte[], long, short) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Sort.Fields
Fields(long, short, byte[], byte[], short) - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Write.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gb29768_Write.Fields
Fields(long, byte[], int, byte[], short) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_BlockWrite.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_BlockWrite.Fields
Fields(byte[], int, short, int, int, boolean, byte[], byte[]) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
Fields(int, long, int, int, IRunnerListener, int) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
Fields(byte[], short, short) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Kill.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Kill.Fields
Fields(byte[], byte[], short) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Lock.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Lock.Fields
Fields(long, int, short, byte[], byte[]) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Read.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Read.Fields
Fields(int, int, short, int, byte[], long, short, short) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Select.Fields
Fields(long, int, byte[], byte[], short) - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Write.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Gen2_Write.Fields
Fields(int, int, long) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_AntennaPower.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_AntennaPower.Fields
Fields(int, boolean, short, BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem[]) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.Fields
Fields(long, boolean, int, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
Fields(int, int, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqHop.Fields
Fields(int, int, short, boolean) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
Fields(int, int, int, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqProfile.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqProfile.Fields
Fields(long, boolean, short, short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
Fields(long, short, short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqRssi.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_FreqRssi.Fields
Fields(int, int, byte, byte) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_FilterCalibration.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_FilterCalibration.Fields
Fields(int, short, int, boolean, int, boolean, int, int, int, boolean, boolean, int, int, int, boolean) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_InventoryCfg.Fields
Fields(int, int, int, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_ProtocolCfg.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_ProtocolCfg.Fields
Fields(int, int, byte) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_RxFilter.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_RxFilter.Fields
Fields(int, int, byte, byte) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_FilterCalibration.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_FilterCalibration.Fields
Fields(boolean, boolean, boolean, boolean, byte, byte, byte, byte, byte[], byte[], int, int, int, boolean, byte, int, int, boolean, boolean, boolean, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_InventoryCfg.Fields
Fields(int, int, int, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_ProtocolCfg.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_ProtocolCfg.Fields
Fields(int, int, byte) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_RxFilter.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_RxFilter.Fields
Fields(int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_Timings.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_Timings.Fields
Fields(boolean) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_PowerAmplifierCfg.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_PowerAmplifierCfg.Fields
Fields(short[], byte[]) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
Fields(short[]) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
Fields(short, byte) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
Fields(short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_Register.Fields
Fields(int, int) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_RwdConfig.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_RwdConfig.Fields
Fields(int, short, BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.Fields
Fields(byte, byte, int, int, short) - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_ST25RU3993_TxRxCfg.Fields
Fields(byte, byte, byte, byte) - Constructor for class com.unitech.stuhflBridge.BR_Version.Fields
Fields() - Constructor for class com.unitech.stuhflBridge.BR_Version.Fields
FindDevice - Class in com.unitech.lib.reader.params
  The FindDevice class stores information about the find device setting.
FindDevice() - Constructor for class com.unitech.lib.reader.params.FindDevice
FindDevice(FindDeviceMode, int) - Constructor for class com.unitech.lib.reader.params.FindDevice
FindDeviceMode - Enum in com.unitech.lib.types
  The FindDeviceMode enumeration represents the type of device associated with the SDK.
findKey(int) - Method in class com.unitech.lib.util.collections.ByteQueue
findKey(int, int) - Method in class com.unitech.lib.util.collections.ByteQueue
findPattern(byte[]) - Method in class com.unitech.lib.util.collections.ByteQueue
findPattern(int, byte[]) - Method in class com.unitech.lib.util.collections.ByteQueue
Finished(IRunnerListener.STUHFL_T_InventoryStatistics, List<IRunnerListener.STUHFL_T_InventoryTag>) - Method in interface com.unitech.stuhflBridge.IRunnerListener
format - Variable in class com.unitech.stuhfl.STUHFL_T_DataFormat
frequency - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
  < I Param: Timeout before settings will be applied
frequency - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
frequency - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqReflectedPowerInfo
frequency - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqRssi
frequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_AntennaPower.Fields
frequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem
frequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqContinuousModulation.Fields
frequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqReflectedPowerInfo.Fields
frequency - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqRssi.Fields
frequency - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Current Q, may vary if adaptiveQEnable is set.
fw - Variable in class com.unitech.stuhfl.STUHFL_T_VersionBoardInfo
  < O Param: human readable board hardware information

A B C D E F G H I K L M N O P Q R S T U V W X _