A B C D E F G H I K L M N O P Q R S T U V W X _

## C

C1 - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
  < I/O Param: Q algorithm C2 values for each Q
C2 - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.Anticollision
  < I/O Param: Q algorithm options
caps - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
  < I/O Param: Current item index in channel list
caps - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_ChannelItem
  < I/O Param: List of frequencies to be used for hopping
caps - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.Fields
ccnThreshold - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision
  < I Param: GBT anticollision end threshold parameter.
changeSelectEPC(int, String) - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
changeState(ConnectState, Object) - Method in class com.unitech.lib.transport.TransportUART
channelListIdx - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
  < I Param: Antenna to which the ChannelList belongs
channelListIdx - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.Fields
checkBufferSize(int) - Method in class com.unitech.lib.transport.BaseTransport
checkError() - Method in interface com.unitech.lib.device.IReader
  Use only within the SDK.
checkError() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
checkError() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
checkError() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
checkServiceAccessable() - Method in class com.unitech.lib.util.ServiceHandler
cin - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_Caps
cin - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
cinThreshold - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.Anticollision
  < I Param: GBT anticollision CCN threshold parameter.
clear() - Method in class com.unitech.lib.reader.event.ReaderEventManager
clear() - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
clear() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Initializes the values set in the SelectMask6cParam instance.
clear() - Method in class com.unitech.lib.util.collections.ByteQueue
clearBuffer() - Method in class com.unitech.lib.htx.protocol.ProtocolHT730
clearBuffer() - Method in interface com.unitech.lib.protocol.IProtocol
clearBuffer() - Method in class com.unitech.lib.rpx.protocol.ProtocolRP902
clearListener() - Method in class com.unitech.lib.reader.BaseReader
  Removes all listeners registered on an instance of the BaseReader class.
clearListener() - Method in class com.unitech.lib.uhf.BaseUHF
  Removes all event handlers from the instance.
clearSelectMask() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
clearSelectMask() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
clen - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_Caps
  < I/O Param: IN capacitance of tuning table
clen - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
  < I/O Param: IN capacitance of tuning table
clockOff() - Method in class com.unitech.lib.pogo.PogoCtrl
  UART high speed Clock turn Off
clockOn() - Method in class com.unitech.lib.pogo.PogoCtrl
  UART high speed Clock turn ON
cmd - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_GenericCmd
  < I Param: Password.
cmd - Variable in class com.unitech.stuhflBridge.BR_Gen2_GenericCmd.Fields
coding - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
  < I Param: Link Frequency for which HP/LP values shall be applied
coding - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
  < I/O Param: backscatter link frequency factor
coding - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
  < I Param: Link Frequency for which HP/LP values shall be applied
coding - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
  < I Param: Link Frequency for which HP/LP values shall be applied
coding - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
  < I/O Param: backscatter link frequency factor: STUHFL_D_GEN2_BLF_40, ...
coding - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
  < I Param: Link Frequency for which HP/LP values shall be applied
coding - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_FilterCalibration.Fields
coding - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_ProtocolCfg.Fields
coding - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gb29768_RxFilter.Fields
coding - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_FilterCalibration.Fields
coding - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_ProtocolCfg.Fields
coding - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_Gen2_RxFilter.Fields
collisionCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Number of empty slots.
com.unitech.lib.device - package com.unitech.lib.device
com.unitech.lib.diagnositics - package com.unitech.lib.diagnositics
com.unitech.lib.htx - package com.unitech.lib.htx
com.unitech.lib.htx.device - package com.unitech.lib.htx.device
com.unitech.lib.htx.protocol - package com.unitech.lib.htx.protocol
com.unitech.lib.pogo - package com.unitech.lib.pogo
com.unitech.lib.protocol - package com.unitech.lib.protocol
com.unitech.lib.reader - package com.unitech.lib.reader
com.unitech.lib.reader.device - package com.unitech.lib.reader.device
com.unitech.lib.reader.event - package com.unitech.lib.reader.event
com.unitech.lib.reader.params - package com.unitech.lib.reader.params
com.unitech.lib.reader.protocol - package com.unitech.lib.reader.protocol
com.unitech.lib.reader.types - package com.unitech.lib.reader.types
com.unitech.lib.rpx - package com.unitech.lib.rpx
com.unitech.lib.rpx.device - package com.unitech.lib.rpx.device
com.unitech.lib.rpx.protocol - package com.unitech.lib.rpx.protocol
com.unitech.lib.rpx.types - package com.unitech.lib.rpx.types
com.unitech.lib.transport - package com.unitech.lib.transport
com.unitech.lib.transport.event - package com.unitech.lib.transport.event
com.unitech.lib.transport.types - package com.unitech.lib.transport.types
com.unitech.lib.types - package com.unitech.lib.types
com.unitech.lib.uhf - package com.unitech.lib.uhf
com.unitech.lib.uhf.event - package com.unitech.lib.uhf.event
com.unitech.lib.uhf.impinj - package com.unitech.lib.uhf.impinj
com.unitech.lib.uhf.module - package com.unitech.lib.uhf.module
com.unitech.lib.uhf.module.impinj - package com.unitech.lib.uhf.module.impinj
com.unitech.lib.uhf.module.impinj.types - package com.unitech.lib.uhf.module.impinj.types
com.unitech.lib.uhf.module.stseries - package com.unitech.lib.uhf.module.stseries
com.unitech.lib.uhf.params - package com.unitech.lib.uhf.params
com.unitech.lib.uhf.stseries - package com.unitech.lib.uhf.stseries
com.unitech.lib.uhf.types - package com.unitech.lib.uhf.types
com.unitech.lib.util - package com.unitech.lib.util
com.unitech.lib.util.collections - package com.unitech.lib.util.collections
com.unitech.lib.util.diagnotics - package com.unitech.lib.util.diagnotics
com.unitech.stuhfl - package com.unitech.stuhfl
com.unitech.stuhflBridge - package com.unitech.stuhflBridge
combine(STUHFL_E.REPORT_OPTION...) - Static method in enum com.unitech.stuhfl.STUHFL_E.REPORT_OPTION
CommandType - Enum in com.unitech.lib.rpx.types
  The CommandType enumeration represents the command type of device associated with the SDK.
commit() - Method in class com.unitech.stuhfl.STUHFL_T_AutoOffTime
  Set auto off time to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_Beeper
  Set beeper
commit() - Method in class com.unitech.stuhfl.STUHFL_T_DataFormat
  Set data format to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_DataInfo
  Set data info to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_DataRange
  Set data info to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_DataTerminator
  Set data terminator to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_FindDevice
  Set find device setting to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_OperatingMode
  Set operating mode to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ReadMode
  Set read mode to device
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_AntennaPower
  Turn antenna power on or off for test purpose.
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  Get frequency channel list
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqContinuousModulation
  Set continuous modulation configuration and start modulating
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqHop
  Set new frequency hopping time configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
  Set listen before talk configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqProfile
  Set frequency profile
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_FilterCalibration
  Set reader Rx Filter calibration for GB/T 29768 config
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg
  Set general GB/T-29768 inventory configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_ProtocolCfg
  Set GB/T-29768 protocol configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_RxFilter
  Get reader Rx Filter configuration for GB/T 29768 config
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_FilterCalibration
  Set reader Rx Filter calibration for Gen2 config
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg
  Set general Gen2 inventory configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_ProtocolCfg
  Set Gen2 protocol configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_RxFilter
  Set reader Rx Filter configuration for Gen2 config
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_Timings
  Set Gen2 protocols timings
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_PowerAmplifierCfg
  Set power amplifier configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Register
  Writes to ST25RU3993 register at address addr the value.
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RegisterMultiple
  Write multiple ST25RU3993 registers at addresses addr with the values data
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
  Set reader configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TuningCaps
  Set Cin, Clen and Cout of tuning caps at given antenna
commit() - Method in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_TxRxCfg
  Set TxRx configuration
commit() - Method in class com.unitech.stuhfl.STUHFL_T_Time
commit() - Method in class com.unitech.stuhfl.STUHFL_T_Vibrator
  Set vibrator
condition - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.QueryParams
configuration - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Lock
  < I Param: Bank (TagInfo, Coding, Security, User) on which apply the lock.
configuration - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Lock.Fields
connect() - Method in class com.unitech.lib.htx.HT730Reader
connect() - Method in class com.unitech.lib.reader.BaseReader
  An instance of the BaseReader class tries to connect to the configured address
connect() - Method in class com.unitech.lib.transport.BaseTransport
  Attempts to connect to the appliance using an instance of the Transport class.
connect() - Method in class com.unitech.lib.transport.TransportBluetooth
connect() - Method in class com.unitech.lib.transport.TransportUART
connect(String) - Method in class com.unitech.stuhfl.STUHFL
  Connect to ST25RU3993 based evaluation board.
connect(ISerialStream) - Method in class com.unitech.stuhfl.STUHFL
  Connect to ST25RU3993 based evaluation board.
ConnectState - Enum in com.unitech.lib.transport.types
  The ConnectState enumeration indicates the connection status of the BaseTransport instance.
ConnectType - Enum in com.unitech.lib.transport.types
  The ConnectType enumeration indicates which communication method the BaseTransport instance uses in its connection with the appliance.
continuousMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The continuous mode setting
copy(SelectMask6cParam) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Copy the SelectMask6cParam instance.
cout - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.STUHFL_T_ST25RU3993_Caps
  < I/O Param: LEN capacitance of tuning table
cout - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_TuningCaps.STUHFL_T_ST25RU3993_Caps
  < I/O Param: LEN capacitance of tuning table
crcErrCnt - Variable in class com.unitech.stuhflBridge.IRunnerListener.STUHFL_T_InventoryStatistics
  < O Param: Number of Preamble errors.
Cycle(IRunnerListener.STUHFL_T_InventoryStatistics, List<IRunnerListener.STUHFL_T_InventoryTag>) - Method in interface com.unitech.stuhflBridge.IRunnerListener

A B C D E F G H I K L M N O P Q R S T U V W X _