# Constant Field Values

## Contents

- com.unitech.*

## com.unitech.*

- com.unitech.lib.pogo.PogoCtrl
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `BUNDLE_ERROR_CODE` | `"errorCode"`
  `public static final java.lang.String` | `BUNDLE_ERROR_MSG` | `"errorMsg"`
  `public static final java.lang.String` | `BUNDLE_UART_PATH` | `"UART"`
  `public static final int` | `RESULT_CODE_ERROR` | `1`
  `public static final int` | `RESULT_CODE_SUCCESS` | `0`

- com.unitech.lib.reader.BaseReader
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final int` | `DEFAULT_BATTERY_CHECK_INTERVAL` | `3000`
  `protected static final int` | `RETRY_COUNT` | `3`

- com.unitech.lib.reader.device.BaseDevice
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final int` | `INFO` | `7`

- com.unitech.lib.reader.protocol.Protocol
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final int` | `DEBUG` | `2`
  `protected static final int` | `DETAIL` | `9`
  `protected static final int` | `INFO` | `7`
  `protected static final int` | `IO` | `8`

- com.unitech.lib.transport.BaseTransport
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final int` | `DUMP` | `9`
  `protected static final int` | `INFO` | `7`
  `protected static final int` | `IO` | `8`

- com.unitech.lib.uhf.module.BaseModuleUHF
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final int` | `DEFAULT_TIMEOUT` | `3000`

- com.unitech.lib.util.LibUtil
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `DEFAULT_PASSWORD` | `"00000000"`

- com.unitech.lib.util.diagnotics.UniLog
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DEBUG` | `2`
  `public static final int` | `DUMP` | `9`
  `public static final int` | `ERROR` | `0`
  `public static final int` | `INFO` | `6`
  `public static final int` | `INTER` | `7`
  `public static final int` | `IO` | `8`
  `public static final int` | `L1` | `2`
  `public static final int` | `L2` | `3`
  `public static final int` | `L3` | `4`
  `public static final int` | `L4` | `5`
  `public static final int` | `WARN` | `1`

- com.unitech.stuhflBridge.NativeDefines
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `GBT29768_SORT_MASK_SIZE` | `32`
  `public static final int` | `GEN2_LOCK_MASK_SIZE` | `3`
  `public static final int` | `GEN2_SELECT_MASK_SIZE` | `32`
  `public static final int` | `INVENTORYREPORT_SLOT_INFO_LIST_SIZE` | `256`
  `public static final int` | `STUHFL_D_DEFAULT_FREQUENCY` | `865700`
  `public static final int` | `STUHFL_D_FREQUENCY_MAX_VALUE` | `999000`
  `public static final int` | `STUHFL_D_GEN2_GENERIC_CMD_MAX_RCV_DATA_BYTES` | `128`
  `public static final int` | `STUHFL_D_GEN2_GENERIC_CMD_MAX_SND_DATA_BYTES` | `64`
  `public static final int` | `STUHFL_D_GEN2_MAXQ` | `15`
  `public static final int` | `STUHFL_D_GEN2_TIMING_USE_DEFAULT_T4MIN` | `0`
  `public static final int` | `STUHFL_D_INVENTORYREPORT_HEART_BEAT_DURATION_MS` | `400`
  `public static final int` | `STUHFL_D_LOG_LEVEL_COUNT` | `10`
  `public static final int` | `STUHFL_D_MAX_ANTENNA` | `4`
  `public static final int` | `STUHFL_D_MAX_BLOCKWRITE_DATA_LEN` | `16`
  `public static final int` | `STUHFL_D_MAX_EPC_LENGTH` | `64`
  `public static final int` | `STUHFL_D_MAX_FREQUENCY` | `53`
  `public static final int` | `STUHFL_D_MAX_PC_LENGTH` | `2`
  `public static final int` | `STUHFL_D_MAX_READ_DATA_LEN` | `64`
  `public static final int` | `STUHFL_D_MAX_REGISTERS` | `64`
  `public static final int` | `STUHFL_D_MAX_TAG_LIST_SIZE` | `64`
  `public static final int` | `STUHFL_D_MAX_TID_LENGTH` | `12`
  `public static final int` | `STUHFL_D_MAX_TIME_LENGTH` | `10`
  `public static final int` | `STUHFL_D_MAX_VERSION_INFO_LENGTH` | `64`
  `public static final int` | `STUHFL_D_MAX_WRITE_DATA_LEN` | `2`
  `public static final int` | `STUHFL_D_MAX_XPC_LENGTH` | `4`
  `public static final int` | `STUHFL_D_NB_C_VALUES` | `16`
  `public static final int` | `STUHFL_D_PASSWORD_LEN` | `4`
  `public static final int` | `STUHFL_D_RESET_DEFAULT_ALL_FREQS` | `0`
  `public static final int` | `STUHFL_D_TUNING_ALGO_ENABLE_FPD` | `128`