A B C D E F G H I K L M N O P Q R S T U V W X _

## I

i(String, int, String, Object...) - Static method in class com.unitech.lib.util.diagnotics.UniLog
i(String, int, String) - Static method in class com.unitech.lib.util.diagnotics.UniLog
i(String, String, Object...) - Static method in class com.unitech.lib.util.diagnotics.UniLog
IBufferControlEventListener - Interface in com.unitech.lib.transport.event
IConnectStateEventListener - Interface in com.unitech.lib.transport.event
  It is an interface to notify the connection status with the equipment.
id - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_RwdConfig
id - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_RwdConfig.Fields
IDeviceEventListener - Interface in com.unitech.lib.device
idleTime - Variable in class com.unitech.lib.reader.params.DutyCycle
idleTime() - Method in enum com.unitech.lib.uhf.module.impinj.types.PowerModeLevel
  Get the idle time value.
idleTime - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The idle time setting
idleTime - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_FreqLBT
  < I/O Param: Time for listing periode
idleTime - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_FreqLBT.Fields
IEnumType - Interface in com.unitech.lib.types
  The IEnumType interface provides the common functionality of all enumerations that the SDK uses.
IModuleRfidUhfEventListener - Interface in com.unitech.lib.uhf.event
INFO - Static variable in class com.unitech.lib.reader.device.BaseDevice
INFO - Static variable in class com.unitech.lib.reader.protocol.Protocol
INFO - Static variable in class com.unitech.lib.transport.BaseTransport
INFO - Static variable in class com.unitech.lib.util.diagnotics.UniLog
initModule() - Method in class com.unitech.lib.uhf.BaseUHF
  After the Device is connected, it calls to instantiate the BaseUHF instance.
initModule() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
initModule() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
initModule() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
initModuleInfo() - Method in class com.unitech.lib.htx.device.DeviceHT730
  Initialize module info for get device's supported module
initModuleInfo() - Method in class com.unitech.lib.rpx.device.DeviceRP902
  Initialize module info for get device's supported module
initReader() - Method in class com.unitech.lib.htx.HT730Reader
initReader() - Method in class com.unitech.lib.reader.BaseReader
  Initializes an BaseReader instance after the BaseReader instance is associated with the device.
initReader() - Method in class com.unitech.lib.rpx.RP902Reader
initSelectMask6cParam() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
initSelectMask6cParam() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.ANTENNA_POWER_MODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.CONTINUOUS_MODULATION_MODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.FREQUENCY_HOP_MODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_ACTION_ATTRIBUTE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_ACTION_SECMODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_AREA
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_BLF
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_CODING
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_CONDITION
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_CONFIGURATION
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_RULE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_SESSION
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_SORT_MODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_SORT_TARGET
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_TARGET
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GB29768_TC
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_BLF
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_CODING
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_GENERIC_CMD
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_MEMORY_BANK
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_SELECT_MODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_SELECT_TARGET
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_SESSION
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_TARGET
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.GEN2_TARI
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.HW_ID
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.POWER
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.PROFILE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.REPORT_OPTION
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.RET_CODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.RSSI_MODE
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.RWD_CFG_ID
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.TREXT_LEAD
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.TUNER_CAP
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.TUNING_ALGO
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.TUNING_STATUS
int2Enum(int) - Static method in enum com.unitech.stuhfl.STUHFL_E.USED_ANTENNA
INTER - Static variable in class com.unitech.lib.util.diagnotics.UniLog
interval - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AdaptiveSensitivity
interval - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gb29768_InventoryCfg.AutoTuning
interval - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AdaptiveSensitivity
  < I/O Param: Flag to enable automatic sensitivity adjustment
interval - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_Gen2_InventoryCfg.AutoTuning
inventory() - Method in class com.unitech.lib.uhf.module.impinj.ModuleUHFRM100
inventory() - Method in class com.unitech.lib.uhf.module.stseries.ModuleUHFST25RU3993
inventory6c() - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to inventory the RFID UHF tag of ISO18000-6c Gen2 standard.
inventory6c() - Method in class com.unitech.lib.uhf.impinj.UHFRM100
inventory6c() - Method in class com.unitech.lib.uhf.stseries.UHFST25RU3993
inventoryDelay - Variable in class com.unitech.stuhfl.STUHFL_T_Gb29768_Inventory
  < I Param: Inventory scan duration (in rounds).
inventoryDelay - Variable in class com.unitech.stuhfl.STUHFL_T_Gen2_Inventory
  < I Param: Inventory scan duration (in rounds).
inventoryDelay - Variable in class com.unitech.stuhflBridge.BR_Gb29768_Inventory.Fields
inventoryDelay - Variable in class com.unitech.stuhflBridge.BR_Gen2_Inventory.Fields
INVENTORYREPORT_SLOT_INFO_LIST_SIZE - Static variable in class com.unitech.stuhflBridge.NativeDefines
inventoryTime - Variable in class com.unitech.lib.reader.params.DutyCycle
inventoryTime() - Method in enum com.unitech.lib.uhf.module.impinj.types.PowerModeLevel
  Get the inventory time value.
inventoryTime - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The inventory time setting
IO - Static variable in class com.unitech.lib.reader.protocol.Protocol
IO - Static variable in class com.unitech.lib.transport.BaseTransport
IO - Static variable in class com.unitech.lib.util.diagnotics.UniLog
IProtocol - Interface in com.unitech.lib.protocol
IProtocolEventListener - Interface in com.unitech.lib.protocol
IReader - Interface in com.unitech.lib.device
  The IReader interface is an interface that defines the methods for reader needs.
IReaderEventListener - Interface in com.unitech.lib.reader.event
IRfidUhfEventListener - Interface in com.unitech.lib.uhf.event
  The IRfidUhfEventListener interface is an interface that defines event handling methods for handling events raised by the BaseUHF instance.
IRunnerListener - Interface in com.unitech.stuhflBridge
IRunnerListener.STUHFL_T_InventoryStatistics - Class in com.unitech.stuhflBridge
IRunnerListener.STUHFL_T_InventoryTag - Class in com.unitech.stuhflBridge
isConnected() - Method in class com.unitech.stuhflBridge.LibBridge
ISerialStream - Interface in com.unitech.stuhflBridge
isLogging(int) - Static method in class com.unitech.lib.util.diagnotics.UniLog
isNullOrEmpty(byte[]) - Static method in class com.unitech.lib.util.diagnotics.BitConvert
isNullOrEmpty(String) - Static method in class com.unitech.lib.util.diagnotics.StringUtil
isTicketExist(long) - Method in class com.unitech.lib.util.ServiceHandler
  Check if your ticket is exist
isUsed() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns whether or not "Selection Mask" is enabled.
itemList - Variable in class com.unitech.stuhfl.STUHFL_T_ST25RU3993_ChannelList
  < I/O Param: Current item index in channel list
items - Variable in class com.unitech.stuhflBridge.BR_ST25RU3993_ChannelList.Fields

A B C D E F G H I K L M N O P Q R S T U V W X _