# Package com.unitech.lib.types

- Interface Summary
  Interface | Description
  --- | ---
  IEnumType | The IEnumType interface provides the common functionality of all enumerations that the SDK uses.

- Enum Summary
  Enum | Description
  --- | ---
  ActionState | ActionState indicates the current operation status of the device.
  ActionType | ActionType indicates the operation type of the device.
  BeepAndVibrateState | The BeepAndVibrateState enumeration represents the type of device associated with the SDK.
  DataFormat | The DataFormat enumeration represents the type of device associated with the SDK.
  DataInfo | The DataInfo enumeration represents the type of device associated with the SDK.
  DataTerminator | The DataTerminator enumeration represents the type of device associated with the SDK.
  DeviceType | The DeviceType enumeration represents the type of device associated with the SDK.
  FindDeviceMode | The FindDeviceMode enumeration represents the type of device associated with the SDK.
  ModuleUHFType | The ModuleUHFType enumeration indicates the type of RFID UHF Module installed in the instrument.
  OperatingMode | The OperatingMode enumeration represents the type of device associated with the SDK.
  ReadMode | The ReadMode enumeration represents the type of device associated with the SDK.
  ReadOnceState | The ReadOnceState enumeration represents the type of device associated with the SDK.
  ResultCode | The ResultCode enumeration represents failure and behavior results.
  SKUType | The SKUType enumeration represents the type of device associated with the SDK.