A B C D E F G H I K L M N O P Q R S T V W _

## B

bankType() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access bank type.
BankType - Enum in com.unitech.lib.uhf.types
  The BankType enumeration specifies the memory bank of the RFID UHF tag.
BaseReader - Class in com.unitech.lib.reader
  The BaseReader class is a class that controls device in connection with unitech's equipment, receives data from device, and delivers it to the application program.
BaseReader(BaseTransport) - Constructor for class com.unitech.lib.reader.BaseReader
  Creates an instance of BaseReader.
BaseTransport - Class in com.unitech.lib.transport
  The Transport class is a class for abstracting connections with Reader devices.
BaseTransport() - Constructor for class com.unitech.lib.transport.BaseTransport
  Create an instance of the Transport class
BaseTransport(DeviceType, String, String) - Constructor for class com.unitech.lib.transport.BaseTransport
  Create an instance of the Transport class
BaseTransport(DeviceType, String, String, String) - Constructor for class com.unitech.lib.transport.BaseTransport
  Create an instance of the Transport class
BaseUHF - Class in com.unitech.lib.uhf
  BaseUHF class is a class that provides the function to control RFID UHF module installed in Device when BaseReader instance is connected to Device.
BaseUHF(IReader) - Constructor for class com.unitech.lib.uhf.BaseUHF
  Create an instance of the BaseUHF class.
BatteryStateEventArgs(BaseReader, int, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.BatteryStateEventArgs
BeepAndVibrateState - Enum in com.unitech.lib.types
  The BeepAndVibrateState enumeration represents the type of device associated with the SDK.
BeeperState - Enum in com.unitech.lib.reader.types
  Indicates the beeper status of equipment that supports Beeper.
blfType - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The BLF setting, only for RP902
BLFType - Enum in com.unitech.lib.uhf.types
  The BLFType enumeration represents the BLF by which the RFID UHF module inventories the TAG.

A B C D E F G H I K L M N O P Q R S T V W _