A B C D E F G H I K L M N O P Q R S T V W _

## O

offset - Variable in class com.unitech.lib.reader.params.DataRange
onAccessResult(ResultCode, ActionType, String, String, Object) - Method in interface com.unitech.lib.uhf.event.IModuleRfidUhfEventListener
onActionChanged(ResultCode, ActionType, Object) - Method in class com.unitech.lib.htx.HT730Reader
onActionChanged(ResultCode, ActionType, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onActionChanged(ResultCode, ActionType, Object) - Method in class com.unitech.lib.rpx.RP902Reader
onBatteryState(int, Object) - Method in class com.unitech.lib.htx.HT730Reader
onBatteryState(int, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onBatteryState(int, Object) - Method in class com.unitech.lib.rpx.RP902Reader
onEvent(int, Object) - Method in class com.unitech.lib.htx.HT730Reader
onEvent(int, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onEvent(int, Object) - Method in class com.unitech.lib.rpx.RP902Reader
onKeyEvent(KeyType, KeyState, Object) - Method in class com.unitech.lib.htx.HT730Reader
onKeyEvent(KeyType, KeyState, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onKeyEvent(KeyType, KeyState, Object) - Method in class com.unitech.lib.rpx.RP902Reader
onNotificationState(NotificationState, Object) - Method in class com.unitech.lib.htx.HT730Reader
onNotificationState(NotificationState, Object) - Method in interface com.unitech.lib.reader.event.IReaderEventListener
  Called to notify the state of the Device.
onNotificationState(NotificationState, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onNotificationState(NotificationState, Object) - Method in class com.unitech.lib.rpx.RP902Reader
onReaderActionChanged(ResultCode, ActionState, Object) - Method in class com.unitech.lib.reader.BaseReader
onReaderActionChanged(BaseReader, ResultCode, ActionState, Object) - Method in interface com.unitech.lib.reader.event.IReaderEventListener
  Called when the operational state of the Device associated with the BaseReader instance changes.
onReaderBatteryState(int, Object) - Method in class com.unitech.lib.reader.BaseReader
onReaderBatteryState(BaseReader, int, Object) - Method in interface com.unitech.lib.reader.event.IReaderEventListener
  Called to report the battery state of the Device attached to the BaseReader instance before it occurs.
onReaderKeyChanged(KeyType, KeyState, Object) - Method in class com.unitech.lib.reader.BaseReader
onReaderKeyChanged(BaseReader, KeyType, KeyState, Object) - Method in interface com.unitech.lib.reader.event.IReaderEventListener
  Called to report the key type and state of the Device attached to the BaseReader instance before it occurs.
onReaderNotificationState(NotificationState, Object) - Method in class com.unitech.lib.reader.BaseReader
onReaderStateChanged(ConnectState, Object) - Method in class com.unitech.lib.reader.BaseReader
onReaderStateChanged(BaseReader, ConnectState, Object) - Method in interface com.unitech.lib.reader.event.IReaderEventListener
  The BaseTransport instance associated with the BaseReader instance is called when the connection state of the Device changes.
onReaderTemperatureState(double, Object) - Method in class com.unitech.lib.reader.BaseReader
onReaderTemperatureState(BaseReader, double, Object) - Method in interface com.unitech.lib.reader.event.IReaderEventListener
  Called to report the temperature state of the Device attached to the BaseReader instance before it occurs.
onReadTag(String, Object) - Method in interface com.unitech.lib.uhf.event.IModuleRfidUhfEventListener
onRfidUhfAccessResult(BaseUHF, ResultCode, ActionState, String, String, Object) - Method in interface com.unitech.lib.uhf.event.IRfidUhfEventListener
  It is called when the device receives the result of executing the functions of Read Memory, Write Memory, Lock and so on.
onRfidUhfReadTag(BaseUHF, String, Object) - Method in interface com.unitech.lib.uhf.event.IRfidUhfEventListener
  Called when the device reads the tag while performing the Inventory function.
onStateChanged(ConnectState, Object) - Method in class com.unitech.lib.htx.HT730Reader
onStateChanged(ConnectState, Object) - Method in class com.unitech.lib.reader.BaseReader
  Called when the connection state of the BaseTransport instance and the device changes.
onStateChanged(ConnectState, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onStateChanged(ConnectState, Object) - Method in class com.unitech.lib.rpx.RP902Reader
onTemperatureState(double, Object) - Method in class com.unitech.lib.htx.HT730Reader
onTemperatureState(double, Object) - Method in class com.unitech.lib.rgx.RG768Reader
onTemperatureState(double, Object) - Method in class com.unitech.lib.rpx.RP902Reader
OperatingMode - Enum in com.unitech.lib.types
  The OperatingMode enumeration represents the type of device associated with the SDK.

A B C D E F G H I K L M N O P Q R S T V W _