A B C D E F G H I K L M N O P Q R S T V W _

## M

Mask6cAction - Enum in com.unitech.lib.uhf.types
  The Mask6cAction enumeration type indicates the status of the Flag when the RFID UHF module performs the Inventory operation and the pattern of the given Selection Mask is set as the Target value of the Selection Mask according to the condition.
Mask6cPattern - Class in com.unitech.lib.uhf.params
  The Mask6cPattern class is a class that represents the Mask Pattern of a Selection Mask in terms of pattern and length.
Mask6cPattern() - Constructor for class com.unitech.lib.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cPattern(<any>) - Constructor for class com.unitech.lib.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cPattern(String, int) - Constructor for class com.unitech.lib.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cTarget - Enum in com.unitech.lib.uhf.types
  The Mask6cTarget enumeration represents the Flag where the result status of the Selection Mask will be saved when the RFID UHF module is inventoried.
maxQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The maximum Q value
minQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The minimum Q value
mLastTime - Variable in class com.unitech.lib.reader.BaseReader
moduleProfile - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The module's profile setting, only for HT730
ModuleUHFType - Enum in com.unitech.lib.types
  The ModuleUHFType enumeration indicates the type of RFID UHF Module installed in the instrument.

A B C D E F G H I K L M N O P Q R S T V W _