A B C D E F G H I K L M N O P Q R S T V W _

## W

write(byte[], int) - Method in class com.unitech.lib.rpx.RP902Reader
write(byte[], int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Transfer data to the device.
write(byte[], int, int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Transfer data to the device.
write(byte[]) - Method in class com.unitech.lib.transport.BaseTransport
  Transfer data to the device.
write(byte[], int) - Method in class com.unitech.lib.transport.BaseTransport
  Transfer data to the device.
write(byte[], int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
write(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
write(byte[], int, int) - Method in class com.unitech.lib.transport.TransportUART
write(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportUART
writeMemory6c(BankType, int, String, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to store data in a specific memory of RFID UHF tag of ISO18000-6c Gen2 standard.

A B C D E F G H I K L M N O P Q R S T V W _