# Package com.unitech.lib.uhf.types

- Class Summary
  Class | Description
  --- | ---
  PowerDutyLimitationMap | The PowerDutyLimitationMap enumeration represents the type of device associated with the SDK.

- Enum Summary
  Enum | Description
  --- | ---
  AlgorithmType | The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
  BankType | The BankType enumeration specifies the memory bank of the RFID UHF tag.
  BLFType | The BLFType enumeration represents the BLF by which the RFID UHF module inventories the TAG.
  Encoding | The Encoding enumeration represents the miller encoding by which the RFID UHF module inventories the TAG.
  GlobalBandType | The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.
  LockState | The LockState enumeration represents the lock state.
  Mask6cAction | The Mask6cAction enumeration type indicates the status of the Flag when the RFID UHF module performs the Inventory operation and the pattern of the given Selection Mask is set as the Target value of the Selection Mask according to the condition.
  Mask6cTarget | The Mask6cTarget enumeration represents the Flag where the result status of the Selection Mask will be saved when the RFID UHF module is inventoried.
  PowerMode | The PowerMode enumeration specifies the power mode while inventory.
  Session | The Session enumeration represents the session of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  Target | The Target enumeration type indicates the status of the Target of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  TARIType | The TARIType enumeration represents the TARI by which the RFID UHF module inventories the TAG.