A B C D E F G H I K L M N O P Q R S T V W _

## A

ActionChangedEventArgs(BaseReader, ResultCode, ActionState, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.ActionChangedEventArgs
ActionState - Enum in com.unitech.lib.types
  ActionState indicates the current operation status of the device.
ActionType - Enum in com.unitech.lib.types
  ActionType indicates the operation type of the device.
actionType() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access action type.
addListener(IReaderEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Adds a Listener to receive events on an instance of the BaseReader class.
addListener(IReaderEventListener) - Method in class com.unitech.lib.reader.event.ReaderEventManager
addListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.BaseUHF
  Adds an event handler to receive events that occur in the instance.
addListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
algorithm - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Q algorithm setting
AlgorithmType - Enum in com.unitech.lib.uhf.types
  The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
antenna() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the antenna at which tag was detected.
available() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the length of data that can be read with the read method.
available() - Method in class com.unitech.lib.transport.TransportBluetooth
available() - Method in class com.unitech.lib.transport.TransportUART

A B C D E F G H I K L M N O P Q R S T V W _