A B C D E F G H I K L M N O P Q R S T U V W _

## S

ScreenOffTime - Class in com.unitech.lib.reader.params
  The ScreenOffTime class stores information about the screen off setting.
ScreenOffTime() - Constructor for class com.unitech.lib.reader.params.ScreenOffTime
ScreenOffTime(int, int) - Constructor for class com.unitech.lib.reader.params.ScreenOffTime
sdata - Variable in class com.unitech.lib.reader.params.DisplayOutput
SelectMask6cParam - Class in com.unitech.lib.uhf.params
  The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
SelectMask6cParam() - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, String, int) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, <any>) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMaskUTEParam - Class in com.unitech.lib.uhf.params
SelectMaskUTEParam() - Constructor for class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Creates an instance of the SelectMask6cParam class.
SelectMaskUTEParam(boolean, PA768eEnums.TagSelectMode, PA768eEnums.TagSelectTarget, PA768eEnums.TagSelectAction, PA768eEnums.TagSelectTruncate, PA768eEnums.BankType, int, short[], int) - Constructor for class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Creates an instance of the SelectMask6cParam class.
sendFwFileData(byte[]) - Method in class com.unitech.lib.uhf.BaseUHF
  Writes the firmware data into flash memory.
session - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Session setting
Session - Enum in com.unitech.lib.uhf.types
  The Session enumeration represents the session of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAction(ActionState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operational state of the device associated with the instance.
setAction(Mask6cAction) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
setAction(PA768eEnums.TagSelectAction) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set Action Flag of "Selection Mask".
setAddress(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the address of the device to which the instance of BaseReader is connected.
setAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the address of the device to which the BaseTransport instance is connected.
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
setAmbientTempProtection(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Ambient Temperature threshold of the RFID UTE module of the Device.
setAntennaSetting(int, int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Antenna Setting of the RFID UTE module of the Device.
setAntennaState(int, boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Antenna State of the RFID UTE module of the Device.
setAntennaSwitchMode(PA768eEnums.SwitchMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Antenna Switching Mode of the RFID UTE module of the Device.
setAutoOffTime(int) - Method in class com.unitech.lib.htx.HT730Reader
setAutoOffTime(int) - Method in class com.unitech.lib.pax.PA768eReader
setAutoOffTime(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time which the equipment automatically turns off.
setAutoOffTime(int) - Method in class com.unitech.lib.rgx.RG768Reader
setAutoOffTime(int) - Method in class com.unitech.lib.rpx.RP902Reader
setBank(BankType) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Bank value in "Selection Mask".
setBank(PA768eEnums.BankType) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set BankType Flag of "Selection Mask".
setBeeper(BeeperState) - Method in class com.unitech.lib.htx.HT730Reader
setBeeper(BeeperState) - Method in class com.unitech.lib.pax.PA768eReader
setBeeper(BeeperState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the beeper operation status of the equipment.
setBeeper(BeeperState) - Method in class com.unitech.lib.rgx.RG768Reader
setBeeper(BeeperState) - Method in class com.unitech.lib.rpx.RP902Reader
setBiStaticAntenna(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Bi-Static Antenna Setting of the RFID UTE module of the Device.
setBLF(BLFType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
setCfgStorageMode(PA768eEnums.CfgStorageMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Configuration Storage Mode of RAM/Flash for the Device.
setCheckInterval(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time period for checking the battery status of the device associated with the BaseReader class instance.
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.BaseUHF
  Setup the config of the RFID module
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets whether or not the RFID UHF module of the device will run the Inventory continuously.
setDataFormat(DataFormat) - Method in class com.unitech.lib.htx.HT730Reader
setDataFormat(DataFormat) - Method in class com.unitech.lib.pax.PA768eReader
setDataFormat(DataFormat) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data format setting of the equipment.
setDataFormat(DataFormat) - Method in class com.unitech.lib.rgx.RG768Reader
setDataFormat(DataFormat) - Method in class com.unitech.lib.rpx.RP902Reader
setDataInfo(DataInfo) - Method in class com.unitech.lib.htx.HT730Reader
setDataInfo(DataInfo) - Method in class com.unitech.lib.pax.PA768eReader
setDataInfo(DataInfo) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data info setting of the equipment.
setDataInfo(DataInfo) - Method in class com.unitech.lib.rgx.RG768Reader
setDataInfo(DataInfo) - Method in class com.unitech.lib.rpx.RP902Reader
setDataRange(DataRange) - Method in class com.unitech.lib.htx.HT730Reader
setDataRange(DataRange) - Method in class com.unitech.lib.pax.PA768eReader
setDataRange(DataRange) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data range setting of the equipment.
setDataRange(DataRange) - Method in class com.unitech.lib.rgx.RG768Reader
setDataRange(DataRange) - Method in class com.unitech.lib.rpx.RP902Reader
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.htx.HT730Reader
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.pax.PA768eReader
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data terminator setting of the equipment.
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.rgx.RG768Reader
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.rpx.RP902Reader
setDeviceName(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the name of the device to which the instance of BaseReader is connected.
setDeviceName(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the name of the device to which the BaseTransport instance is connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.reader.BaseReader
  Sets the type of device to which instance of BaseReader will be connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the type of device to which the instance will be connected.
setDisplayOutput(DisplayOutput) - Method in class com.unitech.lib.htx.HT730Reader
setDisplayOutput(DisplayOutput) - Method in class com.unitech.lib.pax.PA768eReader
setDisplayOutput(DisplayOutput) - Method in class com.unitech.lib.reader.BaseReader
  Sets the display output setting of the equipment.
setDisplayOutput(DisplayOutput) - Method in class com.unitech.lib.rgx.RG768Reader
setDisplayOutput(DisplayOutput) - Method in class com.unitech.lib.rpx.RP902Reader
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.htx.HT730Reader
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.pax.PA768eReader
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.reader.BaseReader
  Sets the display tags setting of the equipment output.
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.rgx.RG768Reader
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.rpx.RP902Reader
setDwellTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the dwellTime representing Antenna Setting of the RFID UTE module of the Device.
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setFastID(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Setup the status of the FastId that the RFID UHF module of the appliance uses to read tid when inventory.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
setFindDevice(FindDevice) - Method in class com.unitech.lib.htx.HT730Reader
setFindDevice(FindDevice) - Method in class com.unitech.lib.pax.PA768eReader
setFindDevice(FindDevice) - Method in class com.unitech.lib.reader.BaseReader
  Sets the find device status of the equipment.
setFindDevice(FindDevice) - Method in class com.unitech.lib.rgx.RG768Reader
setFindDevice(FindDevice) - Method in class com.unitech.lib.rpx.RP902Reader
setFixedFreqParams(RfidUtils.FIXEDFREQ_PARMS) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the multiple Fixed Frequencies value in the frequency hopping table of the RFID UTE module of the Device.
setFreqSwitchMode(PA768eEnums.SwitchMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Antenna Frequency Mode of the RFID UTE module of the Device.
setGlobalBand(GlobalBandType) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the national orientation of the RFID UHF module of the instrument.
setGpioPinsConfig(int, PA768eEnums.GpioDirection) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Direction representing the specified GPIO pins of the RFID UTE module of the Device.
setGpioPinsState(int, PA768eEnums.GpioState) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the State representing the specified GPIO pins of the RFID UTE module of the Device.
setIdleTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument sets the time for which the radio waves are not output in the Inventory operation and the rest of the time.
setInventoryTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the time at which radio waves are actually output in Inventory operation of the RFID UHF module of the instrument.
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setLastError(ResultCode) - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
setLbt(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Listen-Before-Talk Setting of the RFID UTE module of the Device.
setLbtCfgSetting(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the LBT RSSI threshold of RAM/Flash for the Device.
setLength(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Length of the EPCMaskParam instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the pattern length of the Mask6cPattern instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Length value of "Selection Mask".
setLength(int) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set length value of "Selection Mask".
setMacAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the MAC address of the device to which the BaseTransport instance is connected.
setMax(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the maximum Power Gian Level value for a PowerRange instance.
setMaxQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the maximum Q value.
setMin(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the Power Gian Level minimum value for a PowerRange instance.
setMinQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the minimum Q value.
setMinute(int) - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Set Minutes.
setMode(FindDeviceMode) - Method in class com.unitech.lib.reader.params.FindDevice
  Set FindDeviceMode.
setMode(PA768eEnums.TagSelectMode) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set Mode Flag of "Selection Mask".
setModuleProfile(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
setOffset(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the offset of the EPCMaskParam instance.
setOffset(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Offset value of "Selection Mask".
setOffset(int) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set offset value of "Selection Mask".
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.htx.HT730Reader
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.pax.PA768eReader
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operating mode status of the equipment.
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.rgx.RG768Reader
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.rpx.RP902Reader
setPATempProtection(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the PA Temperature threshold of the RFID UTE module of the Device.
setPattern(String) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Pattern for the EPCMaskParam instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the Mask pattern for the instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Pattern value of "Selection Mask".
setPattern(short[]) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set Pattern value of "Selection Mask".
setPower(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the antenna output of the RFID UHF module of the instrument.
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the power mode the RFID UHF module of the appliance uses to perform the inventory.
setPowerSaveMode(PA768eEnums.PowerSaveMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Power Save Mode of the RFID UTE module of the Device.
setReadMode(ReadMode) - Method in class com.unitech.lib.htx.HT730Reader
setReadMode(ReadMode) - Method in class com.unitech.lib.pax.PA768eReader
setReadMode(ReadMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the read mode status of the equipment.
setReadMode(ReadMode) - Method in class com.unitech.lib.rgx.RG768Reader
setReadMode(ReadMode) - Method in class com.unitech.lib.rpx.RP902Reader
setRegion(PA768eEnums.RegionType) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Region of the RFID UTE module of the Device.
setRFMode(PA768eEnums.RfMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the RF Mode of the RFID UTE module of the Device.
setScreenOffTime(ScreenOffTime) - Method in class com.unitech.lib.htx.HT730Reader
setScreenOffTime(ScreenOffTime) - Method in class com.unitech.lib.pax.PA768eReader
setScreenOffTime(ScreenOffTime) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time which the equipment automatically screen off.
setScreenOffTime(ScreenOffTime) - Method in class com.unitech.lib.rgx.RG768Reader
setScreenOffTime(ScreenOffTime) - Method in class com.unitech.lib.rpx.RP902Reader
setSecond(int) - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Set Seconds.
setSelected(PA768eEnums.QueryGroupSelected) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Query Group's Selected of the RFID UTE module of the Device.
setSelectMask6c(int, SelectMask6cParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison behavior of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the memory bank to be compared.
setSelectMask6cEnabled(int, boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set whether or not to use the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the start address of the memory to start the comparison.
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison value and length of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Flag of the tag to save the comparison result of Selection Mask item of the RFID UHF module of the device.
setSelectMaskUTE(int, SelectMaskUTEParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Selection Mask item of the RFID UTE module of the Device.
setSelectMaskUTETruncate(int, PA768eEnums.TagSelectTruncate) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the EPC response format of the Selection Mask item of the RFID UTE module of the device.
setSession(Session) - Method in class com.unitech.lib.uhf.BaseUHF
  Device's RFID UHF module sets the Session to check the status of the Session of the tag to be read by Inventory operation.
setSoftWareScan(boolean) - Method in class com.unitech.lib.htx.HT730Reader
setSoftWareScan(boolean) - Method in class com.unitech.lib.pax.PA768eReader
setSoftWareScan(boolean) - Method in class com.unitech.lib.reader.BaseReader
  Sets the software scan setting of the equipment.
setSoftWareScan(boolean) - Method in class com.unitech.lib.rgx.RG768Reader
setSoftWareScan(boolean) - Method in class com.unitech.lib.rpx.RP902Reader
setStartQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, set the starting Q value.
setState(ConnectState, Object) - Method in class com.unitech.lib.transport.BaseTransport
setStateListener(IConnectStateEventListener) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the listener to receive the connection status of an instance of the BaseTransport class.
setTagAuthenticate(RfidUtils.AUTHENTICATE_PARMS) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Tag Authenticate for the Device.
setTagBlockPermaLock(RfidUtils.BLOCKPERMALOCK_PARMS) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Tag Block PermaLock for the Device.
setTagFocus(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the TagFocus Setting of the RFID UTE module of the Device.
setTarget(Target) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the state of target of tag to read by Inventory operation.
setTarget(Mask6cTarget) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Target Flag of "Selection Mask".
setTarget(PA768eEnums.TagSelectTarget) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set Target Flag of "Selection Mask".
setTARI(TARIType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
setTemperatureProtectMode(PA768eEnums.ProtectionMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Temperature Protection Mode of the RFID UTE module of the Device.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'TID memory'.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'TID memory'.
setTime(Date) - Method in class com.unitech.lib.htx.HT730Reader
setTime(Date) - Method in class com.unitech.lib.pax.PA768eReader
setTime(Date) - Method in class com.unitech.lib.reader.BaseReader
  Sets the system time of the instrument.
setTime(Date) - Method in class com.unitech.lib.rgx.RG768Reader
setTime(Date) - Method in class com.unitech.lib.rpx.RP902Reader
setTimeout(int) - Method in class com.unitech.lib.reader.params.FindDevice
  Set timeout.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
setTruncate(PA768eEnums.TagSelectTruncate) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set Truncate Flag of "Selection Mask".
setTxOnOffTime(int[]) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Tx On/Off Time of the RFID UTE module of the Device.
setUartBaudRate(long) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Baud Rate of the RFID UTE module of the Device.
setUsed(boolean) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set whether or not to use "Selection Mask".
setUsed(boolean) - Method in class com.unitech.lib.uhf.params.SelectMaskUTEParam
  Set whether or not to use "Selection Mask".
setUser(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setUser(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setVibrator(VibratorState) - Method in class com.unitech.lib.htx.HT730Reader
setVibrator(VibratorState) - Method in class com.unitech.lib.pax.PA768eReader
setVibrator(VibratorState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the vibrator operation status of the equipment.
setVibrator(VibratorState) - Method in class com.unitech.lib.rgx.RG768Reader
setVibrator(VibratorState) - Method in class com.unitech.lib.rpx.RP902Reader
SGTIN - Class in com.unitech.lib.tagcoder
  The SGTIN class is a class that convert EPC to SGTIN format.
SGTIN(String) - Constructor for class com.unitech.lib.tagcoder.SGTIN
SKUType - Enum in com.unitech.lib.types
  The SKUType enumeration represents the type of device associated with the SDK.
startFwFileTransfer(String, long) - Method in class com.unitech.lib.uhf.BaseUHF
  Prepares for a firmware update.
startFwUpdate(PA768eEnums.FWUpdateMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Performs a firmware update by switching to update mode
startQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The start Q value
StateChangedEventArgs(BaseReader, ConnectState, Object) - Constructor for class com.unitech.lib.reader.event.ReaderEventManager.StateChangedEventArgs
stop() - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to stop the operation being performed.
stringToBytesASCII(String) - Static method in class com.unitech.lib.reader.params.DisplayOutput
  Returns the ASCII of String.
strZero(String, int) - Static method in class com.unitech.lib.tagcoder.SGTIN
  Padding a string with zeroes
supportedGlobalBand() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the global band types that the RFID UHF module support.
supportedRegionType() - Method in class com.unitech.lib.uhf.BaseUHF

A B C D E F G H I K L M N O P Q R S T U V W _