# Package com.unitech.lib.uhf.params

- Class Summary
  Class | Description
  --- | ---
  EPCMaskParam | The EPCMaskParam class stores information about the EPC Mask when the RFID UHF module sets or returns an EPC Mask.
  GlobalBandTable |
  Lock6cParam | The Lock6cParam class is used to pass information that the RFID UHF's Lock command performs.
  Mask6cPattern | The Mask6cPattern class is a class that represents the Mask Pattern of a Selection Mask in terms of pattern and length.
  PermaLock6cParam | The PermaLock6cParam class is used to pass information pertaining to RFID UHF's PermaLock command.
  PowerRange | The PowerRange class is a class that represents the setting range of the power gain level of an RFID UHF antenna.
  RFIDConfig | The RFIDConfig class stores the config of the RFID module.
  SelectMask6cParam | The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
  TagAccessResult | The TagAccessResult class is used to pass the tag access result information.
  TagExtParam | The TagExtParam class is used to pass the tag information.