A B C D E F G H I K L M N O P Q R S T U V W _

## R

read(byte[], int) - Method in class com.unitech.lib.rpx.RP902Reader
read(byte[], int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[]) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportUART
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportUART
ReaderEventManager - Class in com.unitech.lib.reader.event
ReaderEventManager() - Constructor for class com.unitech.lib.reader.event.ReaderEventManager
ReaderEventManager.ActionChangedEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.BatteryStateEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.KeyChangedEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.NotificationStateEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.StateChangedEventArgs - Class in com.unitech.lib.reader.event
ReaderEventManager.TemperatureStateEventArgs - Class in com.unitech.lib.reader.event
ReaderException - Exception in com.unitech.lib.diagnositics
  The exception class and contain result code
ReaderException(ResultCode) - Constructor for exception com.unitech.lib.diagnositics.ReaderException
ReaderException(ResultCode, String) - Constructor for exception com.unitech.lib.diagnositics.ReaderException
readMemory6c(BankType, int, int, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to read specific memory of RFID UHF tag of ISO18000-6c Gen2 standard.
ReadMode - Enum in com.unitech.lib.types
  The ReadMode enumeration represents the type of device associated with the SDK.
ReadOnceState - Enum in com.unitech.lib.types
  The ReadOnceState enumeration represents the type of device associated with the SDK.
removeListener(IReaderEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Removes the Listener that is listening for events on an instance of the BaseReader class.
removeListener(IReaderEventListener) - Method in class com.unitech.lib.reader.event.ReaderEventManager
removeListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.BaseUHF
  Removes an event handler when it no longer needs to receive events raised by the instance.
removeListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
resetError() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
ResultCode - Enum in com.unitech.lib.types
  The ResultCode enumeration represents failure and behavior results.
resultCode() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access result code.
RETRY_COUNT - Static variable in class com.unitech.lib.reader.BaseReader
RFIDConfig - Class in com.unitech.lib.uhf.params
  The RFIDConfig class stores the config of the RFID module.
RFIDConfig() - Constructor for class com.unitech.lib.uhf.params.RFIDConfig
  The antenna dwellTime value
RfidUhfEventManager - Class in com.unitech.lib.uhf.event
RfidUhfEventManager() - Constructor for class com.unitech.lib.uhf.event.RfidUhfEventManager
rfMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The rf mode setting
RFMode - Enum in com.unitech.lib.uhf.types
RG768Reader - Class in com.unitech.lib.rgx
  The RG768Reader class is a class that controls RG768, receives data from RM100, and delivers it to the application program.
RG768Reader(Context) - Constructor for class com.unitech.lib.rgx.RG768Reader
RP902Reader - Class in com.unitech.lib.rpx
  The RP902Reader class is a class that controls RP902 in connection with unitech's equipment, receives data from RP902, and delivers it to the application program.
RP902Reader(BaseTransport) - Constructor for class com.unitech.lib.rpx.RP902Reader
Russia - Static variable in class com.unitech.lib.uhf.params.GlobalBandTable

A B C D E F G H I K L M N O P Q R S T U V W _