A B C D E F G H I K L M N O P Q R S T U V W _

## G

generateReaderActionChanged(BaseReader, ResultCode, ActionState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderBatteryState(BaseReader, int, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderKeyChanged(BaseReader, KeyType, KeyState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderNotificationState(BaseReader, NotificationState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderStateChanged(BaseReader, ConnectState, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateReaderTemperatureState(BaseReader, double, Object) - Method in class com.unitech.lib.reader.event.ReaderEventManager
generateUHFAccessResult(BaseUHF, ResultCode, ActionState, String, String, Object) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
generateUHFReadTag(BaseUHF, String, Object) - Method in class com.unitech.lib.uhf.event.RfidUhfEventManager
getAccessPassword() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAccessPassword() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAction() - Method in class com.unitech.lib.reader.BaseReader
  Returns the current behavior of the device associated with an instance of the BaseReader class.
getAction() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Action value of "Selection Mask".
getAddress() - Method in class com.unitech.lib.reader.BaseReader
  Returns the address of the device associated with an instance of the BaseReader class.
getAddress() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the address of the device to which the BaseTransport instance is connected.
getAlgorithmType() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
getAmbientTemperature() - Method in class com.unitech.lib.htx.HT730Reader
getAmbientTemperature() - Method in class com.unitech.lib.pax.PA768eReader
getAmbientTemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the ambient temperature of the equipment.
getAmbientTemperature() - Method in class com.unitech.lib.rgx.RG768Reader
getAmbientTemperature() - Method in class com.unitech.lib.rpx.RP902Reader
getAmbientTemperatureProtection() - Method in class com.unitech.lib.htx.HT730Reader
getAmbientTemperatureProtection() - Method in class com.unitech.lib.pax.PA768eReader
getAmbientTemperatureProtection() - Method in class com.unitech.lib.reader.BaseReader
  Returns the ambient temperature protection setting of the equipment.
getAmbientTemperatureProtection() - Method in class com.unitech.lib.rgx.RG768Reader
getAmbientTemperatureProtection() - Method in class com.unitech.lib.rpx.RP902Reader
getAntennaSwitchingMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Antenna Switching Mode of the RFID UTE module of the Device.
getAutoOffTime() - Method in class com.unitech.lib.htx.HT730Reader
getAutoOffTime() - Method in class com.unitech.lib.pax.PA768eReader
getAutoOffTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time which the instrument automatically turns off.
getAutoOffTime() - Method in class com.unitech.lib.rgx.RG768Reader
getAutoOffTime() - Method in class com.unitech.lib.rpx.RP902Reader
getAutoOffTimeList() - Method in class com.unitech.lib.htx.HT730Reader
getAutoOffTimeList() - Method in class com.unitech.lib.pax.PA768eReader
getAutoOffTimeList() - Method in class com.unitech.lib.reader.BaseReader
  Returns the equipment supports auto off time list, the unit is minutes
getAutoOffTimeList() - Method in class com.unitech.lib.rgx.RG768Reader
getAutoOffTimeList() - Method in class com.unitech.lib.rpx.RP902Reader
getBank() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
getBatteryState() - Method in class com.unitech.lib.htx.HT730Reader
getBatteryState() - Method in class com.unitech.lib.pax.PA768eReader
getBatteryState() - Method in class com.unitech.lib.reader.BaseReader
  Returns the battery state of the equipment.
getBatteryState() - Method in class com.unitech.lib.rgx.RG768Reader
getBatteryState() - Method in class com.unitech.lib.rpx.RP902Reader
getBaudRate() - Method in class com.unitech.lib.transport.TransportUART
getBeeper() - Method in class com.unitech.lib.htx.HT730Reader
getBeeper() - Method in class com.unitech.lib.pax.PA768eReader
getBeeper() - Method in class com.unitech.lib.reader.BaseReader
  Returns the beeper operation status of the equipment.
getBeeper() - Method in class com.unitech.lib.rgx.RG768Reader
getBeeper() - Method in class com.unitech.lib.rpx.RP902Reader
getBLF() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
getCfgStorageMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the configuration storage mode of the RFID UTE module of the Device.
getCheckInterval() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time period for checking the battery status of the device associated with an instance of the BaseReader class.
getCode() - Method in exception com.unitech.lib.diagnositics.ReaderException
  Get fault and motion results.
getCode() - Method in enum com.unitech.lib.reader.types.BeeperState
getCode() - Method in enum com.unitech.lib.reader.types.KeyState
getCode() - Method in enum com.unitech.lib.reader.types.KeyType
getCode() - Method in enum com.unitech.lib.reader.types.NotificationState
getCode() - Method in enum com.unitech.lib.reader.types.VibratorState
getCode() - Method in enum com.unitech.lib.transport.types.ConnectState
getCode() - Method in enum com.unitech.lib.transport.types.ConnectType
getCode() - Method in enum com.unitech.lib.types.ActionState
getCode() - Method in enum com.unitech.lib.types.ActionType
getCode() - Method in enum com.unitech.lib.types.BeepAndVibrateState
getCode() - Method in enum com.unitech.lib.types.DataFormat
getCode() - Method in enum com.unitech.lib.types.DataInfo
getCode() - Method in enum com.unitech.lib.types.DataTerminator
getCode() - Method in enum com.unitech.lib.types.DeviceType
getCode() - Method in enum com.unitech.lib.types.EventNotifyId
getCode() - Method in enum com.unitech.lib.types.FindDeviceMode
getCode() - Method in enum com.unitech.lib.types.FirmwareUpdateMode
getCode() - Method in interface com.unitech.lib.types.IEnumType
  Get the enum code value
getCode() - Method in enum com.unitech.lib.types.ModuleUHFType
getCode() - Method in enum com.unitech.lib.types.OperatingMode
getCode() - Method in enum com.unitech.lib.types.ReadMode
getCode() - Method in enum com.unitech.lib.types.ReadOnceState
getCode() - Method in enum com.unitech.lib.types.ResultCode
getCode() - Method in enum com.unitech.lib.types.SKUType
getCode() - Method in enum com.unitech.lib.uhf.types.AlgorithmType
getCode() - Method in enum com.unitech.lib.uhf.types.AntennaSwitchingMode
getCode() - Method in enum com.unitech.lib.uhf.types.BankType
getCode() - Method in enum com.unitech.lib.uhf.types.BLFType
getCode() - Method in enum com.unitech.lib.uhf.types.CfgStorageMode
getCode() - Method in enum com.unitech.lib.uhf.types.Encoding
getCode() - Method in enum com.unitech.lib.uhf.types.FrequencySwitchingMode
getCode() - Method in enum com.unitech.lib.uhf.types.GlobalBandType
getCode() - Method in enum com.unitech.lib.uhf.types.LockState
getCode() - Method in enum com.unitech.lib.uhf.types.Mask6cAction
getCode() - Method in enum com.unitech.lib.uhf.types.Mask6cTarget
getCode() - Method in enum com.unitech.lib.uhf.types.PowerMode
getCode() - Method in enum com.unitech.lib.uhf.types.PowerSavingMode
getCode() - Method in enum com.unitech.lib.uhf.types.RFMode
getCode() - Method in enum com.unitech.lib.uhf.types.SelectMaskMode
getCode() - Method in enum com.unitech.lib.uhf.types.SelectMode
getCode() - Method in enum com.unitech.lib.uhf.types.Session
getCode() - Method in enum com.unitech.lib.uhf.types.Target
getCode() - Method in enum com.unitech.lib.uhf.types.TARIType
getCode() - Method in enum com.unitech.lib.uhf.types.TemperatureProtectionMode
getCode() - Method in enum com.unitech.lib.uhf.types.Truncate
getCompany() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Company number.
getConfig() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the config of RFID module
getConnectType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the instance of BaseReader associated with device.
getConnectType() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the instance of Transport associated with device.
getContinuousMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns whether the RFID UHF module on the device will cause the Inventory to run continuously.
getCount() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get count of GTIN
getData() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access result data value with HEX format.
getDataFormat() - Method in class com.unitech.lib.htx.HT730Reader
getDataFormat() - Method in class com.unitech.lib.pax.PA768eReader
getDataFormat() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data format setting of the equipment.
getDataFormat() - Method in class com.unitech.lib.rgx.RG768Reader
getDataFormat() - Method in class com.unitech.lib.rpx.RP902Reader
getDataInfo() - Method in class com.unitech.lib.htx.HT730Reader
getDataInfo() - Method in class com.unitech.lib.pax.PA768eReader
getDataInfo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data info setting of the equipment.
getDataInfo() - Method in class com.unitech.lib.rgx.RG768Reader
getDataInfo() - Method in class com.unitech.lib.rpx.RP902Reader
getDataRange() - Method in class com.unitech.lib.htx.HT730Reader
getDataRange() - Method in class com.unitech.lib.pax.PA768eReader
getDataRange() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data range setting of the equipment.
getDataRange() - Method in class com.unitech.lib.rgx.RG768Reader
getDataRange() - Method in class com.unitech.lib.rpx.RP902Reader
getDataTerminator() - Method in class com.unitech.lib.htx.HT730Reader
getDataTerminator() - Method in class com.unitech.lib.pax.PA768eReader
getDataTerminator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data terminator setting of the equipment.
getDataTerminator() - Method in class com.unitech.lib.rgx.RG768Reader
getDataTerminator() - Method in class com.unitech.lib.rpx.RP902Reader
getDescription() - Method in exception com.unitech.lib.diagnositics.ReaderException
  Get description of the exception.
getDeviceName() - Method in class com.unitech.lib.reader.BaseReader
  Returns the name of the Device associated with an instance of the BaseReader class.
getDeviceName() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the name of the Device to which the BaseTransport instance is connected.
getDeviceType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the type of Device to which the instance is connected.
getDeviceType() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the type of device to which the instance will be connected.
getDwellTime() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the dwellTime representing Antenna Setting of the RFID UTE module of the Device.
getEncoding() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
getEpc() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get EPC.
getEpc() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access tag's EPC value with HEX format.
getEpc() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's EPC value with HEX format.
getExtensionDigit() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Extension Digit
getFastID() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the FastId that the RFID UHF module of the appliance uses to read tid when inventory.
getFastMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
getFindDevice() - Method in class com.unitech.lib.htx.HT730Reader
getFindDevice() - Method in class com.unitech.lib.pax.PA768eReader
getFindDevice() - Method in class com.unitech.lib.reader.BaseReader
  Returns the find device status of the equipment.
getFindDevice() - Method in class com.unitech.lib.rgx.RG768Reader
getFindDevice() - Method in class com.unitech.lib.rpx.RP902Reader
getFixedFrequency() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Fixed Frequency of the RFID UTE module of the Device.
getFreqSwitchingMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Frequency Switching Mode of the RFID UTE module of the Device.
getFrequency() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's frequency value.
getGlobalBand() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the national orientation of the RFID UHF module of the instrument.
getGTIN14() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get GTIN
getIdleTime() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument returns the time that the radio waves are not output in the Inventory operation and is resting.
getInventoryTime() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the time at which radio waves are actually output from the Inventory operation of the RFID UHF module in the instrument.
getItemReference() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Item Reference
getKeyState() - Method in class com.unitech.lib.reader.params.KeyEventItem
getKeyType() - Method in class com.unitech.lib.reader.params.KeyEventItem
getKillPassword() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getKillPassword() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getLastError() - Method in class com.unitech.lib.reader.BaseReader
  Returns the result code for the last action.
getLbt() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Listen-Before-Talk Setting of the RFID UTE module of the Device.
getLbtCfgSetting() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the LBT RSSI threshold of the RFID UTE module of the Device.
getLength() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns the Length of the EPCMaskParam instance.
getLength() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Returns the pattern length of the Mask6cPattern instance.
getLength() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Length value of "Selection Mask".
getLimitationMap() - Static method in class com.unitech.lib.uhf.types.PowerDutyLimitationMap
  Returns Duty Limitation Map.
getLimitDuty(int) - Static method in class com.unitech.lib.uhf.types.PowerDutyLimitationMap
  Returns Duty Limitation.
getMacAddress() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the MAC address of the device to which the BaseTransport instance is connected.
getMax() - Method in class com.unitech.lib.uhf.params.PowerRange
  Returns the maximum Power Gian Level value for a PowerRange instance.
getMaxQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the maximum Q value.
getMessage() - Method in enum com.unitech.lib.types.ResultCode
  Returns the result code's description.
getMin() - Method in class com.unitech.lib.uhf.params.PowerRange
  Returns the Power Gian Level minimum value for a PowerRange instance.
getMinQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the minimum Q value.
getMinute() - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Returns Minutes.
getMode() - Method in class com.unitech.lib.reader.params.FindDevice
  Returns FindDeviceMode.
getModuleProfile() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
getOffset() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns the offset of the EPCMaskParam instance.
getOffset() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Offset value of "Selection Mask".
getOperatingMode() - Method in class com.unitech.lib.htx.HT730Reader
getOperatingMode() - Method in class com.unitech.lib.pax.PA768eReader
getOperatingMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the operating mode status of the equipment.
getOperatingMode() - Method in class com.unitech.lib.rgx.RG768Reader
getOperatingMode() - Method in class com.unitech.lib.rpx.RP902Reader
getPATemperature() - Method in class com.unitech.lib.htx.HT730Reader
getPATemperature() - Method in class com.unitech.lib.pax.PA768eReader
getPATemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the PA temperature of the equipment.
getPATemperature() - Method in class com.unitech.lib.rgx.RG768Reader
getPATemperature() - Method in class com.unitech.lib.rpx.RP902Reader
getPATemperatureProtection() - Method in class com.unitech.lib.htx.HT730Reader
getPATemperatureProtection() - Method in class com.unitech.lib.pax.PA768eReader
getPATemperatureProtection() - Method in class com.unitech.lib.reader.BaseReader
  Returns the PA temperature protection setting of the equipment.
getPATemperatureProtection() - Method in class com.unitech.lib.rgx.RG768Reader
getPATemperatureProtection() - Method in class com.unitech.lib.rpx.RP902Reader
getPath() - Method in class com.unitech.lib.transport.TransportUART
getPattern() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns Pattern of the EPCMaskParam instance.
getPattern() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Returns the Mask pattern of the Mask6cPattern instance.
getPattern() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Pattern value of "Selection Mask".
getPC() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's PC value with HEX format.
getPower() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna output of the RFID UHF module of the instrument.
getPowerAndDutyLimitationMapInfo() - Method in class com.unitech.lib.htx.HT730Reader
getPowerAndDutyLimitationMapInfo() - Method in class com.unitech.lib.pax.PA768eReader
getPowerAndDutyLimitationMapInfo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the Power Duty Limitation Map setting of the equipment.
getPowerAndDutyLimitationMapInfo() - Method in class com.unitech.lib.rgx.RG768Reader
getPowerAndDutyLimitationMapInfo() - Method in class com.unitech.lib.rpx.RP902Reader
getPowerMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the power mode that the RFID UHF module of the appliance uses to perform the inventory.
getPowerRange() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna output range of the RFID UHF module of the instrument.
getPowerSavingMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Power Saving Mode of the RFID UTE module of the Device.
getPrefiex() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get GTIN prefix
getProtocol() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
getReadMode() - Method in class com.unitech.lib.htx.HT730Reader
getReadMode() - Method in class com.unitech.lib.pax.PA768eReader
getReadMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the read mode status of the equipment.
getReadMode() - Method in class com.unitech.lib.rgx.RG768Reader
getReadMode() - Method in class com.unitech.lib.rpx.RP902Reader
getRfidUhf() - Method in class com.unitech.lib.reader.BaseReader
  If the BaseReader instance supports the RFID UHF module, it returns an interface object that can control the RFID UHF module.
getRFMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the RF Mode of the RFID UTE module of the Device.
getRssi() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's RSSI value.
getScreenOffTime() - Method in class com.unitech.lib.htx.HT730Reader
getScreenOffTime() - Method in class com.unitech.lib.pax.PA768eReader
getScreenOffTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time which the instrument automatically screen off.
getScreenOffTime() - Method in class com.unitech.lib.rgx.RG768Reader
getScreenOffTime() - Method in class com.unitech.lib.rpx.RP902Reader
getSecond() - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Returns Seconds.
getSelectMask6c(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cAction(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the comparison behavior of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cBank(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the Device's RFID UHF module returns the memory bank to compare.
getSelectMask6cEnabled(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns whether to use the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cMaxSize() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the max size of select mask list status of the RFID UHF module.
getSelectMask6cOffset(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the Device returns the starting address of the memory to start the comparison.
getSelectMask6cPattern(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the comparison value and length of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cTarget(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Flag of the tag to store the comparison result of Selection Mask item of RFID UHF module of Device.
getSelectMask6cTruncate(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Truncate item of the RFID UTE module of the Device.
getSelectMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Select Mode of the RFID UTE module of the Device.
getSerial() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Serial number
getSerialNo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the serial number of the device.
getSession() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the device returns the Session to check the state of the Session of the tag to be read by the Inventory operation.
getSKU() - Method in class com.unitech.lib.htx.HT730Reader
getSKU() - Method in class com.unitech.lib.pax.PA768eReader
getSKU() - Method in class com.unitech.lib.reader.BaseReader
  Returns the SKU type of the equipment.
getSKU() - Method in class com.unitech.lib.rgx.RG768Reader
getSKU() - Method in class com.unitech.lib.rpx.RP902Reader
getStartQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, it returns the starting Q value.
getState() - Method in class com.unitech.lib.reader.BaseReader
  Returns the connection status of the device with the instance of the BaseReader class.
getState() - Method in class com.unitech.lib.transport.BaseTransport
  The instance of BaseTransport returns the connection status with device.
getTagFocus() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the TagFocus Setting of the RFID UTE module of the Device.
getTarget() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the device returns the status of the Target of the tag to be read by the Inventory operation.
getTarget() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Target Flag of "Selection Mask".
getTARI() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
getTemperature() - Method in class com.unitech.lib.htx.HT730Reader
getTemperature() - Method in class com.unitech.lib.pax.PA768eReader
getTemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the temperature of the equipment.
getTemperature() - Method in class com.unitech.lib.rgx.RG768Reader
getTemperature() - Method in class com.unitech.lib.rpx.RP902Reader
getTemperatureProtectionMode() - Method in class com.unitech.lib.htx.HT730Reader
getTemperatureProtectionMode() - Method in class com.unitech.lib.pax.PA768eReader
getTemperatureProtectionMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the temperature protection mode of the equipment.
getTemperatureProtectionMode() - Method in class com.unitech.lib.rgx.RG768Reader
getTemperatureProtectionMode() - Method in class com.unitech.lib.rpx.RP902Reader
getTid() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'TID memory'.
getTid() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'TID memory'.
getTID() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's TID value with HEX format.
getTime() - Method in class com.unitech.lib.htx.HT730Reader
getTime() - Method in class com.unitech.lib.pax.PA768eReader
getTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the system time of the device.
getTime() - Method in class com.unitech.lib.rgx.RG768Reader
getTime() - Method in class com.unitech.lib.rpx.RP902Reader
getTimeout() - Method in class com.unitech.lib.reader.params.FindDevice
  Returns timeout value.
getToggleTarget() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
getTransport() - Method in class com.unitech.lib.reader.BaseReader
  Returns an instance of the BaseTransport class that connects an instance of the BaseReader class to the Device.
getTruncate() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Truncate value of "Selection Mask".
getType() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the RFID UHF module type of the connected Device.
getUser() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getUser() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getVersion() - Method in class com.unitech.lib.reader.BaseReader
  Returns the firmware version of the device associated with the instance of the BaseReader class.
getVersion() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the version of the RFID UHF module.
getVibrator() - Method in class com.unitech.lib.htx.HT730Reader
getVibrator() - Method in class com.unitech.lib.pax.PA768eReader
getVibrator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the vibrator operation status of the equipment.
getVibrator() - Method in class com.unitech.lib.rgx.RG768Reader
getVibrator() - Method in class com.unitech.lib.rpx.RP902Reader
GlobalBandTable - Class in com.unitech.lib.uhf.params
GlobalBandTable() - Constructor for class com.unitech.lib.uhf.params.GlobalBandTable
GlobalBandType - Enum in com.unitech.lib.uhf.types
  The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.

A B C D E F G H I K L M N O P Q R S T U V W _