A B C D E F G H I K L M N O P Q R S T U V W X _

## A

abortFirmwareUpdate() - Method in class com.unitech.lib.reader.BaseReader
  Aborts the ongoing firmware update process.
AccessMode - Enum in com.unitech.lib.types
  Enum representing different access modes.
accessPassword - Variable in class com.unitech.lib.uhf.params.AuthenticateParam
accessPassword - Variable in class com.unitech.lib.uhf.params.BlockPermaLockParam
accessPassword - Variable in class com.unitech.lib.uhf.params.MarginReadParam
ActionState - Enum in com.unitech.lib.types
  ActionState indicates the current operation status of the device.
actionType() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access action type.
addListener(IReaderEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Adds a Listener to receive events on an instance of the BaseReader class.
addListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.BaseUHF
  Adds an event handler to receive events that occur in the instance.
algorithm - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Q algorithm setting
AlgorithmType - Enum in com.unitech.lib.uhf.types
  The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
allocateEngine(int) - Method in class com.unitech.lib.reader.BaseReader
  Allocates an engine based on the specified engine model.
allocateUHF(int) - Method in class com.unitech.lib.reader.BaseReader
  Allocates a UHF module of the device associated with the BaseReader instance.
allocateUHF(int, int) - Method in class com.unitech.lib.reader.BaseReader
  Allocates a UHF module based on the specified module type and handle.
antenna() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the antenna identifier associated with the tag
AntennaBeginEnd - Enum in com.unitech.lib.uhf.types
  Enum representing the beginning and end of an antenna operation.
antennaId - Variable in class com.unitech.lib.params.AntennaStatusEventArgs
AntennaStatusEventArgs - Class in com.unitech.lib.params
  Represents the status of an antenna.
AntennaStatusEventArgs(int, AntennaBeginEnd) - Constructor for class com.unitech.lib.params.AntennaStatusEventArgs
antennaSwitchingMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The antenna switching mode setting
AntennaSwitchingMode - Enum in com.unitech.lib.uhf.types
  Enum representing the antenna switching modes.
assertAction() - Method in class com.unitech.lib.reader.BaseReader
  Check the device and action state is ready, if not, it will throw ReaderException
assertAction() - Method in class com.unitech.lib.uhf.BaseUHF
  Asserts that the instance is in a state where it can perform an operation.
assertEngineParamId(EngineParamID) - Method in class com.unitech.lib.engine.BaseEngine
  Asserts that the specified EngineParamID is supported by the engine.
assertModule() - Method in class com.unitech.lib.uhf.BaseUHF
  Asserts that the module is not null and is of a type that supports the operation.
authenticate(AuthenticateParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Authenticate command for the RFID UTE module of the Device.
AuthenticateParam - Class in com.unitech.lib.uhf.params
  AuthenticateParam is used to define the parameters for an authentication operation.
AuthenticateParam() - Constructor for class com.unitech.lib.uhf.params.AuthenticateParam
AuthenticationResponse - Enum in com.unitech.lib.uhf.types
  Enum representing the authentication response types.
available() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the length of data that can be read with the read method.
available() - Method in class com.unitech.lib.transport.TransportBluetooth
available() - Method in class com.unitech.lib.transport.TransportUART
available() - Method in class com.unitech.lib.transport.TransportUsb

A B C D E F G H I K L M N O P Q R S T U V W X _