A B C D E F G H I K L M N O P Q R S T U V W X _

## G

getAccessMode() - Method in enum com.unitech.lib.types.DeviceParamID
  Gets the access mode of the device parameter.
getAccessMode() - Method in enum com.unitech.lib.types.UhfParamId
getAccessPassword() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAccessPassword() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAction() - Method in class com.unitech.lib.reader.BaseReader
  Returns the current behavior of the device associated with an instance of the BaseReader class.
getAction() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Action value of "Selection Mask".
getAddress() - Method in class com.unitech.lib.reader.BaseReader
  Returns the address of the device associated with an instance of the BaseReader class.
getAddress() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the address of the device to which the BaseTransport instance is connected.
getAddress() - Method in class com.unitech.lib.transport.TransportUsb
getAlgorithmType() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
getAmbientTemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the ambient temperature of the equipment.
getAmbientTemperatureProtection() - Method in class com.unitech.lib.reader.BaseReader
  Returns the ambient temperature protection setting of the equipment.
getAntennaRoundCount() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna round count of the RFID UTE module of the Device.
getAntennaSwitchingMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Antenna Switching Mode of the RFID UTE module of the Device.
getAutoOffTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time which the instrument automatically turns off.
getAutoOffTimeList() - Method in class com.unitech.lib.reader.BaseReader
  Returns the equipment supports auto off time list, the unit is minutes
getBank() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
getBarcodeId() - Method in class com.unitech.lib.event.params.BarcodeEventArgs
getBarcodeType() - Method in enum com.unitech.lib.engine.types.BarcodeID
  Gets the category of the barcode type.
getBaseEngine() - Method in class com.unitech.lib.reader.BaseReader
  If the BaseReader instance supports the Scanner module, it returns an interface object that can control the Scanner module.
getBatteryState() - Method in class com.unitech.lib.reader.BaseReader
  Returns the battery state of the equipment.
getBatteryStatus() - Method in class com.unitech.lib.reader.BaseReader
  Returns the battery status of the equipment.
getBatteryStatusExtended(BatteryStatusExtendedType[]) - Method in class com.unitech.lib.reader.BaseReader
  Retrieves the battery status of the device.
getBaudRate() - Method in class com.unitech.lib.transport.TransportUART
getBeeper() - Method in class com.unitech.lib.params.DeviceIndicator
getBeeper() - Method in class com.unitech.lib.reader.BaseReader
  Returns the beeper operation status of the equipment.
getBLF() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
getBluetoothAddress() - Method in class com.unitech.lib.reader.BaseReader
  Returns the Bluetooth address of the device.
getBluetoothName() - Method in class com.unitech.lib.reader.BaseReader
  Returns the Bluetooth name of the device.
getCfgStorageMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the configuration storage mode of the RFID UTE module of the Device.
getChargingStatus() - Method in class com.unitech.lib.params.BatteryStatusExtended
getCharPosition() - Method in class com.unitech.lib.reader.params.DisplayOutput
getCheckInterval() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time period for checking the battery status of the device associated with an instance of the BaseReader class.
getCode() - Method in exception com.unitech.lib.diagnostics.ReaderException
  Get fault and motion results.
getCode() - Method in enum com.unitech.lib.engine.types.BarcodeID.BarcodeType
  Gets the byte value of the category.
getCode() - Method in enum com.unitech.lib.engine.types.BarcodeID
  Gets the integer value of the barcode type.
getCode() - Method in enum com.unitech.lib.engine.types.ConnectionIndicator
  Gets the byte value of the connection indicator.
getCode() - Method in enum com.unitech.lib.engine.types.ControlCharacterFilter
  Gets the byte value of the control character filter.
getCode() - Method in enum com.unitech.lib.engine.types.ErrorIndicator
  Gets the byte value of the error indicator.
getCode() - Method in enum com.unitech.lib.engine.types.GoodReadIndicator
  Gets the byte value of the good read indicator.
getCode() - Method in enum com.unitech.lib.engine.types.GS1AI
  Gets the byte value of the GS1 Application Identifier.
getCode() - Method in enum com.unitech.lib.engine.types.HIDInterCharacterDelay
  Gets the byte value of the inter-character delay.
getCode() - Method in enum com.unitech.lib.engine.types.HIDKeyboardCase
  Gets the byte value of the HID keyboard case.
getCode() - Method in enum com.unitech.lib.engine.types.HIDKeyboardLanguage
  Gets the byte value of the HID keyboard language.
getCode() - Method in enum com.unitech.lib.engine.types.PowerOffIndicator
  Gets the byte value of the power off indicator.
getCode() - Method in enum com.unitech.lib.engine.types.PowerOnIndicator
  Gets the byte value of the power on indicator.
getCode() - Method in enum com.unitech.lib.engine.types.SettingIndicator
  Gets the byte value of the setting indicator.
getCode() - Method in enum com.unitech.lib.reader.types.BeeperState
getCode() - Method in enum com.unitech.lib.reader.types.KeyFunction
getCode() - Method in enum com.unitech.lib.reader.types.KeyState
getCode() - Method in enum com.unitech.lib.reader.types.KeyType
getCode() - Method in enum com.unitech.lib.reader.types.NotificationState
getCode() - Method in enum com.unitech.lib.reader.types.VibratorState
getCode() - Method in enum com.unitech.lib.transport.types.ConnectState
getCode() - Method in enum com.unitech.lib.transport.types.ConnectType
getCode() - Method in enum com.unitech.lib.types.AccessMode
  Returns the integer code of the access mode.
getCode() - Method in enum com.unitech.lib.types.ActionState
getCode() - Method in enum com.unitech.lib.types.BatchDataStatus
getCode() - Method in enum com.unitech.lib.types.BatteryState
getCode() - Method in enum com.unitech.lib.types.BatteryStatusExtendedType
getCode() - Method in enum com.unitech.lib.types.BatteryStatusId
getCode() - Method in enum com.unitech.lib.types.BeepAndVibrateState
getCode() - Method in enum com.unitech.lib.types.BeepIndicator
  Gets the byte value of the beep indicator.
getCode() - Method in enum com.unitech.lib.types.ChargingStatus
getCode() - Method in enum com.unitech.lib.types.ConnectionMode
getCode() - Method in enum com.unitech.lib.types.DataCollectionMode
  Gets the byte value of the operation mode.
getCode() - Method in enum com.unitech.lib.types.DataFormat
getCode() - Method in enum com.unitech.lib.types.DataInfo
getCode() - Method in enum com.unitech.lib.types.DataTerminator
getCode() - Method in enum com.unitech.lib.types.DeviceParamID
  Gets the integer value of the device parameter.
getCode() - Method in enum com.unitech.lib.types.DeviceType
getCode() - Method in enum com.unitech.lib.types.EngineModel.EngineVendor
  Gets the integer value of the engine vendor.
getCode() - Method in enum com.unitech.lib.types.EngineModel
  Gets the integer value of the engine model.
getCode() - Method in enum com.unitech.lib.types.EngineParamID
  Gets the integer value of the engine parameter.
getCode() - Method in enum com.unitech.lib.types.EventNotifyId
getCode() - Method in enum com.unitech.lib.types.FindDeviceMode
getCode() - Method in enum com.unitech.lib.types.FirmwareUpdateMode
getCode() - Method in enum com.unitech.lib.types.FirmwareUpdateState
getCode() - Method in interface com.unitech.lib.types.IEnumType
  Get the enum code value
getCode() - Method in enum com.unitech.lib.types.InventoryDataFormat
getCode() - Method in enum com.unitech.lib.types.LEDIndicator
  Gets the byte value of the LED indicator.
getCode() - Method in enum com.unitech.lib.types.ModuleUHFType
getCode() - Method in enum com.unitech.lib.types.ParamType
  Gets the integer value of the parameter type.
getCode() - Method in enum com.unitech.lib.types.ReadMode
getCode() - Method in enum com.unitech.lib.types.ReadOnceState
getCode() - Method in enum com.unitech.lib.types.ResultCode
getCode() - Method in enum com.unitech.lib.types.ScannerDataFormat
getCode() - Method in enum com.unitech.lib.types.SKUType
getCode() - Method in enum com.unitech.lib.uhf.types.AlgorithmType
getCode() - Method in enum com.unitech.lib.uhf.types.AntennaBeginEnd
getCode() - Method in enum com.unitech.lib.uhf.types.AntennaSwitchingMode
getCode() - Method in enum com.unitech.lib.uhf.types.AuthenticationResponse
getCode() - Method in enum com.unitech.lib.uhf.types.BankType
getCode() - Method in enum com.unitech.lib.uhf.types.BLFType
getCode() - Method in enum com.unitech.lib.uhf.types.CfgStorageMode
getCode() - Method in enum com.unitech.lib.uhf.types.Encoding
getCode() - Method in enum com.unitech.lib.uhf.types.FreqSwitchingMode
getCode() - Method in enum com.unitech.lib.uhf.types.GlobalBandType
getCode() - Method in enum com.unitech.lib.uhf.types.IncludeReplyLength
getCode() - Method in enum com.unitech.lib.uhf.types.LockState
getCode() - Method in enum com.unitech.lib.uhf.types.Mask6cAction
getCode() - Method in enum com.unitech.lib.uhf.types.Mask6cTarget
getCode() - Method in enum com.unitech.lib.uhf.types.PowerMode
getCode() - Method in enum com.unitech.lib.uhf.types.PowerSavingMode
getCode() - Method in enum com.unitech.lib.uhf.types.ReadLock
getCode() - Method in enum com.unitech.lib.uhf.types.RFMode
getCode() - Method in enum com.unitech.lib.uhf.types.SelectMaskMode
getCode() - Method in enum com.unitech.lib.uhf.types.SelectMode
getCode() - Method in enum com.unitech.lib.uhf.types.Session
getCode() - Method in enum com.unitech.lib.uhf.types.TagInfoId
getCode() - Method in enum com.unitech.lib.uhf.types.Target
getCode() - Method in enum com.unitech.lib.uhf.types.TARIType
getCode() - Method in enum com.unitech.lib.uhf.types.TemperatureProtectionMode
getCode() - Method in enum com.unitech.lib.uhf.types.Truncate
getCompany() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Company number.
getConfig() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the config of RFID module
getConnection() - Method in class com.unitech.lib.engine.ScannerIndicator
getConnectionMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the connection mode of the device.
getConnectType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the instance of BaseReader associated with device.
getConnectType() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the instance of Transport associated with device.
getContinuousMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns whether the RFID UHF module on the device will cause the Inventory to run continuously.
getControlCharacterFilter() - Method in class com.unitech.lib.reader.BaseReader
  Returns the Control Character Filter setting of the device.
getCount() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get count of GTIN
getCurrent() - Method in class com.unitech.lib.params.BatteryStatusExtended
getCycleCount() - Method in class com.unitech.lib.params.BatteryStatusExtended
getData() - Method in class com.unitech.lib.event.params.BarcodeEventArgs
getData() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access result data value with HEX format.
getDataCollectionMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data collection mode of the device.
getDataFormat() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data format setting of the equipment.
getDataInfo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data info setting of the equipment.
getDataRange() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data range setting of the equipment.
getDataTerminator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the data terminator setting of the equipment.
getDefaultValue() - Method in class com.unitech.lib.params.DeviceParam
  Get the default value of the parameter
getDefaultValue() - Method in class com.unitech.lib.params.EngineParam
  Get the default value of the parameter.
getDesignCapacity() - Method in class com.unitech.lib.params.BatteryStatusExtended
getDeviceName() - Method in class com.unitech.lib.reader.BaseReader
  Returns the name of the Device associated with an instance of the BaseReader class.
getDeviceName() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the name of the Device to which the BaseTransport instance is connected.
getDeviceType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the type of Device to which the instance is connected.
getDeviceType() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the type of device to which the instance will be connected.
getDwellTime() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the dwellTime representing Antenna Setting of the RFID UTE module of the Device.
getEncoding() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
getEngineModel() - Method in class com.unitech.lib.engine.BaseEngine
  Returns the EngineModel of the engine.
getEngineModel() - Method in class com.unitech.lib.reader.BaseReader
  Returns the engine model of the device.
getEngineSupportedParameters() - Static method in class com.unitech.lib.engine.zebra.EngineSE4107
  Returns an array of EngineParam objects that are supported by the engine.
getEngineSupportedParameters() - Static method in class com.unitech.lib.engine.zebra.EngineSE5500
  Returns an array of EngineParam objects that are supported by the engine.
getEngineVersion() - Method in class com.unitech.lib.reader.BaseReader
  Returns the engine version of the device.
getEpc() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get EPC.
getEpc() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  Returns the access tag's EPC value with HEX format.
getEpc() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's EPC value with HEX format.
getError() - Method in class com.unitech.lib.engine.ScannerIndicator
getExtensionDigit() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Extension Digit
getFastID() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the FastId that the RFID UHF module of the appliance uses to read tid when inventory.
getFastMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
getFind() - Method in class com.unitech.lib.params.FindReplace
  Gets the find byte.
getFindReplace() - Method in class com.unitech.lib.reader.BaseReader
  Returns the FindReplace object that contains find and replace settings.
getFixedFreqParams() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the fixed frequency parameters of the RFID UTE module of the Device.
getFreqSwitchingMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Frequency Switching Mode of the RFID UTE module of the Device.
getFrequency() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's frequency value.
getFullChargeCapacity() - Method in class com.unitech.lib.params.BatteryStatusExtended
getGlobalBand() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the national orientation of the RFID UHF module of the instrument.
getGoodRead() - Method in class com.unitech.lib.engine.ScannerIndicator
getGs1Ai() - Method in class com.unitech.lib.reader.BaseReader
  Returns the GS1 Application Identifier (AI) setting of the device.
getGTIN14() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get GTIN
getHealth() - Method in class com.unitech.lib.params.BatteryStatusExtended
getHidInterCharacterDelay() - Method in class com.unitech.lib.reader.BaseReader
  Returns the HID Inter Character Delay setting of the device.
getHidKeyboardCase() - Method in class com.unitech.lib.reader.BaseReader
  Returns the HID Keyboard Case setting of the device.
getHidKeyboardLanguage() - Method in class com.unitech.lib.reader.BaseReader
  Returns the HID Keyboard Language setting of the device.
getId() - Method in class com.unitech.lib.params.DeviceParam
  Gets the ID of the parameter.
getId() - Method in class com.unitech.lib.params.EngineParam
  Gets the ID of the parameter.
getId() - Method in class com.unitech.lib.params.EventNotification
getIdleTime() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument returns the time that the radio waves are not output in the Inventory operation and is resting.
getInventoryDataFormat() - Method in class com.unitech.lib.reader.BaseReader
  Returns the inventory data format of the device.
getInventoryTime() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the time at which radio waves are actually output from the Inventory operation of the RFID UHF module in the instrument.
getItemReference() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Item Reference
getKeyFunction() - Method in class com.unitech.lib.params.TriggerKeyStatus
getKeyFunction(KeyType) - Method in class com.unitech.lib.reader.BaseReader
  Returns the key function for the specified key type.
getKeyType() - Method in class com.unitech.lib.params.TriggerKeyStatus
getKillPassword() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getKillPassword() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getLastError() - Method in class com.unitech.lib.reader.BaseReader
  Returns the result code for the last action.
getLbt() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Listen-Before-Talk Setting of the RFID UTE module of the Device.
getLbtCfgSetting() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the LBT RSSI threshold of the RFID UTE module of the Device.
getLed() - Method in class com.unitech.lib.params.DeviceIndicator
getLedControl() - Method in class com.unitech.lib.reader.BaseReader
  Returns the LED control setting of the device.
getLength() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns the Length of the EPCMaskParam instance.
getLength() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Returns the pattern length of the Mask6cPattern instance.
getLength() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Length value of "Selection Mask".
getLinePosition() - Method in class com.unitech.lib.reader.params.DisplayOutput
getMacAddress() - Method in class com.unitech.lib.transport.BaseTransport
  Returns the MAC address of the device to which the BaseTransport instance is connected.
getManufactureDate() - Method in class com.unitech.lib.params.BatteryStatusExtended
getMax() - Method in class com.unitech.lib.uhf.params.PowerRange
  Returns the maximum Power Gian Level value for a PowerRange instance.
getMaxQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the maximum Q value.
getMaxValue() - Method in class com.unitech.lib.params.EngineParam
  Get the maximum value of the parameter.
getMaxVersion() - Method in class com.unitech.lib.params.BaseParam
  Returns the maximum version that supports the parameter.
getMessage() - Method in class com.unitech.lib.reader.params.DisplayOutput
getMessage() - Method in enum com.unitech.lib.types.ResultCode
  Returns the result code's description.
getMin() - Method in class com.unitech.lib.uhf.params.PowerRange
  Returns the Power Gian Level minimum value for a PowerRange instance.
getMinQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the minimum Q value.
getMinute() - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Returns Minutes.
getMinValue() - Method in class com.unitech.lib.params.EngineParam
  Get the minimum value of the parameter.
getMinVersion() - Method in class com.unitech.lib.params.BaseParam
  Returns the minimum version that supports the parameter.
getMode() - Method in class com.unitech.lib.reader.params.FindDevice
  Returns FindDeviceMode.
getModelNumber() - Method in class com.unitech.lib.params.BatteryStatusExtended
getModuleProfile() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
getOffset() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns the offset of the EPCMaskParam instance.
getOffset() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Offset value of "Selection Mask".
getOperatingMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the operating mode of the device.
getOperatingMode() - Method in class com.unitech.lib.rpx.RP902Reader
getOptions() - Method in class com.unitech.lib.params.DeviceParam
  Get the options of the parameter
getOptions() - Method in class com.unitech.lib.params.EngineParam
  Get a list of options for the parameter.
getParameter(int, EngineParamID, IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Get a specific engine parameter setting.
getParameter(EngineParamID, IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Get a specific engine parameter setting.
getParameter(int, DeviceParamID, IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Get a specific device parameter setting.
getParameter(DeviceParamID, IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Get a specific device parameter setting.
getParameters(int, EngineParamID[], IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Get multiple engine parameter settings.
getParameters(EngineParamID[], IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Get multiple engine parameter settings.
getParameters(int, DeviceParamID[], IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Get multiple device parameter settings.
getParameters(DeviceParamID[], IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Get multiple device parameter settings.
getPATemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the PA temperature of the equipment.
getPATemperatureProtection() - Method in class com.unitech.lib.reader.BaseReader
  Returns the PA temperature protection setting of the equipment.
getPath() - Method in class com.unitech.lib.transport.TransportUART
getPattern() - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Returns Pattern of the EPCMaskParam instance.
getPattern() - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Returns the Mask pattern of the Mask6cPattern instance.
getPattern() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Pattern value of "Selection Mask".
getPC() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's PC value with HEX format.
getPercentage() - Method in class com.unitech.lib.params.BatteryStatus
getPercentage() - Method in class com.unitech.lib.params.BatteryStatusExtended
getPercentage() - Method in class com.unitech.lib.params.FirmwareUpdateEventArgs
getPhaseSetting() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the phase setting of the RFID UTE module of the Device.
getPower() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna output of the RFID UHF module of the instrument.
getPowerAndDutyLimitationMapInfo() - Method in class com.unitech.lib.rgx.RG768Reader
getPowerMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the power mode that the RFID UHF module of the appliance uses to perform the inventory.
getPowerOff() - Method in class com.unitech.lib.engine.ScannerIndicator
getPowerOn() - Method in class com.unitech.lib.engine.ScannerIndicator
getPowerRange() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the antenna output range of the RFID UHF module of the instrument.
getPowerSavingMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the power saving mode of the RFID UHF module of the device.
getPrefiex() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get GTIN prefix
getProtocol() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
getRawData() - Method in class com.unitech.lib.params.BatteryStatusExtended
getRawValue() - Method in class com.unitech.lib.params.DeviceParam
  Get the value with raw byte array format
getReadMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the read mode status of the equipment.
getRemainingCapacity() - Method in class com.unitech.lib.params.BatteryStatusExtended
getReplace() - Method in class com.unitech.lib.params.FindReplace
  Gets the replace byte.
getRfidModuleFirmware() - Method in class com.unitech.lib.reader.BaseReader
  Returns the firmware version of the RFID module.
getRfidModuleSkuType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the SKU type of the RFID module used in the device.
getRfidModuleType() - Method in class com.unitech.lib.reader.BaseReader
  Returns the type of RFID module used in the device.
getRfidUhf() - Method in class com.unitech.lib.reader.BaseReader
  If the BaseReader instance supports the RFID UHF module, it returns an interface object that can control the RFID UHF module.
getRFMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the RF Mode of the RFID UTE module of the Device.
getRssi() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's RSSI value.
getScannerDataFormat() - Method in class com.unitech.lib.reader.BaseReader
  Returns the scanner data format of the device.
getScannerIndicator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the scanner indicator setting of the device.
getScreenOffTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the time which the instrument automatically screen off.
getSecond() - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Returns Seconds.
getSelectMask6c(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cAction(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the comparison behavior of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cBank(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the Device's RFID UHF module returns the memory bank to compare.
getSelectMask6cEnabled(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns whether to use the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cMaxSize() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the max size of select mask list status of the RFID UHF module.
getSelectMask6cOffset(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the Device returns the starting address of the memory to start the comparison.
getSelectMask6cPattern(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the comparison value and length of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cTarget(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Flag of the tag to store the comparison result of Selection Mask item of RFID UHF module of Device.
getSelectMask6cTruncate(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the truncate of the Selection Mask item of the RFID UHF module of the Device.
getSelectMode() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the Select Mode of the RFID UTE module of the Device.
getSerial() - Method in class com.unitech.lib.tagcoder.SGTIN
  Get Serial number
getSerialNo() - Method in class com.unitech.lib.reader.BaseReader
  Returns the serial number of the device.
getSerialNumber() - Method in class com.unitech.lib.params.BatteryStatusExtended
getSession() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the device returns the Session to check the state of the Session of the tag to be read by the Inventory operation.
getSetting() - Method in class com.unitech.lib.engine.ScannerIndicator
getSettingByLabel() - Method in class com.unitech.lib.reader.BaseReader
  Returns whether the device settings are applied by label.
getSKU() - Method in class com.unitech.lib.reader.BaseReader
  Returns the SKU type of the equipment.
getSKU() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the SKU of the RFID UTE module of the Device.
getStartQ() - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, it returns the starting Q value.
getState() - Method in class com.unitech.lib.params.BatteryStatus
getState() - Method in class com.unitech.lib.params.FirmwareUpdateEventArgs
getState() - Method in class com.unitech.lib.reader.BaseReader
  Returns the connection status of the device with the instance of the BaseReader class.
getState() - Method in class com.unitech.lib.transport.BaseTransport
  The instance of BaseTransport returns the connection status with device.
getSupportedParameterIds() - Method in class com.unitech.lib.engine.BaseEngine
  Returns an array of EngineParamID objects that are supported by the engine.
getSupportedParameterIds() - Method in class com.unitech.lib.reader.BaseReader
  Gets the supported parameter IDs of the device.
getSupportedParameterIds(DeviceType) - Static method in class com.unitech.lib.reader.BaseReader
  Gets the supported parameter IDs of the device based on the specified device type.
getSupportedParameters() - Method in class com.unitech.lib.engine.BaseEngine
  Returns an array of EngineParam objects that are supported by the engine.
getSupportedParameters() - Method in class com.unitech.lib.reader.BaseReader
  Gets the supported parameters of the device.
getSupportedParameters(DeviceType) - Static method in class com.unitech.lib.reader.BaseReader
  Gets the supported parameters of the device based on the specified device type.
getTagFocus() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the TagFocus Setting of the RFID UTE module of the Device.
getTarget() - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the device returns the status of the Target of the tag to be read by the Inventory operation.
getTarget() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Target Flag of "Selection Mask".
getTARI() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
getTemperature() - Method in class com.unitech.lib.params.BatteryStatusExtended
getTemperature() - Method in class com.unitech.lib.reader.BaseReader
  Returns the temperature of the equipment.
getTemperatureProtectionMode() - Method in class com.unitech.lib.reader.BaseReader
  Returns the temperature protection mode of the equipment.
getTid() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'TID memory'.
getTid() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'TID memory'.
getTID() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's TID value with HEX format.
getTime() - Method in class com.unitech.lib.reader.BaseReader
  Returns the system time of the device.
getTimeout() - Method in class com.unitech.lib.reader.params.FindDevice
  Returns timeout value.
getTimestamp() - Method in class com.unitech.lib.event.params.BarcodeEventArgs
getToggleTarget() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
getTransport() - Method in class com.unitech.lib.reader.BaseReader
  Returns an instance of the BaseTransport class that connects an instance of the BaseReader class to the Device.
getTruncate() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns the Truncate value of "Selection Mask".
getType() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the RFID UHF module type of the connected Device.
getUsbPermission() - Method in class com.unitech.lib.reader.DetectReader
getUser() - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getUser() - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getUserData() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the user data value with HEX format.
getValue() - Method in class com.unitech.lib.params.DeviceParam
  Get the value of the parameter
getValue() - Method in class com.unitech.lib.params.EngineParam
  Gets the value of the parameter.
getVendor() - Method in enum com.unitech.lib.types.EngineModel
  Gets the vendor of the engine model.
getVersion() - Method in class com.unitech.lib.engine.BaseEngine
  Returns the version of the engine as a string.
getVersion() - Method in class com.unitech.lib.reader.BaseReader
  Returns the firmware version of the device associated with the instance of the BaseReader class.
getVersion() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the version of the RFID UHF module.
getVibrator() - Method in class com.unitech.lib.reader.BaseReader
  Returns the vibrator operation status of the equipment.
getVoltage() - Method in class com.unitech.lib.params.BatteryStatusExtended
getXPC() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the XPC value with HEX format.
GlobalBandTable - Class in com.unitech.lib.uhf.params
GlobalBandTable() - Constructor for class com.unitech.lib.uhf.params.GlobalBandTable
GlobalBandType - Enum in com.unitech.lib.uhf.types
  The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.
GoodReadIndicator - Enum in com.unitech.lib.engine.types
  The GoodReadIndicator enum represents different types of good read indicators.
GS1AI - Enum in com.unitech.lib.engine.types
  The GS1AI enum represents different types of GS1 Application Identifiers.

A B C D E F G H I K L M N O P Q R S T U V W X _