A B C D E F G H I K L M N O P Q R S T U V W X _

## I

IBarcodeEventListener - Interface in com.unitech.lib.event
  Interface for classes that subscribe to barcode events.
idleTime - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The idle time setting
IEnumType - Interface in com.unitech.lib.types
  The IEnumType interface provides the common functionality of all enumerations that the SDK uses.
IncludeReplyLength - Enum in com.unitech.lib.uhf.types
  Enum representing the inclusion of reply length in a response.
incRepLen - Variable in class com.unitech.lib.uhf.params.AuthenticateParam
INFO - Static variable in class com.unitech.lib.transport.BaseTransport
initModule() - Method in class com.unitech.lib.uhf.BaseUHF
  After the Device is connected, it calls to instantiate the BaseUHF instance.
initReader() - Method in class com.unitech.lib.eax.EA530Reader
initReader() - Method in class com.unitech.lib.htx.HT730Reader
initReader() - Method in class com.unitech.lib.pax.PA768eReader
initReader() - Method in class com.unitech.lib.reader.BaseReader
  Initializes an BaseReader instance after the BaseReader instance is associated with the device.
initReader() - Method in class com.unitech.lib.rgx.RG768Reader
initReader() - Method in class com.unitech.lib.rpx.RP300Reader
initReader() - Method in class com.unitech.lib.rpx.RP902Reader
interferer - Variable in class com.unitech.lib.params.LBTStatusEventArgs
inventory6c() - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to inventory the RFID UHF tag of ISO18000-6c Gen2 standard.
InventoryDataFormat - Enum in com.unitech.lib.types
  The InventoryDataFormat enumeration represents the different formats of inventory data that can be used in RFID operations.
inventoryTime - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The inventory time setting
IO - Static variable in class com.unitech.lib.transport.BaseTransport
IParameterEventListener - Interface in com.unitech.lib.event
  Interface for classes that subscribe to parameter events.
IReaderEventListener - Interface in com.unitech.lib.reader.event
  IReaderEventListener is an interface that defines methods to handle various events related to a BaseReader instance.
IRfidEventListener - Interface in com.unitech.lib.event
  Interface for handling RFID events related to tag access and reading.
isCharging() - Method in class com.unitech.lib.params.BatteryStatus
isClearScreen() - Method in class com.unitech.lib.reader.params.DisplayOutput
isContains(BarcodeInfoId) - Method in class com.unitech.lib.event.params.BarcodeEventArgs
  Checks if the BarcodeInfoId is contained in the barcodeInfoIds array.
isContains(BatteryStatusId) - Method in class com.unitech.lib.params.BatteryStatus
  Checks if the BatteryStatus contains a specific BatteryStatusId.
isContains(UhfParamId) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Checks if the RFIDConfig contains a specific parameter.
isContains(TagInfoId) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Checks if the tag information contains a specific TagInfoId.
isEnable() - Method in class com.unitech.lib.params.EventNotification
isForceToUsb() - Method in class com.unitech.lib.transport.TransportUsb
  Returns the flag indicating whether the transport is forced to USB.
isUsed() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Returns whether or not "Selection Mask" is enabled.
isVibrator() - Method in class com.unitech.lib.params.DeviceIndicator

A B C D E F G H I K L M N O P Q R S T U V W X _