A B C D E F G H I K L M N O P Q R S T U V W X _

## C

CfgStorageMode - Enum in com.unitech.lib.uhf.types
  Enum representing the configuration storage modes.
changeState(ConnectState, Object) - Method in class com.unitech.lib.transport.TransportUART
ChargingStatus - Enum in com.unitech.lib.types
  ChargingStatus enum represents the different states of charging in a device.
checkBufferSize(int) - Method in class com.unitech.lib.transport.BaseTransport
checkError() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
checkLength(int) - Method in class com.unitech.lib.tagcoder.SGTIN
  Check if the EPC length matches the SGTIN-96 or SGTIN-198 format.
clear() - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Initializes the values set in the SelectMask6cParam instance.
clearListener() - Method in class com.unitech.lib.reader.BaseReader
  Removes all listeners registered on an instance of the BaseReader class.
clearListener() - Method in class com.unitech.lib.uhf.BaseUHF
  Removes all event handlers from the instance.
com.unitech.lib.diagnostics - package com.unitech.lib.diagnostics
com.unitech.lib.eax - package com.unitech.lib.eax
com.unitech.lib.engine - package com.unitech.lib.engine
com.unitech.lib.engine.types - package com.unitech.lib.engine.types
com.unitech.lib.engine.zebra - package com.unitech.lib.engine.zebra
com.unitech.lib.event - package com.unitech.lib.event
com.unitech.lib.event.params - package com.unitech.lib.event.params
com.unitech.lib.htx - package com.unitech.lib.htx
com.unitech.lib.params - package com.unitech.lib.params
com.unitech.lib.pax - package com.unitech.lib.pax
com.unitech.lib.reader - package com.unitech.lib.reader
com.unitech.lib.reader.event - package com.unitech.lib.reader.event
com.unitech.lib.reader.params - package com.unitech.lib.reader.params
com.unitech.lib.reader.types - package com.unitech.lib.reader.types
com.unitech.lib.rgx - package com.unitech.lib.rgx
com.unitech.lib.rpx - package com.unitech.lib.rpx
com.unitech.lib.tagcoder - package com.unitech.lib.tagcoder
com.unitech.lib.transport - package com.unitech.lib.transport
com.unitech.lib.transport.types - package com.unitech.lib.transport.types
com.unitech.lib.types - package com.unitech.lib.types
com.unitech.lib.uhf - package com.unitech.lib.uhf
com.unitech.lib.uhf.params - package com.unitech.lib.uhf.params
com.unitech.lib.uhf.types - package com.unitech.lib.uhf.types
connect() - Method in class com.unitech.lib.eax.EA530Reader
connect() - Method in class com.unitech.lib.htx.HT730pReader
connect() - Method in class com.unitech.lib.htx.HT730Reader
connect() - Method in class com.unitech.lib.pax.PA768eReader
connect() - Method in class com.unitech.lib.reader.BaseReader
  An instance of the BaseReader class tries to connect to the configured address
connect() - Method in class com.unitech.lib.rgx.RG768Reader
connect() - Method in class com.unitech.lib.rpx.RP300Reader
connect() - Method in class com.unitech.lib.transport.BaseTransport
  Attempts to connect to the appliance using an instance of the Transport class.
connect() - Method in class com.unitech.lib.transport.TransportBluetooth
connect() - Method in class com.unitech.lib.transport.TransportUART
connect() - Method in class com.unitech.lib.transport.TransportUsb
ConnectionIndicator - Enum in com.unitech.lib.engine.types
  The ConnectionIndicator enum represents different types of connection indicators.
ConnectionMode - Enum in com.unitech.lib.types
  ConnectionMode enum represents the different modes of connection available for a device.
ConnectState - Enum in com.unitech.lib.transport.types
  The ConnectState enumeration indicates the connection status of the BaseTransport instance.
ConnectType - Enum in com.unitech.lib.transport.types
  The ConnectType enumeration indicates which communication method the BaseTransport instance uses in its connection with the appliance.
continuousMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The continuous mode setting
ControlCharacterFilter - Enum in com.unitech.lib.engine.types
  The ControlCharacterFilter enum represents different types of control character filters.
convertVersion(String) - Method in class com.unitech.lib.engine.BaseEngine
  Convert the engine version string to an integer.
copy(SelectMask6cParam) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Copy the SelectMask6cParam instance.
csi - Variable in class com.unitech.lib.uhf.params.AuthenticateParam
cwOnOff(CWParms, boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the CW On/Off command for the RFID UTE module of the Device.
CWParms - Class in com.unitech.lib.uhf.params
  CWParms is a class that represents the parameters for Continuous Wave (CW) mode in RFID operations.
CWParms() - Constructor for class com.unitech.lib.uhf.params.CWParms

A B C D E F G H I K L M N O P Q R S T U V W X _