A B C D E F G H I K L M N O P Q R S T U V W X _

## B

bankType() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access bank type.
BankType - Enum in com.unitech.lib.uhf.types
  The BankType enumeration specifies the memory bank of the RFID UHF tag.
BarcodeEventArgs - Class in com.unitech.lib.event.params
  Encapsulates the data associated with a barcode event.
BarcodeEventArgs() - Constructor for class com.unitech.lib.event.params.BarcodeEventArgs
BarcodeEventArgs(BarcodeID, byte[], Date) - Constructor for class com.unitech.lib.event.params.BarcodeEventArgs
  Constructs a new BarcodeEventArgs object.
BarcodeID - Enum in com.unitech.lib.engine.types
  The BarcodeID enum represents different types of barcodes.
BarcodeID.BarcodeType - Enum in com.unitech.lib.engine.types
  The BarcodeType enum represents categories of barcode types.
BarcodeInfoId - Enum in com.unitech.lib.engine.types
  Enumeration representing different barcode information IDs.
barcodeInfoIds - Variable in class com.unitech.lib.event.params.BarcodeEventArgs
  An array of BarcodeInfoId that contains information about the barcode event.
BaseEngine - Class in com.unitech.lib.engine
  Provides the base functionality for interacting with a barcode reader engine.
BaseEngine(IReader, EngineModel) - Constructor for class com.unitech.lib.engine.BaseEngine
  Constructs a new BaseEngine object.
BaseParam - Class in com.unitech.lib.params
  The BaseParam class is a base class for DeviceParam and EngineParam.
BaseParam(ParamType) - Constructor for class com.unitech.lib.params.BaseParam
  Constructs a new BaseParam object.
BaseReader - Class in com.unitech.lib.reader
  The BaseReader class is a class that controls device in connection with unitech's equipment, receives data from device, and delivers it to the application program.
BaseReader(BaseTransport) - Constructor for class com.unitech.lib.reader.BaseReader
  Creates an instance of BaseReader.
BaseTransport - Class in com.unitech.lib.transport
  The Transport class is a class for abstracting connections with Reader devices.
BaseTransport() - Constructor for class com.unitech.lib.transport.BaseTransport
  Create an instance of the Transport class
BaseTransport(DeviceType, String, String) - Constructor for class com.unitech.lib.transport.BaseTransport
  Create an instance of the Transport class
BaseTransport(DeviceType, String, String, String) - Constructor for class com.unitech.lib.transport.BaseTransport
  Create an instance of the Transport class
BaseUHF - Class in com.unitech.lib.uhf
  BaseUHF class is a class that provides the function to control RFID UHF module installed in Device when BaseReader instance is connected to Device.
BaseUHF(IReader) - Constructor for class com.unitech.lib.uhf.BaseUHF
  Create an instance of the BaseUHF class.
BatchDataStatus - Enum in com.unitech.lib.types
  Enum representing the status of batch data in a RFID system.
BatteryState - Enum in com.unitech.lib.types
  BatteryState enum represents the different states of a battery.
BatteryStatus - Class in com.unitech.lib.params
  Represents the battery status of a device.
BatteryStatus() - Constructor for class com.unitech.lib.params.BatteryStatus
BatteryStatus(BatteryState) - Constructor for class com.unitech.lib.params.BatteryStatus
BatteryStatus(int) - Constructor for class com.unitech.lib.params.BatteryStatus
BatteryStatus(int, boolean) - Constructor for class com.unitech.lib.params.BatteryStatus
BatteryStatusExtended - Class in com.unitech.lib.params
  Represents the extended battery status of a device.
BatteryStatusExtended(BatteryStatusExtendedType[]) - Constructor for class com.unitech.lib.params.BatteryStatusExtended
BatteryStatusExtended(BatteryStatusExtendedType[], byte[]) - Constructor for class com.unitech.lib.params.BatteryStatusExtended
BatteryStatusExtended(int, byte[]) - Constructor for class com.unitech.lib.params.BatteryStatusExtended
BatteryStatusExtendedType - Enum in com.unitech.lib.types
  The BatteryStatusExtendedType enum represents the extended types of battery status.
BatteryStatusId - Enum in com.unitech.lib.types
  BatteryStatusId enum represents the different types of battery status identifiers.
batteryStatusIds - Variable in class com.unitech.lib.params.BatteryStatus
BeepAndVibrateState - Enum in com.unitech.lib.types
  The BeepAndVibrateState enumeration represents the type of device associated with the SDK.
BeeperState - Enum in com.unitech.lib.reader.types
  Indicates the beeper status of equipment that supports Beeper.
BeepIndicator - Enum in com.unitech.lib.types
  The BeepIndicator enum represents different beep indicators for a scanner.
bitLength - Variable in class com.unitech.lib.uhf.params.MarginReadParam
blfType - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The BLF setting, only for RP902
BLFType - Enum in com.unitech.lib.uhf.types
  The BLFType enumeration represents the BLF by which the RFID UHF module inventories the TAG.
blockPermaLock(BlockPermaLockParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Block Perma Lock command for the RFID UTE module of the Device.
BlockPermaLockParam - Class in com.unitech.lib.uhf.params
  BlockPermaLockParam is used to define the parameters for a block permanent lock operation.
BlockPermaLockParam() - Constructor for class com.unitech.lib.uhf.params.BlockPermaLockParam

A B C D E F G H I K L M N O P Q R S T U V W X _