A B C D E F G H I K L M N O P Q R S T U V W X _

## P

PA768eReader - Class in com.unitech.lib.pax
  The PA768eReader class provides methods to connect and interact with the PA768e RFID reader.
PA768eReader(Context) - Constructor for class com.unitech.lib.pax.PA768eReader
parameter - Variable in class com.unitech.lib.reader.params.DisplayOutput
  The parameter for the display output
ParamType - Enum in com.unitech.lib.types
  The ParamType enum represents different types of parameters.
pattern - Variable in class com.unitech.lib.uhf.params.MarginReadParam
pc() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the tag's PC value.
permaLock6c(PermaLock6cParam, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to permanent lock or unlock the RFID UHF tags of the ISO18000-6c Gen2 standard.
PermaLock6cParam - Class in com.unitech.lib.uhf.params
  The PermaLock6cParam class is used to pass information pertaining to RFID UHF's PermaLock command.
PermaLock6cParam() - Constructor for class com.unitech.lib.uhf.params.PermaLock6cParam
  Creates an instance of the PermaLock6cParam class.
PermaLock6cParam(LockState, LockState, LockState, LockState, LockState) - Constructor for class com.unitech.lib.uhf.params.PermaLock6cParam
  Creates an instance of the PermaLock6cParam class.
phaseBegin() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the phase begin value.
phaseEnd() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the phase end value.
power - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The antenna power setting
powerCtrl(boolean) - Method in class com.unitech.lib.eax.EA530Reader
powerCtrl(boolean) - Method in class com.unitech.lib.htx.HT730pReader
powerCtrl(boolean) - Method in class com.unitech.lib.pax.PA768eReader
PowerMode - Enum in com.unitech.lib.uhf.types
  The PowerMode enumeration specifies the power mode while inventory.
PowerOffIndicator - Enum in com.unitech.lib.engine.types
  The PowerOffIndicator enum represents different types of power off indicators.
PowerOnIndicator - Enum in com.unitech.lib.engine.types
  The PowerOnIndicator enum represents different types of power on indicators.
PowerRange - Class in com.unitech.lib.uhf.params
  The PowerRange class is a class that represents the setting range of the power gain level of an RFID UHF antenna.
PowerRange() - Constructor for class com.unitech.lib.uhf.params.PowerRange
  Create an instance of the PowerRange class.
PowerRange(int, int) - Constructor for class com.unitech.lib.uhf.params.PowerRange
  Create an instance of the PowerRange class.
powerSavingMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The power saving mode setting
PowerSavingMode - Enum in com.unitech.lib.uhf.types
  Enum representing the power saving modes for the UHF device.
pumpEvent(ProtocolEventArgs) - Method in class com.unitech.lib.engine.BaseEngine
  Handles protocol events.
pumpEvent(ProtocolEventId, Object) - Method in class com.unitech.lib.uhf.BaseUHF

A B C D E F G H I K L M N O P Q R S T U V W X _