A B C D E F G H I K L M N O P Q R S T U V W X _

## F

factoryReset() - Method in class com.unitech.lib.reader.BaseReader
  Reset the device to factory default.
fastID - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The fast id setting(read tid)
fastMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The fast mode setting, only for RP902
FindDevice - Class in com.unitech.lib.reader.params
  The FindDevice class stores information about the find device setting.
FindDevice() - Constructor for class com.unitech.lib.reader.params.FindDevice
FindDevice(FindDeviceMode, int) - Constructor for class com.unitech.lib.reader.params.FindDevice
FindDeviceMode - Enum in com.unitech.lib.types
  The FindDeviceMode enumeration represents the type of device associated with the SDK.
FindReplace - Class in com.unitech.lib.params
  The FindReplace class represents a find and replace operation.
FindReplace() - Constructor for class com.unitech.lib.params.FindReplace
  Constructs a new FindReplace object with default find and replace bytes (0x00).
FindReplace(byte, byte) - Constructor for class com.unitech.lib.params.FindReplace
  Constructs a new FindReplace object with the specified find and replace bytes.
firmwareUpdate(String, byte[]) - Method in class com.unitech.lib.reader.BaseReader
  Performs a firmware update on the device.
FirmwareUpdateEventArgs - Class in com.unitech.lib.params
  FirmwareUpdateEventArgs is a class that encapsulates the state and progress of a firmware update.
FirmwareUpdateEventArgs(FirmwareUpdateState, int) - Constructor for class com.unitech.lib.params.FirmwareUpdateEventArgs
FirmwareUpdateMode - Enum in com.unitech.lib.types
FirmwareUpdateState - Enum in com.unitech.lib.types
  FirmwareUpdateState represents the various states of a firmware update process.
freqSwitchingMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The frequency switching mode setting
FreqSwitchingMode - Enum in com.unitech.lib.uhf.types
  Enum representing the frequency switching modes.
frequency - Variable in class com.unitech.lib.params.LBTStatusEventArgs
fromName(String) - Static method in enum com.unitech.lib.types.DeviceType
  Returns the enum constant of this type with the specified name.
fromName(String) - Static method in enum com.unitech.lib.types.EngineModel.EngineVendor
  Gets an engine vendor from its name.
fromName(String) - Static method in enum com.unitech.lib.types.EngineModel
  Gets an engine model from its name.
fromValue(byte) - Static method in enum com.unitech.lib.engine.types.BarcodeID.BarcodeType
  Gets a category from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.BarcodeID
  Gets a barcode type from its integer value.
fromValue(byte) - Static method in enum com.unitech.lib.engine.types.ConnectionIndicator
  Gets a connection indicator from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.ControlCharacterFilter
  Gets a control character filter from its byte value.
fromValue(byte) - Static method in enum com.unitech.lib.engine.types.ErrorIndicator
  Gets an error indicator from its byte value.
fromValue(byte) - Static method in enum com.unitech.lib.engine.types.GoodReadIndicator
  Gets a good read indicator from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.GS1AI
  Gets a GS1 Application Identifier from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.HIDInterCharacterDelay
  Gets an inter-character delay from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.HIDKeyboardCase
  Gets a HID keyboard case from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.HIDKeyboardLanguage
  Gets a HID keyboard language from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.PowerOffIndicator
  Gets a power off indicator from its byte value.
fromValue(byte) - Static method in enum com.unitech.lib.engine.types.PowerOnIndicator
  Gets a power on indicator from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.engine.types.SettingIndicator
  Gets a setting indicator from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.reader.types.KeyFunction
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.reader.types.KeyType
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.types.AccessMode
  Returns the AccessMode enum corresponding to the given integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.BatchDataStatus
fromValue(int) - Static method in enum com.unitech.lib.types.BatteryState
fromValue(int) - Static method in enum com.unitech.lib.types.BatteryStatusExtendedType
fromValue(int) - Static method in enum com.unitech.lib.types.BatteryStatusId
fromValue(byte) - Static method in enum com.unitech.lib.types.BeepIndicator
  Gets a beep indicator from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.types.BeepIndicator
  Gets a beep indicator from its integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.ChargingStatus
fromValue(int) - Static method in enum com.unitech.lib.types.ConnectionMode
fromValue(int) - Static method in enum com.unitech.lib.types.DataCollectionMode
  Gets an operation mode from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.types.DeviceParamID
  Gets a device parameter from its integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.EngineModel.EngineVendor
  Gets an engine vendor from its integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.EngineModel
  Gets an engine model from its integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.EngineParamID
  Gets an engine parameter from its integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.InventoryDataFormat
  Returns the InventoryDataFormat corresponding to the given code.
fromValue(byte) - Static method in enum com.unitech.lib.types.LEDIndicator
  Gets an LED indicator from its byte value.
fromValue(int) - Static method in enum com.unitech.lib.types.LEDIndicator
  Gets an LED indicator from its integer value.
fromValue(int) - Static method in enum com.unitech.lib.types.ScannerDataFormat
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.AuthenticationResponse
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.ESMode
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.Gen2xAppSize
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.Gen2xCode
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.Gen2xCr
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.Gen2xCrypto
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.Gen2xId
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.Gen2xProtection
  Returns the enum constant of this type with the specified code.
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.IncludeReplyLength
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.ReadLock
fromValue(int) - Static method in enum com.unitech.lib.uhf.types.TemperatureProtectionMode
  Returns the enum constant of this type with the specified code.

A B C D E F G H I K L M N O P Q R S T U V W X _