A B C D E F G H I K L M N O P Q R S T U V W X _

## S

ScannerDataFormat - Enum in com.unitech.lib.types
  The ScannerDataFormat enum represents the different data formats that a scanner can use.
ScannerIndicator - Class in com.unitech.lib.engine
  The ScannerIndicator class represents the status indicators of a scanner.
ScannerIndicator(GoodReadIndicator, ConnectionIndicator, SettingIndicator, ErrorIndicator, PowerOnIndicator, PowerOffIndicator) - Constructor for class com.unitech.lib.engine.ScannerIndicator
ScreenOffTime - Class in com.unitech.lib.reader.params
  The ScreenOffTime class stores information about the screen off setting.
ScreenOffTime() - Constructor for class com.unitech.lib.reader.params.ScreenOffTime
ScreenOffTime(int, int) - Constructor for class com.unitech.lib.reader.params.ScreenOffTime
sdata - Variable in class com.unitech.lib.reader.params.DisplayOutput
SelectMask6cParam - Class in com.unitech.lib.uhf.params
  The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
SelectMask6cParam() - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, String, int) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, <any>) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, String, int, Truncate) - Constructor for class com.unitech.lib.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMaskMode - Enum in com.unitech.lib.uhf.types
selectMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The select mode setting
SelectMode - Enum in com.unitech.lib.uhf.types
  The SelectMode enumeration represents the selection mode of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
sendFwFileData(byte[]) - Method in class com.unitech.lib.htx.HT730pReader
sendFwFileData(byte[]) - Method in class com.unitech.lib.pax.PA768eReader
senRep - Variable in class com.unitech.lib.uhf.params.AuthenticateParam
session - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The Session setting
Session - Enum in com.unitech.lib.uhf.types
  The Session enumeration represents the session of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAccessPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAction(ActionState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operational state of the device associated with the instance.
setAction(Mask6cAction) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
setAddress(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the address of the device to which the instance of BaseReader is connected.
setAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the address of the device to which the BaseTransport instance is connected.
setAlgorithm(AlgorithmType) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the algorithm type for the RFID module.
setAlgorithmType(AlgorithmType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
setAmbientTemperatureProtection(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the ambient temperature protection setting of the equipment.
setAntenna(short) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the antenna identifier associated with the tag
setAntennaRoundCount(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the antenna round count of the RFID UTE module of the Device.
setAntennaSwitchingMode(AntennaSwitchingMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Antenna Switching Mode of the RFID UTE module of the Device.
setAntennaSwitchingMode(AntennaSwitchingMode) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the antenna switching mode for the RFID module.
setAutoOffTime(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time which the equipment automatically turns off.
setBank(BankType) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Bank value in "Selection Mask".
setBarcodeEventListener(IBarcodeEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Sets the barcode event listener for the BaseReader instance.
setBarcodeID(BarcodeID) - Method in class com.unitech.lib.event.params.BarcodeEventArgs
setBeeper(BeepIndicator) - Method in class com.unitech.lib.params.DeviceIndicator
setBeeper(BeeperState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the beeper operation status of the equipment.
setBLF(BLFType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the BLF that the RFID UHF module of the appliance uses to perform the inventory.
setBlfType(BLFType) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the BLF type for the RFID module.
setBluetoothSecuritySimplePairing(boolean) - Method in class com.unitech.lib.reader.BaseReader
  Sets whether Bluetooth Security Simple Pairing is enabled.
setCfgStorageMode(CfgStorageMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the configuration storage mode of the RFID UTE module of the Device.
setCharging(boolean) - Method in class com.unitech.lib.params.BatteryStatus
setCharPosition(byte) - Method in class com.unitech.lib.reader.params.DisplayOutput
setCheckInterval(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time period for checking the battery status of the device associated with the BaseReader class instance.
setClearScreen(boolean) - Method in class com.unitech.lib.reader.params.DisplayOutput
setConfig(RFIDConfig) - Method in class com.unitech.lib.uhf.BaseUHF
  Setup the config of the RFID module
setConnection(ConnectionIndicator) - Method in class com.unitech.lib.engine.ScannerIndicator
setConnectionMode(ConnectionMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the connection mode of the device.
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets whether or not the RFID UHF module of the device will run the Inventory continuously.
setContinuousMode(boolean) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the continuous mode.
setControlCharacterFilter(ControlCharacterFilter) - Method in class com.unitech.lib.reader.BaseReader
  Sets the Control Character Filter setting of the device.
setCurrentValue(Object) - Method in class com.unitech.lib.params.DeviceParam
  Set the value of the parameter without checking the access mode.
setData(byte[]) - Method in class com.unitech.lib.event.params.BarcodeEventArgs
setDataCollectionMode(DataCollectionMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data collection mode of the device.
setDataDisplayMode(DataDisplayMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data display mode of the device.
setDataDisplayTime(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data display time of the device.
setDataFormat(DataFormat) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data format setting of the equipment.
setDataInfo(DataInfo) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data info setting of the equipment.
setDataRange(DataRange) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data range setting of the equipment.
setDataTerminator(DataTerminator) - Method in class com.unitech.lib.reader.BaseReader
  Sets the data terminator setting of the equipment.
setDeviceIndicator(DeviceIndicator) - Method in class com.unitech.lib.reader.BaseReader
  Sets the device indicator for the device.
setDeviceName(String) - Method in class com.unitech.lib.reader.BaseReader
  Sets the name of the device to which the instance of BaseReader is connected.
setDeviceName(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the name of the device to which the BaseTransport instance is connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.reader.BaseReader
  Sets the type of device to which instance of BaseReader will be connected.
setDeviceType(DeviceType) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the type of device to which the instance will be connected.
setDisplayOutput(DisplayOutput) - Method in class com.unitech.lib.reader.BaseReader
  Sets the display output setting of the equipment.
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.reader.BaseReader
  Returns the display tags of the device.
setDisplayTags(DisplayTags) - Method in class com.unitech.lib.rpx.RP902Reader
setDwellTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the dwellTime representing Antenna Setting of the RFID UTE module of the Device.
setDwellTime(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the dwell time for the RFID module.
setEnable(boolean) - Method in class com.unitech.lib.params.EventNotification
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the encoding that the RFID UHF module of the appliance uses to perform the inventory.
setEncoding(Encoding) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the encoding for the RFID module.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setEpc(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setEpc(byte[]) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the tag's EPC value.
setError(ErrorIndicator) - Method in class com.unitech.lib.engine.ScannerIndicator
setErrSuppressMode(ESMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Error Suppression Mode of the RFID UTE module of the Device.
setException(ReaderException) - Method in class com.unitech.lib.uhf.BaseUHF
setFastID(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Setup the status of the FastId that the RFID UHF module of the appliance uses to read tid when inventory.
setFastID(boolean) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the fast ID (read TID) setting for the RFID module.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the fast mode that the RFID UHF module of the appliance uses to perform the inventory.
setFastMode(boolean) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the fast mode for the RFID module.
setFind(byte) - Method in class com.unitech.lib.params.FindReplace
  Sets the find byte.
setFindDevice(FindDevice) - Method in class com.unitech.lib.reader.BaseReader
  Sets the find device status of the equipment.
setFindReplace(FindReplace) - Method in class com.unitech.lib.reader.BaseReader
  Sets the FindReplace object that contains find and replace settings.
setFixedFreqParams(long[]) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the fixed frequency parameters of the RFID UTE module of the Device.
setFreqSwitchingMode(FreqSwitchingMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Frequency Switching Mode of the RFID UTE module of the Device.
setFreqSwitchingMode(FreqSwitchingMode) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the frequency switching mode for the RFID module.
setFrequency(int) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the tag's frequency value.
setGen2xScan(Gen2XScanSetting) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the gen2x scan for the RFID module.
setGen2xScanId(Gen2XScanIdSetting) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the gen2x scanId for the RFID module
setGen2XScanIdSetting(Gen2XScanIdSetting) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Gen2X ScanID Command Control Setting of the RFID UTE module of the Device.
setGen2XScanSetting(Gen2XScanSetting) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Gen2X Scan Command Control Setting of the RFID UTE module of the Device.
setGlobalBand(GlobalBandType) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the national orientation of the RFID UHF module of the instrument.
setGoodRead(GoodReadIndicator) - Method in class com.unitech.lib.engine.ScannerIndicator
setGs1Ai(GS1AI) - Method in class com.unitech.lib.reader.BaseReader
  Sets the GS1 Application Identifier (AI) setting of the device.
setHidInterCharacterDelay(HIDInterCharacterDelay) - Method in class com.unitech.lib.reader.BaseReader
  Sets the HID Inter Character Delay setting of the device.
setHidKeyboardCase(HIDKeyboardCase) - Method in class com.unitech.lib.reader.BaseReader
  Sets the HID Keyboard Case setting of the device.
setHidKeyboardLanguage(HIDKeyboardLanguage) - Method in class com.unitech.lib.reader.BaseReader
  Sets the HID Keyboard Language setting of the device.
setId(EventNotifyId) - Method in class com.unitech.lib.params.EventNotification
setIdleTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  The RFID UHF module of the instrument sets the time for which the radio waves are not output in the Inventory operation and the rest of the time.
setIdleTime(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the idle time for the RFID module.
setInventoryDataFormat(InventoryDataFormat[]) - Method in class com.unitech.lib.reader.BaseReader
  Sets the inventory data format of the device.
setInventoryTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the time at which radio waves are actually output in Inventory operation of the RFID UHF module of the instrument.
setInventoryTime(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the inventory time for the RFID module.
setKeyFunction(KeyFunction) - Method in class com.unitech.lib.params.TriggerKeyStatus
setKeyFunction(TriggerKeyStatus) - Method in class com.unitech.lib.reader.BaseReader
  Sets the key function for the specified trigger key status.
setKeyType(KeyType) - Method in class com.unitech.lib.params.TriggerKeyStatus
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setKillPassword(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setLastError(ResultCode) - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
setLbt(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Listen-Before-Talk Setting of the RFID UTE module of the Device.
setLbt(boolean) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the lbt (Listen Before Talk) setting for the RFID module.
setLbtCfgSetting(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the LBT RSSI threshold of RAM/Flash for the Device.
setLbtCfgSetting(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the LBT configuration setting for the RFID module.
setLed(LEDIndicator) - Method in class com.unitech.lib.params.DeviceIndicator
setLedControl(boolean) - Method in class com.unitech.lib.reader.BaseReader
  Sets the LED control setting of the device.
setLength(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Length of the EPCMaskParam instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the pattern length of the Mask6cPattern instance.
setLength(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Length value of "Selection Mask".
setLinePosition(byte) - Method in class com.unitech.lib.reader.params.DisplayOutput
setMacAddress(String) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the MAC address of the device to which the BaseTransport instance is connected.
setMax(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the maximum Power Gian Level value for a PowerRange instance.
setMaxQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the maximum Q value.
setMaxQ(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the maximum Q value for the RFID module.
setMessage(String) - Method in class com.unitech.lib.reader.params.DisplayOutput
setMin(int) - Method in class com.unitech.lib.uhf.params.PowerRange
  Sets the Power Gian Level minimum value for a PowerRange instance.
setMinQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the minimum Q value.
setMinQ(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the minimum Q value for the RFID module.
setMinute(int) - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Set Minutes.
setMode(FindDeviceMode) - Method in class com.unitech.lib.reader.params.FindDevice
  Set FindDeviceMode.
setModuleProfile(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the module's profile that the RFID UHF module of the appliance uses to perform the inventory.
setModuleProfile(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the module profile for the RFID module.
setOffset(int) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the offset of the EPCMaskParam instance.
setOffset(int) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Offset value of "Selection Mask".
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the operating mode of the device.
setOperatingMode(OperatingMode) - Method in class com.unitech.lib.rpx.RP902Reader
setParameter(int, EngineParam, IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Set an engine parameter setting.
setParameter(EngineParam, IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Set an engine parameter setting.
setParameter(int, DeviceParam, IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Set a device parameter setting.
setParameter(DeviceParam, IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Set a device parameter setting.
setParameters(int, EngineParam[], IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Set multiple engine parameter settings.
setParameters(EngineParam[], IParameterEventListener) - Method in class com.unitech.lib.engine.BaseEngine
  Set multiple engine parameter settings.
setParameters(int, DeviceParam[], IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Set multiple device parameter settings.
setParameters(DeviceParam[], IParameterEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Set multiple device parameter settings.
setPATemperatureProtection(int) - Method in class com.unitech.lib.reader.BaseReader
  Sets the PA temperature protection setting of the equipment.
setPattern(String) - Method in class com.unitech.lib.uhf.params.EPCMaskParam
  Sets the Pattern for the EPCMaskParam instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.Mask6cPattern
  Sets the Mask pattern for the instance.
setPattern(String) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Pattern value of "Selection Mask".
setPc(byte[]) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the tag's PC value.
setPc(int) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the tag's PC value using an integer.
setPercentage(int) - Method in class com.unitech.lib.params.BatteryStatus
setPhaseBegin(float) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the phase begin value.
setPhaseEnd(float) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the phase end value.
setPhaseSetting(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the phase setting of the RFID UTE module of the Device.
setPower(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the antenna output of the RFID UHF module of the instrument.
setPower(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the power for the RFID module.
setPowerMode(PowerMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the power mode the RFID UHF module of the appliance uses to perform the inventory.
setPowerOff(PowerOffIndicator) - Method in class com.unitech.lib.engine.ScannerIndicator
setPowerOn(PowerOnIndicator) - Method in class com.unitech.lib.engine.ScannerIndicator
setPowerSaveTime(int) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Power Save Timeout of the RFID UTE module of the Device.
setPowerSavingMode(PowerSavingMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the power saving mode of the RFID UHF module of the device.
setPowerSavingMode(PowerSavingMode) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the power saving mode for the RFID module.
setQ(short) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the Q value.
setRawValue(String) - Method in class com.unitech.lib.params.DeviceParam
setReadMode(ReadMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the read mode status of the equipment.
setReplace(byte) - Method in class com.unitech.lib.params.FindReplace
  Sets the replace byte.
setRfidEventListener(IRfidEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Sets the RFID event listener for the BaseReader instance.
setRFMode(RFMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the RF Mode of the RFID UTE module of the Device.
setRfMode(RFMode) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the RF mode for the RFID module.
setRN16Data(byte[]) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the rn16 data value.
setRoundCnt(long) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the round count associated with the tag.
setRoundCount(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the round count for the RFID module.
setRssi(float) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the tag's RSSI value.
setScannerDataFormat(ScannerDataFormat[]) - Method in class com.unitech.lib.reader.BaseReader
  Sets the scanner data format of the device.
setScannerIndicator(ScannerIndicator) - Method in class com.unitech.lib.reader.BaseReader
  Sets the scanner indicator setting of the device.
setScreenOffTime(ScreenOffTime) - Method in class com.unitech.lib.reader.BaseReader
  Sets the time which the equipment automatically screen off.
setSecond(int) - Method in class com.unitech.lib.reader.params.ScreenOffTime
  Set Seconds.
setSelectMask6c(int, SelectMask6cParam) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cAction(int, Mask6cAction) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison behavior of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cBank(int, BankType) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the memory bank to be compared.
setSelectMask6cEnabled(int, boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set whether or not to use the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cOffset(int, int) - Method in class com.unitech.lib.uhf.BaseUHF
  The Selection Mask item of the RFID UHF module of the device sets the start address of the memory to start the comparison.
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the comparison value and length of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Flag of the tag to save the comparison result of Selection Mask item of the RFID UHF module of the device.
setSelectMask6cTruncate(int, Truncate) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the truncate of the Selection Mask item of the RFID UHF module of the device.
setSelectMode(SelectMode) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the Select Mode of the RFID UTE module of the Device.
setSelectMode(SelectMode) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the select mode for the RFID module.
setSession(Session) - Method in class com.unitech.lib.uhf.BaseUHF
  Device's RFID UHF module sets the Session to check the status of the Session of the tag to be read by Inventory operation.
setSession(Session) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the session for the RFID module.
setSetting(SettingIndicator) - Method in class com.unitech.lib.engine.ScannerIndicator
setSettingByLabel(boolean) - Method in class com.unitech.lib.reader.BaseReader
  Sets whether the device settings are applied by label.
setSkipInventoryActionStop(boolean) - Method in class com.unitech.lib.htx.HT730pReader
setSkipInventoryActionStop(boolean) - Method in class com.unitech.lib.rgx.RG768Reader
setSoftWareScan(boolean) - Method in class com.unitech.lib.rpx.RP902Reader
setStartQ(int) - Method in class com.unitech.lib.uhf.BaseUHF
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, set the starting Q value.
setStartQ(int) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the start Q value for the RFID module.
setState(BatteryState) - Method in class com.unitech.lib.params.BatteryStatus
setState(ConnectState, Object) - Method in class com.unitech.lib.transport.BaseTransport
setStateListener(IConnectStateEventListener) - Method in class com.unitech.lib.transport.BaseTransport
  Sets the listener to receive the connection status of an instance of the BaseTransport class.
setTagCount(long) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the number of tags detected.
setTagFocus(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Set the TagFocus Setting of the RFID UTE module of the Device.
setTagFocus(boolean) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the tag focus setting for the RFID module.
setTagUnique(TagUnique) - Method in class com.unitech.lib.reader.BaseReader
  Sets the Tag Unique setting of the device.
setTarget(Target) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the state of target of tag to read by Inventory operation.
setTarget(Target) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the target for the RFID module.
setTarget(Mask6cTarget) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Target Flag of "Selection Mask".
setTARI(TARIType) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the TARI that the RFID UHF module of the appliance uses to perform the inventory.
setTariType(TARIType) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the TARI type for the RFID module.
setTemperatureProtectionMode(TemperatureProtectionMode) - Method in class com.unitech.lib.reader.BaseReader
  Sets the temperature protection mode of the equipment.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access operation for 'TID memory'.
setTid(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'TID memory'.
setTid(byte[]) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the tag's TID value.
setTime(Date) - Method in class com.unitech.lib.reader.BaseReader
  Sets the system time of the instrument.
setTimeout(int) - Method in class com.unitech.lib.reader.params.FindDevice
  Set timeout.
setTimestamp(Date) - Method in class com.unitech.lib.event.params.BarcodeEventArgs
setTimestamp(Date) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the timestamp of the tag detection.
SettingIndicator - Enum in com.unitech.lib.engine.types
  The SettingIndicator enum represents different types of setting indicators.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.BaseUHF
  Sets the status of the toggle target that the RFID UHF module of the appliance uses to perform the inventory.
setToggleTarget(boolean) - Method in class com.unitech.lib.uhf.params.RFIDConfig
  Sets the toggle target for the RFID module.
setTruncate(Truncate) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set the Truncate value of "Selection Mask".
setUsed(boolean) - Method in class com.unitech.lib.uhf.params.SelectMask6cParam
  Set whether or not to use "Selection Mask".
setUser(LockState) - Method in class com.unitech.lib.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setUser(LockState) - Method in class com.unitech.lib.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setUserData(byte[]) - Method in class com.unitech.lib.reader.BaseReader
  Sets the user data on the device.
setUserData(byte[]) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the user data value.
setValue(Object) - Method in class com.unitech.lib.params.DeviceParam
  Set the value of the parameter
setValue(String) - Method in class com.unitech.lib.params.EngineParam
  Sets the value of the parameter.
setVibrator(boolean) - Method in class com.unitech.lib.params.DeviceIndicator
setVibrator(VibratorState) - Method in class com.unitech.lib.reader.BaseReader
  Sets the vibrator operation status of the equipment.
setXpc(byte[]) - Method in class com.unitech.lib.uhf.params.TagExtParam
  Sets the XPC value.
SGTIN - Class in com.unitech.lib.tagcoder
  The SGTIN class is a class that convert EPC to SGTIN format.
SGTIN(String) - Constructor for class com.unitech.lib.tagcoder.SGTIN
shutDown() - Method in class com.unitech.lib.reader.BaseReader
  Shuts down the device.
SKUType - Enum in com.unitech.lib.types
  The SKUType enumeration represents the type of device associated with the SDK.
stagingReset() - Method in class com.unitech.lib.reader.BaseReader
  Resets the staging area of the device.
start() - Method in class com.unitech.lib.reader.DetectReader
  Starts the USB detection process by registering the USB broadcast receiver.
startAddress - Variable in class com.unitech.lib.uhf.params.BlockPermaLockParam
startAddress - Variable in class com.unitech.lib.uhf.params.MarginReadParam
startDecode() - Method in class com.unitech.lib.reader.BaseReader
  Starts the decoding process on the device.
startFwFileTransfer(String, long) - Method in class com.unitech.lib.htx.HT730pReader
startFwFileTransfer(String, long) - Method in class com.unitech.lib.pax.PA768eReader
startFwUpdate(FirmwareUpdateMode) - Method in class com.unitech.lib.htx.HT730pReader
startFwUpdate(FirmwareUpdateMode) - Method in class com.unitech.lib.pax.PA768eReader
startQ - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The start Q value
status - Variable in class com.unitech.lib.params.AntennaStatusEventArgs
stop() - Method in class com.unitech.lib.reader.DetectReader
  Stops the USB detection process by unregistering the USB broadcast receiver.
stop() - Method in class com.unitech.lib.uhf.BaseUHF
  Instructs the Device to stop the operation being performed.
stopDecode() - Method in class com.unitech.lib.reader.BaseReader
  Stops the decoding process on the device.
stringToBytesASCII(String) - Static method in class com.unitech.lib.reader.params.DisplayOutput
  Returns the ASCII of String.
strVersion - Variable in class com.unitech.lib.engine.BaseEngine
strZero(String, int) - Static method in class com.unitech.lib.tagcoder.SGTIN
  Padding a string with zeroes
supportedGlobalBand() - Method in class com.unitech.lib.uhf.BaseUHF
  Returns the global band types that the RFID UHF module support.
supportedParams - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The list of supported parameters This is used to check which parameters are set in the config

A B C D E F G H I K L M N O P Q R S T U V W X _