# Package com.unitech.lib.uhf.types

- Enum Summary
  Enum | Description
  --- | ---
  AlgorithmType | The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
  AntennaBeginEnd | Enum representing the beginning and end of an antenna operation.
  AntennaSwitchingMode | Enum representing the antenna switching modes.
  AuthenticationResponse | Enum representing the authentication response types.
  BankType | The BankType enumeration specifies the memory bank of the RFID UHF tag.
  BLFType | The BLFType enumeration represents the BLF by which the RFID UHF module inventories the TAG.
  CfgStorageMode | Enum representing the configuration storage modes.
  Encoding | The Encoding enumeration represents the miller encoding by which the RFID UHF module inventories the TAG.
  ESMode | The Target enumeration type indicates the status of the Target of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  FreqSwitchingMode | Enum representing the frequency switching modes.
  Gen2xAppSize |
  Gen2xCode |
  Gen2xCr |
  Gen2xCrypto |
  Gen2xId |
  Gen2xProtection |
  GlobalBandType | The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.
  IncludeReplyLength | Enum representing the inclusion of reply length in a response.
  LockState | The LockState enumeration represents the lock state.
  Mask6cAction | The Mask6cAction enumeration type indicates the status of the Flag when the RFID UHF module performs the Inventory operation and the pattern of the given Selection Mask is set as the Target value of the Selection Mask according to the condition.
  Mask6cTarget | The Mask6cTarget enumeration represents the Flag where the result status of the Selection Mask will be saved when the RFID UHF module is inventoried.
  PowerMode | The PowerMode enumeration specifies the power mode while inventory.
  PowerSavingMode | Enum representing the power saving modes for the UHF device.
  ReadLock | Enum representing the read lock types for RFID tags.
  RFMode | Enum representing the RF modes for the UHF device.
  SelectMaskMode |
  SelectMode | The SelectMode enumeration represents the selection mode of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  Session | The Session enumeration represents the session of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  TagInfoId | Enumeration representing different tag information IDs.
  Target | The Target enumeration type indicates the status of the Target of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  TARIType | The TARIType enumeration represents the TARI by which the RFID UHF module inventories the TAG.
  TemperatureProtectionMode | Enum representing the temperature protection mode for a device.
  Truncate | Enum representing the truncate modes for EPC.