A B C D E F G H I K L M N O P Q R S T U V W X _

## R

read(byte[], int) - Method in class com.unitech.lib.rpx.RP902Reader
  Use only within the SDK.
read(byte[], int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[]) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int) - Method in class com.unitech.lib.transport.BaseTransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportBluetooth
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportUART
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportUART
read(byte[], int, int) - Method in class com.unitech.lib.transport.TransportUsb
read(byte[], int, int, int) - Method in class com.unitech.lib.transport.TransportUsb
reader - Variable in class com.unitech.lib.engine.BaseEngine
ReaderException - Exception in com.unitech.lib.diagnostics
  The exception class and contain result code
ReaderException(ResultCode) - Constructor for exception com.unitech.lib.diagnostics.ReaderException
ReaderException(ResultCode, String) - Constructor for exception com.unitech.lib.diagnostics.ReaderException
readLock - Variable in class com.unitech.lib.uhf.params.BlockPermaLockParam
ReadLock - Enum in com.unitech.lib.uhf.types
  Enum representing the read lock types for RFID tags.
readMemory6c(BankType, int, int, String) - Method in class com.unitech.lib.uhf.BaseUHF
  Device instructs to read specific memory of RFID UHF tag of ISO18000-6c Gen2 standard.
ReadMode - Enum in com.unitech.lib.types
  The ReadMode enumeration represents the type of device associated with the SDK.
ReadOnceState - Enum in com.unitech.lib.types
  The ReadOnceState enumeration represents the type of device associated with the SDK.
reboot() - Method in class com.unitech.lib.reader.BaseReader
  Reboots the device.
removeListener(IReaderEventListener) - Method in class com.unitech.lib.reader.BaseReader
  Removes the Listener that is listening for events on an instance of the BaseReader class.
removeListener(IRfidUhfEventListener) - Method in class com.unitech.lib.uhf.BaseUHF
  Removes an event handler when it no longer needs to receive events raised by the instance.
resetBuffer() - Method in class com.unitech.lib.transport.BaseTransport
  Resets the buffer by clearing the byte queue.
resetError() - Method in class com.unitech.lib.reader.BaseReader
  Use only within the SDK.
ResultCode - Enum in com.unitech.lib.types
  The ResultCode enumeration represents failure and behavior results.
resultCode() - Method in class com.unitech.lib.uhf.params.TagAccessResult
  The access result code.
retrieveBatchedData() - Method in class com.unitech.lib.reader.BaseReader
  Retrieves batched data from the device.
RETRY_COUNT - Static variable in class com.unitech.lib.reader.BaseReader
RFIDConfig - Class in com.unitech.lib.uhf.params
  The RFIDConfig class stores the config of the RFID module.
RFIDConfig() - Constructor for class com.unitech.lib.uhf.params.RFIDConfig
rfMode - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The rf mode setting
RFMode - Enum in com.unitech.lib.uhf.types
  Enum representing the RF modes for the UHF device.
RG768Reader - Class in com.unitech.lib.rgx
  The RG768Reader class is a class that controls RG768, receives data from RM100, and delivers it to the application program.
RG768Reader(Context) - Constructor for class com.unitech.lib.rgx.RG768Reader
rn16Data() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the rn16 data value.
roundCnt() - Method in class com.unitech.lib.uhf.params.TagExtParam
  Returns the round count associated with the tag.
roundCount - Variable in class com.unitech.lib.uhf.params.RFIDConfig
  The antenna roundCount value
RP300Reader - Class in com.unitech.lib.rpx
  RP300Reader is a class that represents a reader for the RP300 device.
RP300Reader(BaseTransport, Context) - Constructor for class com.unitech.lib.rpx.RP300Reader
RP902Reader - Class in com.unitech.lib.rpx
  The RP902Reader class is a class that controls RP902 in connection with unitech's equipment, receives data from RP902, and delivers it to the application program.
RP902Reader(BaseTransport) - Constructor for class com.unitech.lib.rpx.RP902Reader
rssi - Variable in class com.unitech.lib.params.LBTStatusEventArgs
Russia - Static variable in class com.unitech.lib.uhf.params.GlobalBandTable

A B C D E F G H I K L M N O P Q R S T U V W X _